### - a -

- adc_get_trim_func() : gr55xx_hal_adc.h
- ags_non_stream_send() : ags.h
- ags_service_init() : ags.h
- ags_stream_send() : ags.h
- ams_c_attr_display_set() : ams_c.h
- ams_c_attr_focus_set() : ams_c.h
- ams_c_attr_update_notify_set() : ams_c.h
- ams_c_client_init() : ams_c.h
- ams_c_cmd_enable_check() : ams_c.h
- ams_c_cmd_notify_set() : ams_c.h
- ams_c_cmd_send() : ams_c.h
- ams_c_cplt_attr_read() : ams_c.h
- ams_c_disc_srvc_start() : ams_c.h
- ancs_action_perform() : ancs_protocol.h
- ancs_c_client_init() : ancs_c.h
- ancs_c_data_source_notify_set() : ancs_c.h
- ancs_c_discovery_service() : ancs_c.h
- ancs_c_ntf_source_notify_set() : ancs_c.h
- ancs_c_write_control_point() : ancs_c.h
- ancs_decode_data_source() : ancs_protocol.h
- ancs_decode_notification_source() : ancs_protocol.h
- ancs_get_uid() : ancs_protocol.h
- ancs_notify_attr_get() : ancs_protocol.h
- ans_c_ctrl_point_set() : ans_c.h
- ans_c_disc_srvc_start() : ans_c.h
- ans_c_new_alert_notify_set() : ans_c.h
- ans_c_sup_new_alert_cat_read() : ans_c.h
- ans_c_sup_unread_alert_cat_read() : ans_c.h
- ans_c_unread_alert_notify_set() : ans_c.h
- ans_client_init() : ans_c.h
- ans_new_alert_send() : ans.h
- ans_service_init() : ans.h
- ans_unread_alert_send() : ans.h
- app_adc_conversion_async() : app_adc.h
- app_adc_conversion_sync() : app_adc.h
- app_adc_deinit() : app_adc.h
- app_adc_dma_deinit() : app_adc_dma.h
- app_adc_dma_init() : app_adc_dma.h
- app_adc_get_handle() : app_adc.h
- app_adc_init() : app_adc.h
- app_adc_multi_channel_conversion_async() : app_adc.h
- app_adc_voltage_extern() : app_adc.h
- app_adc_voltage_intern() : app_adc.h
- app_aes_decrypt_async() : app_aes.h
- app_aes_decrypt_sync() : app_aes.h
- app_aes_deinit() : app_aes.h
- app_aes_dma_decrypt_async() : app_aes_dma.h
- app_aes_dma_deinit() : app_aes_dma.h
- app_aes_dma_encrypt_async() : app_aes_dma.h
- app_aes_dma_init() : app_aes_dma.h
- app_aes_encrypt_async() : app_aes.h
- app_aes_encrypt_sync() : app_aes.h
- app_aes_get_handle() : app_aes.h
- app_aes_init() : app_aes.h
- app_aon_wdt_deinit() : app_aon_wdt.h
- app_aon_wdt_init() : app_aon_wdt.h
- app_aon_wdt_refresh() : app_aon_wdt.h
- app_bod_deinit() : app_bod.h
- app_bod_enable() : app_bod.h
- app_bod_event_enable() : app_bod.h
- app_bod_event_set_level() : app_bod.h
- app_bod_init() : app_bod.h
- app_bod_static_mode_enable() : app_bod.h
- app_boot_security_clock_set() : gr55xx_sys.h
- app_boot_turn_on_encrypt_clock() : gr55xx_sys.h
- app_comp_deinit() : app_comp.h
- app_comp_get_handle() : app_comp.h
- app_comp_init() : app_comp.h
- app_comp_start() : app_comp.h
- app_comp_stop() : app_comp.h
- app_dma_deinit() : app_dma.h
- app_dma_get_handle() : app_dma.h
- app_dma_init() : app_dma.h
- app_dma_start() : app_dma.h
- app_dspi_abort() : app_dspi.h
- app_dspi_abort_it() : app_dspi.h
- app_dspi_command_async() : app_dspi.h
- app_dspi_command_sync() : app_dspi.h
- app_dspi_command_transmit_async() : app_dspi.h
- app_dspi_command_transmit_sync() : app_dspi.h
- app_dspi_config_data_size() : app_dspi.h
- app_dspi_config_mode() : app_dspi.h
- app_dspi_deinit() : app_dspi.h
- app_dspi_dma_command_async() : app_dspi_dma.h
- app_dspi_dma_command_transmit_async() : app_dspi_dma.h
- app_dspi_dma_deinit() : app_dspi_dma.h
- app_dspi_dma_init() : app_dspi_dma.h
- app_dspi_dma_sg_llp_transmit_async() : app_dspi_dma.h
- app_dspi_dma_transmit_async() : app_dspi_dma.h
- app_dspi_get_handle() : app_dspi.h
- app_dspi_init() : app_dspi.h
- app_dspi_transmit_async() : app_dspi.h
- app_dspi_transmit_sync() : app_dspi.h
- app_dual_tim_deinit() : app_dual_tim.h
- app_dual_tim_get_counter_value() : app_dual_tim.h
- app_dual_tim_get_handle() : app_dual_tim.h
- app_dual_tim_init() : app_dual_tim.h
- app_dual_tim_set_background_reload() : app_dual_tim.h
- app_dual_tim_set_params() : app_dual_tim.h
- app_dual_tim_set_reload_value_bg_reload_value() : app_dual_tim.h
- app_dual_tim_start() : app_dual_tim.h
- app_dual_tim_stop() : app_dual_tim.h
- app_gpiote_config() : app_gpiote.h
- app_gpiote_deinit() : app_gpiote.h
- app_gpiote_init() : app_gpiote.h
- app_graphics_adjust_dcore_policy() : app_graphics_ospi.h
- app_graphics_dc_dspi_send_cmd_data_in_3wire_1lane() : app_graphics_dc.h
- app_graphics_dc_dspi_send_cmd_data_in_4wire_2lane() : app_graphics_dc.h
- app_graphics_dc_dspi_send_cmd_datas_in_4wire_2lane() : app_graphics_dc.h
- app_graphics_dc_dspi_send_cmd_in_3wire_1lane() : app_graphics_dc.h
- app_graphics_dc_freq_set() : app_graphics_dc.h
- app_graphics_dc_send_single_frame() : app_graphics_dc.h
- app_graphics_dc_set_power_state() : app_graphics_dc.h
- app_graphics_dc_spi_send() : app_graphics_dc.h
- app_graphics_gpu_set_power_state() : app_graphics_gpu.h
- app_graphics_is_ospi_address() : app_graphics_ospi.h
- app_graphics_ospi_deinit() : app_graphics_ospi.h
- app_graphics_ospi_get_base_address() : app_graphics_ospi.h
- app_graphics_ospi_get_byte_size() : app_graphics_ospi.h
- app_graphics_ospi_get_read_prefetch() : app_graphics_ospi.h
- app_graphics_ospi_get_sleep_state() : app_graphics_ospi.h
- app_graphics_ospi_init() : app_graphics_ospi.h
- app_graphics_ospi_pasr_update() : app_graphics_ospi.h
- app_graphics_ospi_register_psram_reload_func() : app_graphics_ospi.h
- app_graphics_ospi_reset() : app_graphics_ospi.h
- app_graphics_ospi_set_pasr() : app_graphics_ospi.h
- app_graphics_ospi_set_power_state() : app_graphics_ospi.h
- app_graphics_ospi_set_read_prefetch() : app_graphics_ospi.h
- app_graphics_ospi_set_sleep_state() : app_graphics_ospi.h
- app_hmac_deinit() : app_hmac.h
- app_hmac_get_handle() : app_hmac.h
- app_hmac_init() : app_hmac.h
- app_hmac_sha256_async() : app_hmac.h
- app_hmac_sha256_sync() : app_hmac.h
- app_hmac_user_hash() : app_hmac.h
- app_i2c_deinit() : app_i2c.h
- app_i2c_dma_deinit() : app_i2c_dma.h
- app_i2c_dma_init() : app_i2c_dma.h
- app_i2c_dma_mem_read_async() : app_i2c_dma.h
- app_i2c_dma_mem_write_async() : app_i2c_dma.h
- app_i2c_dma_receive_async() : app_i2c_dma.h
- app_i2c_dma_transmit_async() : app_i2c_dma.h
- app_i2c_get_handle() : app_i2c.h
- app_i2c_init() : app_i2c.h
- app_i2c_master_abort_it() : app_i2c.h
- app_i2c_mem_read_async() : app_i2c.h
- app_i2c_mem_read_sync() : app_i2c.h
- app_i2c_mem_write_async() : app_i2c.h
- app_i2c_mem_write_sync() : app_i2c.h
- app_i2c_receive_async() : app_i2c.h
- app_i2c_receive_sync() : app_i2c.h
- app_i2c_timing_adjust() : app_i2c.h
- app_i2c_timing_get() : app_i2c.h
- app_i2c_transmit_async() : app_i2c.h
- app_i2c_transmit_receive_sync() : app_i2c.h
- app_i2c_transmit_sync() : app_i2c.h
- app_i2s_abort() : app_i2s.h
- app_i2s_deinit() : app_i2s.h
- app_i2s_disable() : app_i2s.h
- app_i2s_disable_clock() : app_i2s.h
- app_i2s_dma_deinit() : app_i2s_dma.h
- app_i2s_dma_init() : app_i2s_dma.h
- app_i2s_dma_receive_async() : app_i2s_dma.h
- app_i2s_dma_transmit_async() : app_i2s_dma.h
- app_i2s_dma_transmit_receive_async() : app_i2s_dma.h
- app_i2s_enable() : app_i2s.h
- app_i2s_enable_clock() : app_i2s.h
- app_i2s_flush_rx_fifo() : app_i2s.h
- app_i2s_flush_tx_fifo() : app_i2s.h
- app_i2s_get_handle() : app_i2s.h
- app_i2s_init() : app_i2s.h
- app_i2s_receive_async() : app_i2s.h
- app_i2s_receive_sync() : app_i2s.h
- app_i2s_transmit_async() : app_i2s.h
- app_i2s_transmit_receive_async() : app_i2s.h
- app_i2s_transmit_receive_sync() : app_i2s.h
- app_i2s_transmit_sync() : app_i2s.h
- app_io_deinit() : app_io.h
- app_io_event_register_cb() : app_io.h
- app_io_event_unregister() : app_io.h
- app_io_init() : app_io.h
- app_io_read_pin() : app_io.h
- app_io_set_intput_type() : app_io.h
- app_io_set_speed() : app_io.h
- app_io_set_strength() : app_io.h
- app_io_toggle_pin() : app_io.h
- app_io_write_pin() : app_io.h
- app_pdm_abort() : app_pdm.h
- app_pdm_deinit() : app_pdm.h
- app_pdm_get_handle() : app_pdm.h
- app_pdm_init() : app_pdm.h
- app_pdm_left_start_dma() : app_pdm.h
- app_pdm_left_start_dma_sg_llp() : app_pdm.h
- app_pdm_right_start_dma() : app_pdm.h
- app_pdm_right_start_dma_sg_llp() : app_pdm.h
- app_pdm_stereo_start_dma() : app_pdm.h
- app_pdm_stereo_start_dma_sg_llp() : app_pdm.h
- app_pkc_big_number_add_async() : app_pkc.h
- app_pkc_big_number_add_sync() : app_pkc.h
- app_pkc_big_number_multi_async() : app_pkc.h
- app_pkc_big_number_multi_sync() : app_pkc.h
- app_pkc_deinit() : app_pkc.h
- app_pkc_ecc_point_multi_async() : app_pkc.h
- app_pkc_ecc_point_multi_sync() : app_pkc.h
- app_pkc_get_handle() : app_pkc.h
- app_pkc_init() : app_pkc.h
- app_pkc_modular_add_async() : app_pkc.h
- app_pkc_modular_add_sync() : app_pkc.h
- app_pkc_modular_compare_async() : app_pkc.h
- app_pkc_modular_compare_sync() : app_pkc.h
- app_pkc_modular_left_shift_async() : app_pkc.h
- app_pkc_modular_left_shift_sync() : app_pkc.h
- app_pkc_modular_sub_async() : app_pkc.h
- app_pkc_modular_sub_sync() : app_pkc.h
- app_pkc_montgomery_inversion_async() : app_pkc.h
- app_pkc_montgomery_inversion_sync() : app_pkc.h
- app_pkc_montgomery_multi_async() : app_pkc.h
- app_pkc_montgomery_multi_sync() : app_pkc.h
- app_pwm_config_channel() : app_pwm.h
- app_pwm_deinit() : app_pwm.h
- app_pwm_get_handle() : app_pwm.h
- app_pwm_init() : app_pwm.h
- app_pwm_start() : app_pwm.h
- app_pwm_stop() : app_pwm.h
- app_pwm_update_freq() : app_pwm.h
- app_pwr_mgmt_init() : app_pwr_mgmt.h
- app_qspi_abort() : app_qspi.h
- app_qspi_command_async() : app_qspi.h
- app_qspi_command_receive_async() : app_qspi.h
- app_qspi_command_receive_sync() : app_qspi.h
- app_qspi_command_sync() : app_qspi.h
- app_qspi_command_transmit_async() : app_qspi.h
- app_qspi_command_transmit_sync() : app_qspi.h
- app_qspi_deinit() : app_qspi.h
- app_qspi_dma_command_async() : app_qspi_dma.h
- app_qspi_dma_command_receive_async() : app_qspi_dma.h
- app_qspi_dma_command_transmit_async() : app_qspi_dma.h
- app_qspi_dma_deinit() : app_qspi_dma.h
- app_qspi_dma_init() : app_qspi_dma.h
- app_qspi_dma_receive_async() : app_qspi_dma.h
- app_qspi_dma_receive_async_ex() : app_qspi_dma.h
- app_qspi_dma_transmit_async() : app_qspi_dma.h
- app_qspi_dma_transmit_async_ex() : app_qspi_dma.h
- app_qspi_dma_transmit_in_qpi_async() : app_qspi_dma.h
- app_qspi_get_handle() : app_qspi.h
- app_qspi_init() : app_qspi.h
- app_qspi_receive_async() : app_qspi.h
- app_qspi_receive_async_ex() : app_qspi.h
- app_qspi_receive_sync() : app_qspi.h
- app_qspi_receive_sync_ex() : app_qspi.h
- app_qspi_transmit_async() : app_qspi.h
- app_qspi_transmit_async_ex() : app_qspi.h
- app_qspi_transmit_in_qpi_async() : app_qspi.h
- app_qspi_transmit_sync() : app_qspi.h
- app_qspi_transmit_sync_ex() : app_qspi.h
- app_rng_deinit() : app_rng.h
- app_rng_gen_async() : app_rng.h
- app_rng_gen_sync() : app_rng.h
- app_rng_get_handle() : app_rng.h
- app_rng_init() : app_rng.h
- app_rtc_deinit() : app_rtc.h
- app_rtc_disable_event() : app_rtc.h
- app_rtc_get_time() : app_rtc.h
- app_rtc_init() : app_rtc.h
- app_rtc_init_time() : app_rtc.h
- app_rtc_setup_alarm() : app_rtc.h
- app_rtc_setup_tick() : app_rtc.h
- app_spi_abort() : app_spi.h
- app_spi_deinit() : app_spi.h
- app_spi_dma_deinit() : app_spi_dma.h
- app_spi_dma_init() : app_spi_dma.h
- app_spi_dma_read_eeprom_async() : app_spi_dma.h
- app_spi_dma_read_memory_async() : app_spi_dma.h
- app_spi_dma_receive_async() : app_spi_dma.h
- app_spi_dma_receive_high_speed_sync() : app_spi_dma.h
- app_spi_dma_transmit_async() : app_spi_dma.h
- app_spi_dma_transmit_high_speed_sync() : app_spi_dma.h
- app_spi_dma_transmit_receive_async() : app_spi_dma.h
- app_spi_dma_write_memory_async() : app_spi_dma.h
- app_spi_get_handle() : app_spi.h
- app_spi_init() : app_spi.h
- app_spi_read_eeprom_async() : app_spi.h
- app_spi_read_eeprom_sync() : app_spi.h
- app_spi_read_memory_async() : app_spi.h
- app_spi_receive_async() : app_spi.h
- app_spi_receive_high_speed_sync() : app_spi.h
- app_spi_receive_sync() : app_spi.h
- app_spi_transmit_async() : app_spi.h
- app_spi_transmit_high_speed_sync() : app_spi.h
- app_spi_transmit_receive_async() : app_spi.h
- app_spi_transmit_receive_sync() : app_spi.h
- app_spi_transmit_sync() : app_spi.h
- app_spi_write_memory_async() : app_spi.h
- app_spim_dma_receive_with_ia() : app_spi_dma.h
- app_spim_dma_transmit_with_ia() : app_spi_dma.h
- app_spim_receive_with_ia() : app_spi.h
- app_spim_transmit_with_ia() : app_spi.h
- app_tim_deinit() : app_tim.h
- app_tim_get_handle() : app_tim.h
- app_tim_init() : app_tim.h
- app_tim_start() : app_tim.h
- app_tim_stop() : app_tim.h
- app_uart_abort() : app_uart.h
- app_uart_abort_receive() : app_uart.h
- app_uart_abort_transmit() : app_uart.h
- app_uart_deinit() : app_uart.h
- app_uart_dma_deinit() : app_uart_dma.h
- app_uart_dma_init() : app_uart_dma.h
- app_uart_dma_receive_async() : app_uart_dma.h
- app_uart_dma_transmit_async() : app_uart_dma.h
- app_uart_flush() : app_uart.h
- app_uart_get_handle() : app_uart.h
- app_uart_init() : app_uart.h
- app_uart_receive_async() : app_uart.h
- app_uart_receive_sync() : app_uart.h
- app_uart_transmit_async() : app_uart.h
- app_uart_transmit_sync() : app_uart.h