Macros
QSPI Concurrent Xip Inst Sent Mode
Peripheral Driver » LL Driver » QSPI | Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS 0u
#define | LL_QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS 1u

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS

#define LL_QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS 0u

Send instruction for every transaction

Definition at line 684 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS

#define LL_QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS 1u

Send instruction only for first transaction

Definition at line 685 of file gr55xx_ll_qspi.h.