Here is a list of all file members with links to the files they belong to:

### - a -

- AANS_C_CAT_ID_NB : ans_c.h
- ACTION_ID_NEGATIVE : ancs_protocol.h
- ACTION_ID_POSITIVE : ancs_protocol.h
- ACTIVE : gr55xx_hal_pwr_mgmt.h
- ADC_CFG_REG_DEFAULT : gr55xx_hal_adc.h
- ADC_DEFAULT_CONFIG : gr55xx_hal_adc.h
- adc_get_trim_func() : gr55xx_hal_adc.h
- adc_handle_t : gr55xx_hal_adc.h
- adc_init_t : gr55xx_hal_adc.h
- ADC_INPUT_DIFFERENTIAL : gr55xx_hal_adc.h
- ADC_INPUT_SINGLE : gr55xx_hal_adc.h
- ADC_INPUT_SRC_BAT : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO0 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO1 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO2 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO3 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO4 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO5 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO6 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_IO7 : gr55xx_hal_adc.h
- ADC_INPUT_SRC_REF : gr55xx_hal_adc.h
- ADC_INPUT_SRC_TMP : gr55xx_hal_adc.h
- ADC_PWR_ID : app_pwr_mgmt.h
- ADC_REF_SRC_BUF_INT : gr55xx_hal_adc.h
- ADC_REF_SRC_IO0 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO1 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO2 : gr55xx_hal_adc.h
- ADC_REF_SRC_IO3 : gr55xx_hal_adc.h
- ADC_REF_VALUE_0P8 : gr55xx_hal_adc.h
- ADC_REF_VALUE_1P2 : gr55xx_hal_adc.h
- ADC_REF_VALUE_1P6 : gr55xx_hal_adc.h
- ADC_REF_VALUE_2P0 : gr55xx_hal_adc.h
- AES_BLOCK_MAX : gr55xx_hal_aes.h
- AES_BLOCKSIZE_BITS : gr55xx_hal_aes.h
- AES_BLOCKSIZE_BYTES : gr55xx_hal_aes.h
- AES_BLOCKSIZE_WORDS : gr55xx_hal_aes.h
- AES_CHAININGMODE_CBC : gr55xx_hal_aes.h
- AES_CHAININGMODE_ECB : gr55xx_hal_aes.h
- AES_FLAG_DATAREADY : gr55xx_hal_aes.h
- AES_FLAG_DMA_DONE : gr55xx_hal_aes.h
- AES_FLAG_DMA_ERR : gr55xx_hal_aes.h
- AES_FLAG_KEY_VALID : gr55xx_hal_aes.h
- aes_handle_t : gr55xx_hal_aes.h
- aes_init_t : gr55xx_hal_aes.h
- AES_IT_DONE : gr55xx_hal_aes.h
- AES_KEYSIZE_128BITS : gr55xx_hal_aes.h
- AES_KEYSIZE_192BITS : gr55xx_hal_aes.h
- AES_KEYSIZE_256BITS : gr55xx_hal_aes.h
- AES_OPERATION_MODE_DECRYPT : gr55xx_hal_aes.h
- AES_OPERATION_MODE_ENCRYPT : gr55xx_hal_aes.h
- aes_result_cb : ble.h
- AGS_ACK_ACK : ags.h
- AGS_ACK_NACK : ags.h
- AGS_ALEXA_STREAM_ID : ags.h
- AGS_CHAR_FULL : ags.h
- AGS_CHAR_MANDATORY : ags.h
- AGS_CONNECTION_MAX : ags.h
- AGS_CONTROL_STREAM_ID : ags.h
- AGS_EVT_ECHO_RX_DATA_SENT : ags.h
- AGS_EVT_ECHO_RX_NOTI_DISABLE : ags.h
- AGS_EVT_ECHO_RX_NOTI_ENABLE : ags.h
- AGS_EVT_ECHO_TX_DATA_RECEIVED : ags.h
- ags_evt_handler_t : ags.h
- AGS_EVT_INVALID : ags.h
- ags_evt_type_t : ags.h
- ags_header_ack_flag_t : ags.h
- AGS_HEADER_ACK_PAYLOAD_LEN : ags.h
- AGS_HEADER_ACK_RES_1 : ags.h
- AGS_HEADER_ACK_RES_2 : ags.h
- AGS_HEADER_FIRST_RES : ags.h
- ags_header_length_ext_t : ags.h
- ags_header_result_code_t : ags.h
- ags_header_stream_id_t : ags.h
- ags_header_trxn_type_t : ags.h
- AGS_LEN_EXT_EXT : ags.h
- AGS_LEN_EXT_NO_EXT : ags.h
- ags_non_stream_send() : ags.h
- AGS_OTA_STREAM_ID : ags.h
- AGS_PAIR_ADV_FLAG : ags.h
- AGS_RECONNECT_ADV_FLAG : ags.h
- AGS_RES_CODE_SUCCESS : ags.h
- AGS_RES_CODE_UNKNOWN : ags.h
- AGS_RES_CODE_UNSUPPORTED : ags.h
- AGS_RX_VAL_LEN_MAX : ags.h
- ags_service_init() : ags.h
- AGS_SERVICE_UUID : ags.h
- ags_stream_cb_t : ags.h
- ags_stream_send() : ags.h
- AGS_TRANSACTION_TYPE_CONT : ags.h
- AGS_TRANSACTION_TYPE_CTRL : ags.h
- AGS_TRANSACTION_TYPE_FIRST : ags.h
- AGS_TRANSACTION_TYPE_LAST : ags.h
- AGS_TX_VAL_LEN_MAX : ags.h
- ALARM_ERROR : gr55xx_hal_rtc.h
- alarm_handle_t : gr55xx_hal_rtc.h
- ALARM_READY : gr55xx_hal_rtc.h
- ALARM_RUNNING : gr55xx_hal_rtc.h
- ALL_DEVICES_BACKUP : gr55xx_hal_pwr_mgmt.h
- ALL_DEVICES_SLEEP : gr55xx_hal_pwr_mgmt.h
- AMS_ATTR_DISPLAY_UUID : ams_c.h
- AMS_ATTR_UPDATE_UUID : ams_c.h
- AMS_C_ATTR_COUNT_MAX : ams_c.h
- ams_c_attr_display_set() : ams_c.h
- ams_c_attr_focus_set() : ams_c.h
- ams_c_attr_update_notify_set() : ams_c.h
- ams_c_client_init() : ams_c.h
- ams_c_cmd_enable_check() : ams_c.h
- ams_c_cmd_id_t : ams_c.h
- ams_c_cmd_notify_set() : ams_c.h
- ams_c_cmd_send() : ams_c.h
- AMS_C_CONNECTION_MAX : ams_c.h
- ams_c_cplt_attr_read() : ams_c.h
- ams_c_disc_srvc_start() : ams_c.h
- ams_c_ett_id_t : ams_c.h
- AMS_C_EVT_ATTR_FOCUS_SET_SUCCESS : ams_c.h
- AMS_C_EVT_ATTR_UPDATE_NTF_SET_SUCCESS : ams_c.h
- AMS_C_EVT_ATTR_UPDATE_RECEIVE : ams_c.h
- AMS_C_EVT_CMD_SEND_SUCCESS : ams_c.h
- AMS_C_EVT_CMD_UPDATE_NTF_SET_SUCCESS : ams_c.h
- AMS_C_EVT_CMD_UPDATE_RECEIVE : ams_c.h
- AMS_C_EVT_CPLT_ATTR_DISPLAY_SET_SUCCESS : ams_c.h
- AMS_C_EVT_CPLT_ATTR_READ_RSP : ams_c.h
- AMS_C_EVT_DISCOVERY_CPLT : ams_c.h
- AMS_C_EVT_DISCOVERY_FAIL : ams_c.h
- ams_c_evt_handler_t : ams_c.h
- AMS_C_EVT_INVALID : ams_c.h
- ams_c_evt_type_t : ams_c.h
- AMS_C_EVT_WRITE_OP_ERR : ams_c.h
- AMS_C_TRUNCATED_FLAG : ams_c.h
- AMS_CMD_ID_ADVANCE_REPEAT_MODE : ams_c.h
- AMS_CMD_ID_ADVANCE_SHUFFLE_MODE : ams_c.h
- AMS_CMD_ID_BOOK_MARK_TRACK : ams_c.h
- AMS_CMD_ID_DISLIKE_TRACK : ams_c.h
- AMS_CMD_ID_LIKE_TRACK : ams_c.h
- AMS_CMD_ID_NEXT_TRACK : ams_c.h
- AMS_CMD_ID_PAUSE : ams_c.h
- AMS_CMD_ID_PLAY : ams_c.h
- AMS_CMD_ID_PREVIOUS_TRACK : ams_c.h
- AMS_CMD_ID_SKIP_BACKWARD : ams_c.h
- AMS_CMD_ID_SKIP_FORWARD : ams_c.h
- AMS_CMD_ID_TOGGLE_PLAY_PAUSE : ams_c.h
- AMS_CMD_ID_VOLUME_DOWN : ams_c.h
- AMS_CMD_ID_VOLUME_UP : ams_c.h
- AMS_CMD_UUID : ams_c.h
- AMS_ETT_ID_PLAYER : ams_c.h
- AMS_ETT_ID_QUEUE : ams_c.h
- AMS_ETT_ID_TRACK : ams_c.h
- AMS_PLAYER_ATTR_ID_NAME : ams_c.h
- AMS_PLAYER_ATTR_ID_PLAYBACK_INFO : ams_c.h
- AMS_PLAYER_ATTR_ID_VOLUME : ams_c.h
- AMS_QUEUE_ATTR_ID_COUNT : ams_c.h
- AMS_QUEUE_ATTR_ID_INDEX : ams_c.h
- AMS_QUEUE_ATTR_ID_REPEAT_MODE : ams_c.h
- AMS_QUEUE_ATTR_ID_SHUFFLE_MODE : ams_c.h
- AMS_SRVC_UUID : ams_c.h
- AMS_TRACK_ATTR_ID_ALBUM : ams_c.h
- AMS_TRACK_ATTR_ID_ARTIST : ams_c.h
- AMS_TRACK_ATTR_ID_DURATION : ams_c.h
- AMS_TRACK_ATTR_ID_TITTLE : ams_c.h
- ancs_action_perform() : ancs_protocol.h
- ANCS_ATTR : ancs_protocol.h
- ANCS_ATTR_MAXLEN : ancs_protocol.h
- ancs_c_action_id_t : ancs_protocol.h
- ancs_c_client_init() : ancs_c.h
- ANCS_C_CONNECTION_MAX : ancs_c.h
- ancs_c_ctrl_point_t : ancs_protocol.h
- ancs_c_data_source_notify_set() : ancs_c.h
- ancs_c_discovery_service() : ancs_c.h
- ancs_c_evt_handler_t : ancs_c.h
- ancs_c_ntf_source_notify_set() : ancs_c.h
- ancs_c_write_control_point() : ancs_c.h
- ANCS_CATEGORY_ID_BUSINESS_AND_FINANCE : ancs_protocol.h
- ANCS_CATEGORY_ID_EMAIL : ancs_protocol.h
- ANCS_CATEGORY_ID_ENTERTAINMENT : ancs_protocol.h
- ANCS_CATEGORY_ID_HEALTH_AND_FITNESS : ancs_protocol.h
- ANCS_CATEGORY_ID_INCOMING_CALL : ancs_protocol.h
- ANCS_CATEGORY_ID_LOCATION : ancs_protocol.h
- ANCS_CATEGORY_ID_MISSED_CALL : ancs_protocol.h
- ANCS_CATEGORY_ID_NEWS : ancs_protocol.h
- ANCS_CATEGORY_ID_OTHER : ancs_protocol.h
- ANCS_CATEGORY_ID_SCHEDULE : ancs_protocol.h
- ANCS_CATEGORY_ID_SOCIAL : ancs_protocol.h
- ancs_category_id_t : ancs_protocol.h
- ANCS_CATEGORY_ID_VOICE_MAIL : ancs_protocol.h
- ANCS_CONTROL_POINT_UUID : ancs_c.h
- ANCS_DATA_SOURCE_UUID : ancs_c.h
- ancs_decode_data_source() : ancs_protocol.h
- ancs_decode_notification_source() : ancs_protocol.h
- ANCS_EVENT_ID_NOTIFICATION_ADDED : ancs_protocol.h
- ANCS_EVENT_ID_NOTIFICATION_MODIFIED : ancs_protocol.h
- ANCS_EVENT_ID_NOTIFICATION_REMOVED : ancs_protocol.h
- ancs_evt_id_t : ancs_protocol.h
- ancs_get_uid() : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_APP_IDENTIFIER : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_DATE : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_MESSAGE : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_MESSAGE_SIZE : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_NEGATIVE_ACTION_LABEL : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_POSITIVE_ACTION_LABEL : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_SUBTITLE : ancs_protocol.h
- ANCS_NOTIF_ATTR_ID_TITLE : ancs_protocol.h
- ancs_notification_attr_t : ancs_protocol.h
- ancs_notify_attr_get() : ancs_protocol.h
- ANCS_NTF_SOURCE_UUID : ancs_c.h
- ANCS_SRVC_UUID : ancs_c.h
- ans_alert_cat_id_t : ans.h
- ANS_ALERT_NTF_CTRL_PT_VAL_LEN : ans.h
- ANS_ALL_CAT_SUP : ans.h
- ans_c_alert_cat_id_t : ans_c.h
- ANS_C_ALERT_NTF_CTRL_PT_VAL_LEN : ans_c.h
- ANS_C_ALL_CAT_SUP : ans_c.h
- ANS_C_CALL_SUP : ans_c.h
- ANS_C_CAT_ID_ALL : ans_c.h
- ANS_C_CAT_ID_CALL : ans_c.h
- ANS_C_CAT_ID_EMAIL : ans_c.h
- ANS_C_CAT_ID_HG_PRIO_ALERT : ans_c.h
- ANS_C_CAT_ID_INSTANT_MES : ans_c.h
- ANS_C_CAT_ID_MISSED_CALL : ans_c.h
- ANS_C_CAT_ID_NEWS : ans_c.h
- ANS_C_CAT_ID_SCHEDULE : ans_c.h
- ANS_C_CAT_ID_SMPL_ALERT : ans_c.h
- ANS_C_CAT_ID_SMS_MMS : ans_c.h
- ANS_C_CAT_ID_VOICE_MAIL : ans_c.h
- ANS_C_CONNECTION_MAX : ans_c.h
- ans_c_ctrl_point_set() : ans_c.h
- ANS_C_CTRL_PT_DIS_NEW_INC_ALERT_NTF : ans_c.h
- ANS_C_CTRL_PT_DIS_UNREAD_CAT_STA_NTF : ans_c.h
- ANS_C_CTRL_PT_EN_NEW_INC_ALERT_NTF : ans_c.h
- ANS_C_CTRL_PT_EN_UNREAD_CAT_STA_NTF : ans_c.h
- ans_c_ctrl_pt_id_t : ans_c.h
- ANS_C_CTRL_PT_NTF_NEW_INC_ALERT_IMME : ans_c.h
- ANS_C_CTRL_PT_NTF_UNREAD_CAT_STA_IMME : ans_c.h
- ans_c_disc_srvc_start() : ans_c.h
- ANS_C_EMAIL_SUP : ans_c.h
- ANS_C_ERROR_CMD_NOT_SUP : ans_c.h
- ANS_C_EVT_CTRL_POINT_SET_SUCCESS : ans_c.h
- ANS_C_EVT_DISCOVERY_COMPLETE : ans_c.h
- ANS_C_EVT_DISCOVERY_FAIL : ans_c.h
- ans_c_evt_handler_t : ans_c.h
- ANS_C_EVT_INVALID : ans_c.h
- ANS_C_EVT_NEW_ALERT_NTF_SET_SUCCESS : ans_c.h
- ANS_C_EVT_NEW_ALERT_RECEIVE : ans_c.h
- ANS_C_EVT_SUP_NEW_ALERT_CAT_RECEIV : ans_c.h
- ANS_C_EVT_SUP_UNREAD_ALERT_CAT_REC : ans_c.h
- ans_c_evt_type_t : ans_c.h
- ANS_C_EVT_UNREAD_ALERT_RECEIVE : ans_c.h
- ANS_C_EVT_UNREAD_ALERT_STA_NTF_SET_SUCCESS : ans_c.h
- ANS_C_EVT_WRITE_OP_ERR : ans_c.h
- ANS_C_HG_PRIO_ALERT_SUP : ans_c.h
- ANS_C_INSTANT_MES : ans_c.h
- ANS_C_MISSED_CALL_SUP : ans_c.h
- ans_c_new_alert_notify_set() : ans_c.h
- ANS_C_NEWS_SUP : ans_c.h
- ANS_C_SCHEDULE_SUP : ans_c.h
- ANS_C_SMPL_ALERT_SUP : ans_c.h
- ANS_C_SMS_MMS_SUP : ans_c.h
- ans_c_sup_new_alert_cat_read() : ans_c.h
- ans_c_sup_unread_alert_cat_read() : ans_c.h
- ans_c_unread_alert_notify_set() : ans_c.h
- ANS_C_UTF_8_STR_LEN_MAX : ans_c.h
- ANS_C_VOICE_MAIL_SUP : ans_c.h
- ANS_CALL_SUP : ans.h
- ANS_CAT_ID_ALL : ans.h
- ANS_CAT_ID_CALL : ans.h
- ANS_CAT_ID_EMAIL : ans.h
- ANS_CAT_ID_HG_PRIO_ALERT : ans.h
- ANS_CAT_ID_INSTANT_MES : ans.h
- ANS_CAT_ID_MISSED_CALL : ans.h
- ANS_CAT_ID_NB : ans.h
- ANS_CAT_ID_NEWS : ans.h
- ANS_CAT_ID_SCHEDULE : ans.h
- ANS_CAT_ID_SMPL_ALERT : ans.h
- ANS_CAT_ID_SMS_MMS : ans.h
- ANS_CAT_ID_VOICE_MAIL : ans.h
- ans_client_init() : ans_c.h
- ANS_CONNECTION_MAX : ans.h
- ANS_CTRL_PT_DIS_NEW_INC_ALERT_NTF : ans.h
- ANS_CTRL_PT_DIS_UNREAD_CAT_STA_NTF : ans.h
- ANS_CTRL_PT_EN_NEW_INC_ALERT_NTF : ans.h
- ANS_CTRL_PT_EN_UNREAD_CAT_STA_NTF : ans.h
- ans_ctrl_pt_id_t : ans.h
- ANS_CTRL_PT_NTF_NEW_INC_ALERT_IMME : ans.h
- ANS_CTRL_PT_NTF_UNREAD_CAT_STA_IMME : ans.h
- ANS_EMAIL_SUP : ans.h
- ANS_ERROR_CMD_NOT_SUP : ans.h
- ans_evt_handler_t : ans.h
- ANS_EVT_INVALID : ans.h
- ANS_EVT_NEW_ALERT_IMME_NTF_REQ : ans.h
- ANS_EVT_NEW_ALERT_NTF_DISABLE : ans.h
- ANS_EVT_NEW_ALERT_NTF_ENABLE : ans.h
- ans_evt_type_t : ans.h
- ANS_EVT_Unread_ALERT_IMME_NTF_REQ : ans.h
- ANS_EVT_UNREAD_ALERT_STA_NTF_DISABLE : ans.h
- ANS_EVT_UNREAD_ALERT_STA_NTF_ENABLE : ans.h
- ANS_HG_PRIO_ALERT_SUP : ans.h
- ANS_INSTANT_MES : ans.h
- ANS_MISSED_CALL_SUP : ans.h
- ans_new_alert_send() : ans.h
- ANS_NEWS_ALERT_VAL_LEN : ans.h
- ANS_NEWS_SUP : ans.h
- ANS_SCHEDULE_SUP : ans.h
- ans_service_init() : ans.h
- ANS_SMPL_ALERT_SUP : ans.h
- ANS_SMS_MMS_SUP : ans.h
- ANS_SUP_NEW_ALERT_CAT_VAL_LEN : ans.h
- ANS_SUP_UNREAD_ALERT_CAT_VAL_LEN : ans.h
- ans_unread_alert_send() : ans.h
- ANS_UNREAD_ALERT_STA_VAL_LEN : ans.h
- ANS_UTF_8_STR_LEN_MAX : ans.h
- ANS_VOICE_MAIL_SUP : ans.h
- AON_GPIO_DEFAULT_CONFIG : gr55xx_hal_aon_gpio.h
- aon_gpio_init_t : gr55xx_hal_aon_gpio.h
- AON_GPIO_INPUT_TYPE_CMOS : gr55xx_hal_aon_gpio.h
- AON_GPIO_INPUT_TYPE_SCHMITT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_INOUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_INPUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_BOTH_EDGE : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_FALLING : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_HIGH : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_LOW : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_IT_RISING : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_MUX : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_NONE : gr55xx_hal_aon_gpio.h
- AON_GPIO_MODE_OUTPUT : gr55xx_hal_aon_gpio.h
- AON_GPIO_MUX_0 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_1 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_2 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_3 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_4 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_5 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_6 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_7 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_MUX_8 : gr55xx_hal_aon_gpio_ex.h
- AON_GPIO_NOPULL : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_0 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_1 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_2 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_3 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_4 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_5 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_6 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_7 : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_ALL : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_MASK : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_RESET : gr55xx_hal_aon_gpio.h
- AON_GPIO_PIN_SET : gr55xx_hal_aon_gpio.h
- aon_gpio_pin_state_t : gr55xx_hal_aon_gpio.h
- AON_GPIO_PULLDOWN : gr55xx_hal_aon_gpio.h
- AON_GPIO_PULLUP : gr55xx_hal_aon_gpio.h
- AON_GPIO_SPEED_HIGH : gr55xx_hal_aon_gpio.h
- AON_GPIO_SPEED_MEDIUM : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_HIGH : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_LOW : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_MEDIUM : gr55xx_hal_aon_gpio.h
- AON_GPIO_STRENGTH_ULTRA : gr55xx_hal_aon_gpio.h
- aon_wdt_handle_t : gr55xx_hal_aon_wdt.h
- aon_wdt_init_t : gr55xx_hal_aon_wdt.h
- AON_WDT_REG_READ : gr55xx_ll_aon_wdt.h
- AP_SYNC_KEY_MATERIAL_LEN : esls.h
- APP_ADC_ACTIVITY : app_adc.h
- app_adc_conversion_async() : app_adc.h
- app_adc_conversion_sync() : app_adc.h
- app_adc_deinit() : app_adc.h
- APP_ADC_DMA_ACTIVITY : app_adc.h
- app_adc_dma_conversion_async : app_adc_dma.h
- app_adc_dma_deinit() : app_adc_dma.h
- app_adc_dma_init() : app_adc_dma.h
- APP_ADC_DMA_INVALID : app_adc.h
- app_adc_dma_multi_channel_conversion_async : app_adc_dma.h
- app_adc_dma_state_t : app_adc.h
- APP_ADC_EVT_CONV_CPLT : app_adc.h
- app_adc_evt_handler_t : app_adc.h
- app_adc_evt_type_t : app_adc.h
- app_adc_get_handle() : app_adc.h
- app_adc_init() : app_adc.h
- APP_ADC_INVALID : app_adc.h
- app_adc_multi_channel_conversion_async() : app_adc.h
- app_adc_sample_node_t : app_adc.h
- app_adc_state_t : app_adc.h
- app_adc_voltage_extern() : app_adc.h
- app_adc_voltage_intern() : app_adc.h
- APP_AES_ACTIVITY : app_aes.h
- app_aes_decrypt_async() : app_aes.h
- app_aes_decrypt_sync() : app_aes.h
- app_aes_deinit() : app_aes.h
- app_aes_dma_decrypt_async() : app_aes_dma.h
- app_aes_dma_deinit() : app_aes_dma.h
- app_aes_dma_encrypt_async() : app_aes_dma.h
- app_aes_dma_init() : app_aes_dma.h
- app_aes_encrypt_async() : app_aes.h
- app_aes_encrypt_sync() : app_aes.h
- APP_AES_EVT_DONE : app_aes.h
- APP_AES_EVT_ERROR : app_aes.h
- app_aes_evt_handler_t : app_aes.h
- app_aes_evt_type_t : app_aes.h
- app_aes_get_handle() : app_aes.h
- app_aes_init() : app_aes.h
- APP_AES_INVALID : app_aes.h
- APP_AES_MODE_CBC : app_aes.h
- APP_AES_MODE_ECB : app_aes.h
- APP_AES_MODE_MAX : app_aes.h
- app_aes_mode_t : app_aes.h
- app_aes_state_t : app_aes.h
- APP_AON_IO_PIN_ALL : app_io.h
- APP_AON_WDT_ACTIVITY : app_aon_wdt.h
- app_aon_wdt_deinit() : app_aon_wdt.h
- app_aon_wdt_evt_handler_t : app_aon_wdt.h
- app_aon_wdt_init() : app_aon_wdt.h
- APP_AON_WDT_INVALID : app_aon_wdt.h
- app_aon_wdt_refresh() : app_aon_wdt.h
- app_aon_wdt_state_t : app_aon_wdt.h
- APP_BOD_ACTIVITY : app_bod.h
- app_bod_deinit() : app_bod.h
- APP_BOD_DISABLE : app_bod.h
- app_bod_enable() : app_bod.h
- APP_BOD_ENABLE : app_bod.h
- APP_BOD_EVENT_DISABLE : app_bod.h
- app_bod_event_enable() : app_bod.h
- APP_BOD_EVENT_ENABLE : app_bod.h
- APP_BOD_EVENT_LEVEL_0 : app_bod.h
- APP_BOD_EVENT_LEVEL_1 : app_bod.h
- APP_BOD_EVENT_LEVEL_2 : app_bod.h
- APP_BOD_EVENT_LEVEL_3 : app_bod.h
- APP_BOD_EVENT_LEVEL_4 : app_bod.h
- APP_BOD_EVENT_LEVEL_5 : app_bod.h
- APP_BOD_EVENT_LEVEL_6 : app_bod.h
- APP_BOD_EVENT_LEVEL_7 : app_bod.h
- app_bod_event_set_level() : app_bod.h
- app_bod_evt_handler_t : app_bod.h
- APP_BOD_EVT_REMOVED : app_bod.h
- APP_BOD_EVT_TRIGGERED : app_bod.h
- app_bod_evt_type_t : app_bod.h
- app_bod_init() : app_bod.h
- APP_BOD_INVALID : app_bod.h
- app_bod_state_t : app_bod.h
- APP_BOD_STATIC_DISABLE : app_bod.h
- APP_BOD_STATIC_ENABLE : app_bod.h
- app_bod_static_mode_enable() : app_bod.h
- app_boot_security_clock_set() : gr55xx_sys.h
- app_boot_turn_on_encrypt_clock() : gr55xx_sys.h
- APP_COMP_ACTIVITY : app_comp.h
- app_comp_deinit() : app_comp.h
- APP_COMP_EVT_DONE : app_comp.h
- APP_COMP_EVT_ERROR : app_comp.h
- app_comp_evt_handler_t : app_comp.h
- app_comp_evt_t : app_comp.h
- app_comp_get_handle() : app_comp.h
- app_comp_init() : app_comp.h
- APP_COMP_INVALID : app_comp.h
- app_comp_start() : app_comp.h
- app_comp_state_t : app_comp.h
- app_comp_stop() : app_comp.h
- app_dev_reset_cbk_t : esls.h
- APP_DMA_ACTIVITY : app_dma.h
- app_dma_deinit() : app_dma.h
- APP_DMA_EVT_BLK : app_dma.h
- APP_DMA_EVT_ERROR : app_dma.h
- app_dma_evt_handler_t : app_dma.h
- APP_DMA_EVT_TFR : app_dma.h
- app_dma_evt_type_t : app_dma.h
- app_dma_get_handle() : app_dma.h
- app_dma_init() : app_dma.h
- APP_DMA_INVALID : app_dma.h
- app_dma_start() : app_dma.h
- app_dma_state_t : app_dma.h
- APP_DRIVER_ADC_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_AES_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_COMP_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_DMA_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_DUAL_TIM_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_GR5332X : app_drv_config.h
- APP_DRIVER_GR5405 : app_drv_config.h
- APP_DRIVER_GR551X : app_drv_config.h
- APP_DRIVER_GR5525X : app_drv_config.h
- APP_DRIVER_GR5526X : app_drv_config.h
- APP_DRIVER_HMAC_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_I2C_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_I2S_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_ISO7816_WAKEUP_PRIORITY : app_drv_config.h
- app_driver_mutex_deinit : app_rtos_cfg.h
- app_driver_mutex_init : app_rtos_cfg.h
- app_driver_mutex_pend : app_rtos_cfg.h
- app_driver_mutex_post : app_rtos_cfg.h
- APP_DRIVER_PKC_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_PWM_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_QSPI_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_RNG_WAKEUP_PRIORITY : app_drv_config.h
- app_driver_sem_deinit : app_rtos_cfg.h
- app_driver_sem_init : app_rtos_cfg.h
- app_driver_sem_pend : app_rtos_cfg.h
- app_driver_sem_post : app_rtos_cfg.h
- app_driver_sem_post_from_isr : app_rtos_cfg.h
- APP_DRIVER_SPI_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_TIM_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRIVER_UART_WAKEUP_PRIORITY : app_drv_config.h
- APP_DRV_ASSERT : app_drv.h
- APP_DRV_ASSERT_ENABLE : app_drv_config.h
- APP_DRV_DEPRECATED : app_drv.h
- APP_DRV_ERR_BUSY : app_drv_error.h
- APP_DRV_ERR_CODE_CHECK : app_drv_error.h
- APP_DRV_ERR_HAL : app_drv_error.h
- APP_DRV_ERR_INVALID_ID : app_drv_error.h
- APP_DRV_ERR_INVALID_INIT : app_drv_error.h
- APP_DRV_ERR_INVALID_MODE : app_drv_error.h
- APP_DRV_ERR_INVALID_PARAM : app_drv_error.h
- APP_DRV_ERR_INVALID_TYPE : app_drv_error.h
- APP_DRV_ERR_NOT_INIT : app_drv_error.h
- APP_DRV_ERR_POINTER_NULL : app_drv_error.h
- app_drv_err_t : app_drv_error.h
- APP_DRV_ERR_TIMEOUT : app_drv_error.h
- APP_DRV_LOG_ERR : app_drv.h
- APP_DRV_LOG_INFO : app_drv.h
- APP_DRV_LOG_INTERFACE : app_drv_config.h
- APP_DRV_LOG_LEVEL : app_drv_config.h
- APP_DRV_LOG_WARN : app_drv.h
- APP_DRV_MAX_TIMEOUT : app_drv.h
- APP_DRV_MUTEX_DECL : app_rtos_cfg.h
- APP_DRV_MUTEX_STATIC : app_rtos_cfg.h
- APP_DRV_NEVER_TIMEOUT : app_drv.h
- APP_DRV_SEM_DECL : app_rtos_cfg.h
- APP_DRV_SEM_STATIC : app_rtos_cfg.h
- APP_DRV_SUCCESS : app_drv_error.h
- app_dspi_abort() : app_dspi.h
- app_dspi_abort_it() : app_dspi.h
- APP_DSPI_ACTIVITY : app_dspi.h
- app_dspi_command_async() : app_dspi.h
- app_dspi_command_sync() : app_dspi.h
- app_dspi_command_t : app_dspi.h
- app_dspi_command_transmit_async() : app_dspi.h
- app_dspi_command_transmit_sync() : app_dspi.h
- app_dspi_config_data_size() : app_dspi.h
- app_dspi_config_mode() : app_dspi.h
- app_dspi_deinit() : app_dspi.h
- APP_DSPI_DMA_ACTIVITY : app_dspi.h
- app_dspi_dma_command_async() : app_dspi_dma.h
- app_dspi_dma_command_transmit_async() : app_dspi_dma.h
- app_dspi_dma_deinit() : app_dspi_dma.h
- app_dspi_dma_init() : app_dspi_dma.h
- APP_DSPI_DMA_INVALID : app_dspi.h
- app_dspi_dma_sg_llp_transmit_async() : app_dspi_dma.h
- app_dspi_dma_state_t : app_dspi.h
- app_dspi_dma_transmit_async() : app_dspi_dma.h
- APP_DSPI_EVT_ABORT : app_dspi.h
- APP_DSPI_EVT_ERROR : app_dspi.h
- app_dspi_evt_handler_t : app_dspi.h
- APP_DSPI_EVT_TX_CPLT : app_dspi.h
- app_dspi_evt_type_t : app_dspi.h
- app_dspi_get_handle() : app_dspi.h
- app_dspi_init() : app_dspi.h
- APP_DSPI_INVALID : app_dspi.h
- APP_DSPI_PIN_DISABLE : app_dspi.h
- APP_DSPI_PIN_ENABLE : app_dspi.h
- app_dspi_state_t : app_dspi.h
- app_dspi_transmit_async() : app_dspi.h
- app_dspi_transmit_sync() : app_dspi.h
- APP_DUAL_TIM_ACTIVITY : app_dual_tim.h
- app_dual_tim_deinit() : app_dual_tim.h
- APP_DUAL_TIM_EVT_DONE : app_dual_tim.h
- APP_DUAL_TIM_EVT_ERROR : app_dual_tim.h
- app_dual_tim_evt_handler_t : app_dual_tim.h
- app_dual_tim_evt_t : app_dual_tim.h
- app_dual_tim_get_counter_value() : app_dual_tim.h
- app_dual_tim_get_handle() : app_dual_tim.h
- APP_DUAL_TIM_ID_0 : app_dual_tim.h
- APP_DUAL_TIM_ID_1 : app_dual_tim.h
- APP_DUAL_TIM_ID_MAX : app_dual_tim.h
- app_dual_tim_id_t : app_dual_tim.h
- app_dual_tim_init() : app_dual_tim.h
- APP_DUAL_TIM_INVALID : app_dual_tim.h
- app_dual_tim_set_background_reload() : app_dual_tim.h
- app_dual_tim_set_params() : app_dual_tim.h
- app_dual_tim_set_reload_value_bg_reload_value() : app_dual_tim.h
- app_dual_tim_start() : app_dual_tim.h
- app_dual_tim_state_t : app_dual_tim.h
- app_dual_tim_stop() : app_dual_tim.h
- APP_DVR_LOG_LVL_ERR : app_drv_config.h
- APP_DVR_LOG_LVL_INFO : app_drv_config.h
- APP_DVR_LOG_LVL_NONE : app_drv_config.h
- APP_DVR_LOG_LVL_WARN : app_drv_config.h
- app_gpiote_config() : app_gpiote.h
- app_gpiote_deinit() : app_gpiote.h
- app_gpiote_init() : app_gpiote.h
- app_graphics_adjust_dcore_policy() : app_graphics_ospi.h
- app_graphics_dc_access_type_e : app_graphics_dc.h
- app_graphics_dc_dspi_send_cmd_data_in_3wire_1lane() : app_graphics_dc.h
- app_graphics_dc_dspi_send_cmd_data_in_4wire_2lane() : app_graphics_dc.h
- app_graphics_dc_dspi_send_cmd_datas_in_4wire_2lane() : app_graphics_dc.h
- app_graphics_dc_dspi_send_cmd_in_3wire_1lane() : app_graphics_dc.h
- app_graphics_dc_frame_address_width_e : app_graphics_dc.h
- app_graphics_dc_frame_result_e : app_graphics_dc.h
- app_graphics_dc_frame_timing_e : app_graphics_dc.h
- app_graphics_dc_freq_set() : app_graphics_dc.h
- app_graphics_dc_send_single_frame() : app_graphics_dc.h
- app_graphics_dc_set_power_state() : app_graphics_dc.h
- app_graphics_dc_spi_send() : app_graphics_dc.h
- app_graphics_gpu_set_power_state() : app_graphics_gpu.h
- app_graphics_is_ospi_address() : app_graphics_ospi.h
- app_graphics_ospi_deinit() : app_graphics_ospi.h
- app_graphics_ospi_get_base_address() : app_graphics_ospi.h
- app_graphics_ospi_get_byte_size() : app_graphics_ospi.h
- app_graphics_ospi_get_read_prefetch() : app_graphics_ospi.h
- app_graphics_ospi_get_sleep_state() : app_graphics_ospi.h
- app_graphics_ospi_init() : app_graphics_ospi.h
- app_graphics_ospi_pasr_update() : app_graphics_ospi.h
- app_graphics_ospi_register_psram_reload_func() : app_graphics_ospi.h
- app_graphics_ospi_reset() : app_graphics_ospi.h
- app_graphics_ospi_set_pasr() : app_graphics_ospi.h
- app_graphics_ospi_set_power_state() : app_graphics_ospi.h
- app_graphics_ospi_set_read_prefetch() : app_graphics_ospi.h
- app_graphics_ospi_set_sleep_state() : app_graphics_ospi.h
- APP_HMAC_ACTIVITY : app_hmac.h
- app_hmac_deinit() : app_hmac.h
- APP_HMAC_EVT_DONE : app_hmac.h
- APP_HMAC_EVT_ERROR : app_hmac.h
- app_hmac_evt_handler_t : app_hmac.h
- app_hmac_evt_type_t : app_hmac.h
- app_hmac_get_handle() : app_hmac.h
- app_hmac_init() : app_hmac.h
- APP_HMAC_INVALID : app_hmac.h
- app_hmac_sha256_async() : app_hmac.h
- app_hmac_sha256_sync() : app_hmac.h
- app_hmac_state_t : app_hmac.h
- APP_HMAC_TYPE_DMA : app_hmac.h
- APP_HMAC_TYPE_INTERRUPT : app_hmac.h
- APP_HMAC_TYPE_MAX : app_hmac.h
- APP_HMAC_TYPE_POLLING : app_hmac.h
- app_hmac_type_t : app_hmac.h
- app_hmac_user_hash() : app_hmac.h
- APP_I2C_ABORT : app_i2c.h
- APP_I2C_ACTIVITY : app_i2c.h
- app_i2c_deinit() : app_i2c.h
- APP_I2C_DMA_ACTIVITY : app_i2c.h
- app_i2c_dma_deinit() : app_i2c_dma.h
- app_i2c_dma_init() : app_i2c_dma.h
- APP_I2C_DMA_INVALID : app_i2c.h
- app_i2c_dma_mem_read_async() : app_i2c_dma.h
- app_i2c_dma_mem_write_async() : app_i2c_dma.h
- app_i2c_dma_receive_async() : app_i2c_dma.h
- app_i2c_dma_state_t : app_i2c.h
- app_i2c_dma_transmit_async() : app_i2c_dma.h
- APP_I2C_EVT_ERROR : app_i2c.h
- app_i2c_evt_handler_t : app_i2c.h
- APP_I2C_EVT_RX_DATA : app_i2c.h
- APP_I2C_EVT_TX_CPLT : app_i2c.h
- app_i2c_evt_type_t : app_i2c.h
- app_i2c_get_handle() : app_i2c.h
- APP_I2C_ID_0 : app_i2c.h
- APP_I2C_ID_1 : app_i2c.h
- APP_I2C_ID_MAX : app_i2c.h
- app_i2c_id_t : app_i2c.h
- app_i2c_init() : app_i2c.h
- APP_I2C_INVALID : app_i2c.h
- app_i2c_master_abort_it() : app_i2c.h
- app_i2c_mem_read_async() : app_i2c.h
- app_i2c_mem_read_sync() : app_i2c.h
- app_i2c_mem_write_async() : app_i2c.h
- app_i2c_mem_write_sync() : app_i2c.h
- app_i2c_receive_async() : app_i2c.h
- app_i2c_receive_sync() : app_i2c.h
- APP_I2C_ROLE_MASTER : app_i2c.h
- APP_I2C_ROLE_MAX : app_i2c.h
- APP_I2C_ROLE_SLAVE : app_i2c.h
- app_i2c_role_t : app_i2c.h
- app_i2c_state_t : app_i2c.h
- app_i2c_timing_adjust() : app_i2c.h
- app_i2c_timing_get() : app_i2c.h
- app_i2c_transmit_async() : app_i2c.h
- app_i2c_transmit_receive_sync() : app_i2c.h
- app_i2c_transmit_sync() : app_i2c.h
- app_i2s_abort() : app_i2s.h
- APP_I2S_ACTIVITY : app_i2s.h
- app_i2s_deinit() : app_i2s.h
- app_i2s_disable() : app_i2s.h
- app_i2s_disable_clock() : app_i2s.h
- APP_I2S_DMA_ACTIVITY : app_i2s.h
- app_i2s_dma_deinit() : app_i2s_dma.h
- app_i2s_dma_init() : app_i2s_dma.h
- APP_I2S_DMA_INVALID : app_i2s.h
- app_i2s_dma_receive_async() : app_i2s_dma.h
- app_i2s_dma_state_t : app_i2s.h
- app_i2s_dma_transmit_async() : app_i2s_dma.h
- app_i2s_dma_transmit_receive_async() : app_i2s_dma.h
- app_i2s_enable() : app_i2s.h
- app_i2s_enable_clock() : app_i2s.h
- APP_I2S_EVT_ERROR : app_i2s.h
- app_i2s_evt_handler_t : app_i2s.h
- APP_I2S_EVT_RX_DATA : app_i2s.h
- APP_I2S_EVT_TX_CPLT : app_i2s.h
- APP_I2S_EVT_TX_RX : app_i2s.h
- app_i2s_evt_type_t : app_i2s.h
- app_i2s_flush_rx_fifo() : app_i2s.h
- app_i2s_flush_tx_fifo() : app_i2s.h
- app_i2s_get_handle() : app_i2s.h
- APP_I2S_ID_MASTER : app_i2s.h
- APP_I2S_ID_MAX : app_i2s.h
- APP_I2S_ID_SLAVE : app_i2s.h
- app_i2s_id_t : app_i2s.h
- app_i2s_init() : app_i2s.h
- APP_I2S_INVALID : app_i2s.h
- app_i2s_receive_async() : app_i2s.h
- app_i2s_receive_sync() : app_i2s.h
- app_i2s_state_t : app_i2s.h
- app_i2s_transmit_async() : app_i2s.h
- app_i2s_transmit_receive_async() : app_i2s.h
- app_i2s_transmit_receive_sync() : app_i2s.h
- app_i2s_transmit_sync() : app_i2s.h
- app_io_callback_t : app_io.h
- APP_IO_DEFAULT_CONFIG : app_io.h
- app_io_deinit() : app_io.h
- app_io_event_register_cb() : app_io.h
- app_io_event_unregister() : app_io.h
- app_io_init() : app_io.h
- APP_IO_INPUT_TYPE_CMOS : app_io.h
- APP_IO_INPUT_TYPE_MAX : app_io.h
- APP_IO_INPUT_TYPE_SCHMITT : app_io.h
- app_io_input_type_t : app_io.h
- APP_IO_MODE_ANALOG : app_io.h
- APP_IO_MODE_INPUT : app_io.h
- APP_IO_MODE_IT_FALLING : app_io.h
- APP_IO_MODE_IT_HIGH : app_io.h
- APP_IO_MODE_IT_LOW : app_io.h
- APP_IO_MODE_IT_RISING : app_io.h
- APP_IO_MODE_MAX : app_io.h
- APP_IO_MODE_MUX : app_io.h
- APP_IO_MODE_NONE : app_io.h
- APP_IO_MODE_OUTPUT : app_io.h
- app_io_mode_t : app_io.h
- APP_IO_MUX : app_io.h
- APP_IO_MUX_0 : app_io.h
- APP_IO_MUX_1 : app_io.h
- APP_IO_MUX_2 : app_io.h
- APP_IO_MUX_3 : app_io.h
- APP_IO_MUX_4 : app_io.h
- APP_IO_MUX_5 : app_io.h
- APP_IO_MUX_6 : app_io.h
- APP_IO_MUX_7 : app_io.h
- APP_IO_MUX_8 : app_io.h
- APP_IO_MUX_MAX : app_io.h
- app_io_mux_t : app_io.h
- APP_IO_NOPULL : app_io.h
- APP_IO_PIN_0 : app_io.h
- APP_IO_PIN_1 : app_io.h
- APP_IO_PIN_10 : app_io.h
- APP_IO_PIN_11 : app_io.h
- APP_IO_PIN_12 : app_io.h
- APP_IO_PIN_13 : app_io.h
- APP_IO_PIN_14 : app_io.h
- APP_IO_PIN_15 : app_io.h
- APP_IO_PIN_16 : app_io.h
- APP_IO_PIN_17 : app_io.h
- APP_IO_PIN_18 : app_io.h
- APP_IO_PIN_19 : app_io.h
- APP_IO_PIN_2 : app_io.h
- APP_IO_PIN_20 : app_io.h
- APP_IO_PIN_21 : app_io.h
- APP_IO_PIN_22 : app_io.h
- APP_IO_PIN_23 : app_io.h
- APP_IO_PIN_24 : app_io.h
- APP_IO_PIN_25 : app_io.h
- APP_IO_PIN_26 : app_io.h
- APP_IO_PIN_27 : app_io.h
- APP_IO_PIN_28 : app_io.h
- APP_IO_PIN_29 : app_io.h
- APP_IO_PIN_3 : app_io.h
- APP_IO_PIN_30 : app_io.h
- APP_IO_PIN_31 : app_io.h
- APP_IO_PIN_4 : app_io.h
- APP_IO_PIN_5 : app_io.h
- APP_IO_PIN_6 : app_io.h
- APP_IO_PIN_7 : app_io.h
- APP_IO_PIN_8 : app_io.h
- APP_IO_PIN_9 : app_io.h
- APP_IO_PIN_ALL : app_io.h
- APP_IO_PIN_MASK : app_io.h
- APP_IO_PIN_RESET : app_io.h
- APP_IO_PIN_SET : app_io.h
- app_io_pin_state_t : app_io.h
- APP_IO_PINS_0_15 : app_io.h
- APP_IO_PINS_0_7 : app_io.h
- APP_IO_PINS_16_31 : app_io.h
- APP_IO_PULL_MAX : app_io.h
- app_io_pull_t : app_io.h
- APP_IO_PULLDOWN : app_io.h
- APP_IO_PULLUP : app_io.h
- app_io_read_pin() : app_io.h
- app_io_set_intput_type() : app_io.h
- app_io_set_speed() : app_io.h
- app_io_set_strength() : app_io.h
- app_io_speed_t : app_io.h
- APP_IO_SPPED_HIGH : app_io.h
- APP_IO_SPPED_MAX : app_io.h
- APP_IO_SPPED_MEDIUM : app_io.h
- APP_IO_STRENGTH_HIGH : app_io.h
- APP_IO_STRENGTH_LOW : app_io.h
- APP_IO_STRENGTH_MAX : app_io.h
- APP_IO_STRENGTH_MEDIUM : app_io.h
- app_io_strength_t : app_io.h
- APP_IO_STRENGTH_ULTRA : app_io.h
- app_io_toggle_pin() : app_io.h
- APP_IO_TYPE_AON : app_io.h
- APP_IO_TYPE_GPIOA : app_io.h
- APP_IO_TYPE_GPIOB : app_io.h
- APP_IO_TYPE_GPIOC : app_io.h
- APP_IO_TYPE_MAX : app_io.h
- APP_IO_TYPE_MSIO : app_io.h
- APP_IO_TYPE_NORMAL : app_io.h
- app_io_type_t : app_io.h
- app_io_write_pin() : app_io.h
- APP_MSIO_IO_PIN_ALL : app_io.h
- app_ospi_access_mode_e : app_graphics_ospi.h
- app_ospi_clock_freq_e : app_graphics_ospi.h
- app_ospi_pasr_e : app_graphics_ospi.h
- app_ospi_phy_delay_e : app_graphics_ospi.h
- app_ospi_psram_drv_strength_e : app_graphics_ospi.h
- app_ospi_psram_rd_latency_e : app_graphics_ospi.h
- app_ospi_psram_wr_latency_e : app_graphics_ospi.h
- app_ospi_work_state_e : app_graphics_ospi.h
- APP_PARAM_ID_ACTIVITY_MOVE_CONFIG : nvds_tag.h
- APP_PARAM_ID_RF_LPCLK_DRIFT : nvds_tag.h
- APP_PARAM_ID_RF_XO_OFFSET : nvds_tag.h
- app_pdm_abort() : app_pdm.h
- APP_PDM_ACTIVITY : app_pdm.h
- app_pdm_deinit() : app_pdm.h
- APP_PDM_EVT_DMA_BLK : app_pdm.h
- APP_PDM_EVT_DMA_ERROR : app_pdm.h
- APP_PDM_EVT_DMA_TFR : app_pdm.h
- app_pdm_evt_handler_t : app_pdm.h
- APP_PDM_EVT_LEFT_OVERFLOW : app_pdm.h
- APP_PDM_EVT_RIGHT_OVERFLOW : app_pdm.h
- app_pdm_evt_type_t : app_pdm.h
- app_pdm_get_handle() : app_pdm.h
- APP_PDM_INACTIVITY : app_pdm.h
- app_pdm_init() : app_pdm.h
- app_pdm_left_start_dma() : app_pdm.h
- app_pdm_left_start_dma_sg_llp() : app_pdm.h
- app_pdm_right_start_dma() : app_pdm.h
- app_pdm_right_start_dma_sg_llp() : app_pdm.h
- app_pdm_state_t : app_pdm.h
- app_pdm_stereo_start_dma() : app_pdm.h
- app_pdm_stereo_start_dma_sg_llp() : app_pdm.h
- APP_PKC_ACTIVITY : app_pkc.h
- app_pkc_big_number_add_async() : app_pkc.h
- app_pkc_big_number_add_sync() : app_pkc.h
- app_pkc_big_number_add_t : app_pkc.h
- app_pkc_big_number_multi_async() : app_pkc.h
- app_pkc_big_number_multi_sync() : app_pkc.h
- app_pkc_big_number_multi_t : app_pkc.h
- app_pkc_deinit() : app_pkc.h
- app_pkc_ecc_point_multi_async() : app_pkc.h
- app_pkc_ecc_point_multi_sync() : app_pkc.h
- app_pkc_ecc_point_multi_t : app_pkc.h
- APP_PKC_EVT_DONE : app_pkc.h
- APP_PKC_EVT_ERROR : app_pkc.h
- app_pkc_evt_handler_t : app_pkc.h
- app_pkc_evt_type_t : app_pkc.h
- app_pkc_get_handle() : app_pkc.h
- app_pkc_init() : app_pkc.h
- APP_PKC_INVALID : app_pkc.h
- app_pkc_modular_add_async() : app_pkc.h
- app_pkc_modular_add_sync() : app_pkc.h
- app_pkc_modular_add_t : app_pkc.h
- app_pkc_modular_compare_async() : app_pkc.h
- app_pkc_modular_compare_sync() : app_pkc.h
- app_pkc_modular_compare_t : app_pkc.h
- app_pkc_modular_left_shift_async() : app_pkc.h
- app_pkc_modular_left_shift_sync() : app_pkc.h
- app_pkc_modular_shift_t : app_pkc.h
- app_pkc_modular_sub_async() : app_pkc.h
- app_pkc_modular_sub_sync() : app_pkc.h
- app_pkc_modular_sub_t : app_pkc.h
- app_pkc_montgomery_inversion_async() : app_pkc.h
- app_pkc_montgomery_inversion_sync() : app_pkc.h
- app_pkc_montgomery_inversion_t : app_pkc.h
- app_pkc_montgomery_multi_async() : app_pkc.h
- app_pkc_montgomery_multi_sync() : app_pkc.h
- app_pkc_montgomery_multi_t : app_pkc.h
- app_pkc_state_t : app_pkc.h
- APP_PKC_TYPE_INTERRUPT : app_pkc.h
- APP_PKC_TYPE_MAX : app_pkc.h
- APP_PKC_TYPE_POLLING : app_pkc.h
- app_pkc_type_t : app_pkc.h
- APP_PWM_ACTIVE_CHANNEL_A : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_ALL : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_B : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_C : app_pwm.h
- APP_PWM_ACTIVE_CHANNEL_CLEARED : app_pwm.h
- app_pwm_active_channel_t : app_pwm.h
- APP_PWM_ACTIVITY : app_pwm.h
- app_pwm_config_channel() : app_pwm.h
- app_pwm_deinit() : app_pwm.h
- app_pwm_get_handle() : app_pwm.h
- APP_PWM_ID_0 : app_pwm.h
- APP_PWM_ID_1 : app_pwm.h
- APP_PWM_ID_MAX : app_pwm.h
- app_pwm_id_t : app_pwm.h
- app_pwm_init() : app_pwm.h
- APP_PWM_INVALID : app_pwm.h
- app_pwm_module_state_t : app_pwm.h
- APP_PWM_PIN_DISABLE : app_pwm.h
- APP_PWM_PIN_ENABLE : app_pwm.h
- app_pwm_start() : app_pwm.h
- APP_PWM_START : app_pwm.h
- app_pwm_state_t : app_pwm.h
- app_pwm_stop() : app_pwm.h
- APP_PWM_STOP : app_pwm.h
- app_pwm_update_freq() : app_pwm.h
- app_pwr_mgmt_init() : app_pwr_mgmt.h
- app_qspi_abort() : app_qspi.h
- APP_QSPI_ACTIVITY : app_qspi.h
- app_qspi_command_async() : app_qspi.h
- app_qspi_command_receive_async() : app_qspi.h
- app_qspi_command_receive_sync() : app_qspi.h
- app_qspi_command_sync() : app_qspi.h
- app_qspi_command_t : app_qspi.h
- app_qspi_command_transmit_async() : app_qspi.h
- app_qspi_command_transmit_sync() : app_qspi.h
- app_qspi_deinit() : app_qspi.h
- APP_QSPI_DMA_ACTIVITY : app_qspi.h
- app_qspi_dma_command_async() : app_qspi_dma.h
- app_qspi_dma_command_receive_async() : app_qspi_dma.h
- app_qspi_dma_command_transmit_async() : app_qspi_dma.h
- app_qspi_dma_deinit() : app_qspi_dma.h
- app_qspi_dma_init() : app_qspi_dma.h
- APP_QSPI_DMA_INVALID : app_qspi.h
- app_qspi_dma_receive_async() : app_qspi_dma.h
- app_qspi_dma_receive_async_ex() : app_qspi_dma.h
- app_qspi_dma_state_t : app_qspi.h
- app_qspi_dma_transmit_async() : app_qspi_dma.h
- app_qspi_dma_transmit_async_ex() : app_qspi_dma.h
- app_qspi_dma_transmit_in_qpi_async() : app_qspi_dma.h
- APP_QSPI_EVT_ABORT : app_qspi.h
- APP_QSPI_EVT_ERROR : app_qspi.h
- app_qspi_evt_handler_t : app_qspi.h
- APP_QSPI_EVT_RX_DATA : app_qspi.h
- APP_QSPI_EVT_TX_CPLT : app_qspi.h
- app_qspi_evt_type_t : app_qspi.h
- app_qspi_get_handle() : app_qspi.h
- APP_QSPI_ID_0 : app_qspi.h
- APP_QSPI_ID_1 : app_qspi.h
- APP_QSPI_ID_MAX : app_qspi.h
- app_qspi_id_t : app_qspi.h
- app_qspi_init() : app_qspi.h
- APP_QSPI_INVALID : app_qspi.h
- APP_QSPI_PIN_DISABLE : app_qspi.h
- APP_QSPI_PIN_ENABLE : app_qspi.h
- app_qspi_receive_async() : app_qspi.h
- app_qspi_receive_async_ex() : app_qspi.h
- app_qspi_receive_sync() : app_qspi.h
- app_qspi_receive_sync_ex() : app_qspi.h
- app_qspi_state_t : app_qspi.h
- app_qspi_transmit_async() : app_qspi.h
- app_qspi_transmit_async_ex() : app_qspi.h
- app_qspi_transmit_in_qpi_async() : app_qspi.h
- app_qspi_transmit_sync() : app_qspi.h
- app_qspi_transmit_sync_ex() : app_qspi.h
- APP_RNG_ACTIVITY : app_rng.h
- app_rng_deinit() : app_rng.h
- APP_RNG_EVT_DONE : app_rng.h
- APP_RNG_EVT_ERROR : app_rng.h
- app_rng_evt_handler_t : app_rng.h
- app_rng_evt_type_t : app_rng.h
- app_rng_gen_async() : app_rng.h
- app_rng_gen_sync() : app_rng.h
- app_rng_get_handle() : app_rng.h
- app_rng_init() : app_rng.h
- APP_RNG_INVALID : app_rng.h
- app_rng_state_t : app_rng.h
- APP_RNG_TYPE_INTERRUPT : app_rng.h
- APP_RNG_TYPE_MAX : app_rng.h
- APP_RNG_TYPE_POLLING : app_rng.h
- app_rng_type_t : app_rng.h
- APP_RTC_ALARM_DISABLE_ALL : app_rtc.h
- APP_RTC_ALARM_DISABLE_DATE : app_rtc.h
- APP_RTC_ALARM_DISABLE_TICK : app_rtc.h
- app_rtc_alarm_t : app_rtc.h
- app_rtc_deinit() : app_rtc.h
- app_rtc_disable_event() : app_rtc.h
- APP_RTC_EVT_DATE_ALARM : app_rtc.h
- app_rtc_evt_handler_t : app_rtc.h
- APP_RTC_EVT_OVERFLOW : app_rtc.h
- APP_RTC_EVT_TICK_ALARM : app_rtc.h
- app_rtc_evt_type_t : app_rtc.h
- app_rtc_get_time() : app_rtc.h
- app_rtc_init() : app_rtc.h
- app_rtc_init_time() : app_rtc.h
- app_rtc_setup_alarm() : app_rtc.h
- app_rtc_setup_tick() : app_rtc.h
- app_rtc_time_t : app_rtc.h
- APP_SLEEP_CB_MAX : app_pwr_mgmt.h
- app_spi_abort() : app_spi.h
- APP_SPI_ACTIVITY : app_spi.h
- app_spi_deinit() : app_spi.h
- APP_SPI_DMA_ACTIVITY : app_spi.h
- app_spi_dma_deinit() : app_spi_dma.h
- app_spi_dma_init() : app_spi_dma.h
- APP_SPI_DMA_INVALID : app_spi.h
- app_spi_dma_read_eeprom_async() : app_spi_dma.h
- app_spi_dma_read_memory_async() : app_spi_dma.h
- app_spi_dma_receive_async() : app_spi_dma.h
- app_spi_dma_receive_high_speed_sync() : app_spi_dma.h
- app_spi_dma_state_t : app_spi.h
- app_spi_dma_transmit_async() : app_spi_dma.h
- app_spi_dma_transmit_high_speed_sync() : app_spi_dma.h
- app_spi_dma_transmit_receive_async() : app_spi_dma.h
- app_spi_dma_write_memory_async() : app_spi_dma.h
- APP_SPI_EVT_ABORT : app_spi.h
- APP_SPI_EVT_ERROR : app_spi.h
- app_spi_evt_handler_t : app_spi.h
- APP_SPI_EVT_RX_CPLT : app_spi.h
- APP_SPI_EVT_TX_CPLT : app_spi.h
- APP_SPI_EVT_TX_RX_CPLT : app_spi.h
- app_spi_evt_type_t : app_spi.h
- app_spi_get_handle() : app_spi.h
- APP_SPI_ID_MASTER : app_spi.h
- APP_SPI_ID_MAX : app_spi.h
- APP_SPI_ID_SLAVE : app_spi.h
- app_spi_id_t : app_spi.h
- app_spi_init() : app_spi.h
- APP_SPI_INVALID : app_spi.h
- APP_SPI_PIN_DISABLE : app_spi.h
- APP_SPI_PIN_ENABLE : app_spi.h
- app_spi_read_eeprom_async() : app_spi.h
- app_spi_read_eeprom_sync() : app_spi.h
- app_spi_read_memory_async() : app_spi.h
- app_spi_receive_async() : app_spi.h
- app_spi_receive_high_speed_sync() : app_spi.h
- app_spi_receive_sync() : app_spi.h
- app_spi_state_t : app_spi.h
- app_spi_transmit_async() : app_spi.h
- app_spi_transmit_high_speed_sync() : app_spi.h
- app_spi_transmit_receive_async() : app_spi.h
- app_spi_transmit_receive_sync() : app_spi.h
- app_spi_transmit_sync() : app_spi.h
- app_spi_write_memory_async() : app_spi.h
- app_spim_dma_receive_with_ia() : app_spi_dma.h
- app_spim_dma_transmit_with_ia() : app_spi_dma.h
- app_spim_receive_with_ia() : app_spi.h
- app_spim_transmit_with_ia() : app_spi.h
- APP_STORAGE_RAM_ID : app_qspi.h
- APP_TIM_ACTIVITY : app_tim.h
- app_tim_deinit() : app_tim.h
- APP_TIM_EVT_DONE : app_tim.h
- APP_TIM_EVT_ERROR : app_tim.h
- app_tim_evt_handler_t : app_tim.h
- app_tim_evt_t : app_tim.h
- app_tim_get_handle() : app_tim.h
- APP_TIM_ID_0 : app_tim.h
- APP_TIM_ID_1 : app_tim.h
- APP_TIM_ID_MAX : app_tim.h
- app_tim_id_t : app_tim.h
- app_tim_init() : app_tim.h
- APP_TIM_INVALID : app_tim.h
- app_tim_start() : app_tim.h
- app_tim_state_t : app_tim.h
- app_tim_stop() : app_tim.h
- app_uart_abort() : app_uart.h
- app_uart_abort_receive() : app_uart.h
- app_uart_abort_transmit() : app_uart.h
- APP_UART_ACTIVITY : app_uart.h
- app_uart_deinit() : app_uart.h
- APP_UART_DMA_ACTIVITY : app_uart.h
- app_uart_dma_deinit() : app_uart_dma.h
- app_uart_dma_init() : app_uart_dma.h
- APP_UART_DMA_INVALID : app_uart.h
- app_uart_dma_receive_async() : app_uart_dma.h
- app_uart_dma_state_t : app_uart.h
- app_uart_dma_transmit_async() : app_uart_dma.h
- APP_UART_EVT_ABORT_RX : app_uart.h
- APP_UART_EVT_ABORT_TX : app_uart.h
- APP_UART_EVT_ABORT_TXRX : app_uart.h
- APP_UART_EVT_ERROR : app_uart.h
- app_uart_evt_handler_t : app_uart.h
- APP_UART_EVT_RX_DATA : app_uart.h
- APP_UART_EVT_TX_CPLT : app_uart.h
- app_uart_evt_type_t : app_uart.h
- app_uart_flush() : app_uart.h
- app_uart_get_handle() : app_uart.h
- APP_UART_ID_0 : app_uart.h
- APP_UART_ID_1 : app_uart.h
- APP_UART_ID_MAX : app_uart.h
- app_uart_id_t : app_uart.h
- app_uart_init() : app_uart.h
- APP_UART_INVALID : app_uart.h
- app_uart_receive_async() : app_uart.h
- app_uart_receive_sync() : app_uart.h
- app_uart_state_t : app_uart.h
- app_uart_transmit_async() : app_uart.h
- app_uart_transmit_sync() : app_uart.h
- assert_err_cb_t : gr55xx_sys_sdk.h
- assert_param_cb_t : gr55xx_sys_sdk.h
- assert_warn_cb_t : gr55xx_sys_sdk.h
- ate_version : gr55xx_efuse_layout.h
- att_format_t : ble_att.h
- att_uuid_t : ble_att.h
- AUTO_RELOAD : gr55xx_hal_rtc.h