Public Attributes | List of all members
_ll_iso7816_init Struct Reference
Peripheral Driver » LL Driver » ISO7816 » Structures » ISO7816 Exported init structure

LL ISO7816 init Structure definition. More...

`#include <gr55xx_ll_iso7816.h>`

## Public Attributes
uint32_t | clk_div
uint32_t | wait_time
uint16_t | guard_time
uint8_t | detect_coding

## Detailed Description

LL ISO7816 init Structure definition.

Definition at line 74 of file gr55xx_ll_iso7816.h.

## Member Data Documentation

## ◆ clk_div

uint32_t _ll_iso7816_init::clk_div

clk_div is used for dividing the system clock, and IOS7816 output clock is equal to (system clock)/(clk_div+1).

Definition at line 76 of file gr55xx_ll_iso7816.h.

## ◆ detect_coding

uint8_t _ll_iso7816_init::detect_coding

Specifies whether automatically detect coding convention during ATR receiption.

Definition at line 80 of file gr55xx_ll_iso7816.h.

## ◆ guard_time

uint16_t _ll_iso7816_init::guard_time

Specifies the maximum card response time (leading edge to leading edge)

Definition at line 79 of file gr55xx_ll_iso7816.h.

## ◆ wait_time

uint32_t _ll_iso7816_init::wait_time

Specifies the guard time value in terms of number of baud clocks

Definition at line 78 of file gr55xx_ll_iso7816.h.

The documentation for this struct was generated from the following file:

- gr55xx_ll_iso7816.h