Functions
IO operation functions
Peripheral Driver » HAL Driver » DSPI » Functions

Data transfers functions. More...

## Functions
hal_status_t | hal_dspi_command_transmit (dspi_handle_t *p_dspi, dspi_command_t *p_cmd, uint8_t *p_data, uint32_t timeout)
| Transmit an amount of data with the specified instruction in blocking mode. More...
hal_status_t | hal_dspi_command (dspi_handle_t *p_dspi, dspi_command_t *p_cmd, uint32_t timeout)
| Transmit only instruction in blocking mode. More...
hal_status_t | hal_dspi_transmit (dspi_handle_t *p_qspi, uint8_t *p_data, uint32_t length, uint32_t timeout)
| Transmit an amount of data in blocking mode. More...
hal_status_t | hal_dspi_command_transmit_it (dspi_handle_t *p_dspi, dspi_command_t *p_cmd, uint8_t *p_data)
| Transmit an amount of data with the specified instruction in non-blocking mode with Interrupt. More...
hal_status_t | hal_dspi_command_it (dspi_handle_t *p_dspi, dspi_command_t *p_cmd)
| Transmit instruction in non-blocking mode with Interrupt. More...
hal_status_t | hal_dspi_transmit_it (dspi_handle_t *p_dspi, uint8_t *p_data, uint32_t length)
| Transmit an amount of data in non-blocking mode with Interrupt. More...
hal_status_t | hal_dspi_command_transmit_dma (dspi_handle_t *p_dspi, dspi_command_t *p_cmd, uint8_t *p_data)
| Transmit an amount of data with the specified instruction in non-blocking mode with DMA . More...
hal_status_t | hal_dspi_command_transmit_dma_sg_llp (dspi_handle_t *p_dspi, dspi_command_t *p_cmd, uint8_t *p_data, dma_sg_llp_config_t *sg_llp_config)
| Transmit an amount of data with the specified instruction in non-blocking mode with DMA SG or LLP. More...
hal_status_t | hal_dspi_command_dma (dspi_handle_t *p_dspi, dspi_command_t *p_cmd)
| Transmit instruction in non-blocking mode with DMA. More...
hal_status_t | hal_dspi_transmit_dma (dspi_handle_t *p_dspi, uint8_t *p_data, uint32_t length)
| Transmit an amount of data in non-blocking mode with DMA. More...
hal_status_t | hal_dspi_transmit_dma_sg_llp (dspi_handle_t *p_dspi, uint8_t *p_data, uint32_t length, dma_sg_llp_config_t *sg_llp_config)
| Transmit an amount of data in non-blocking mode with DMA SG or LLP. More...
hal_status_t | hal_dspi_abort (dspi_handle_t *p_dspi)
| Abort the current transmission. More...
hal_status_t | hal_dspi_abort_it (dspi_handle_t *p_dspi)
| Abort the current transmission (non-blocking function) More...

## Detailed Description

Data transfers functions.

      ==============================================================================
                          ##### IO operation functions #####
     ===============================================================================
     [..]
        This subsection provides a set of functions allowing to manage the DSPI
        data transfers.

        [..] The DSPI only supports master:

        (#) There are two modes of transfer:
           (++) Blocking mode: The communication is performed in polling mode.
                The HAL status of all data processing is returned by the same function
                after finishing transfer.
           (++) No-Blocking mode: The communication is performed using Interrupts.
                or DMA, These APIs return the HAL status.
                The end of the data processing will be indicated through the
                dedicated DSPI IRQ when using Interrupt mode or the DMA IRQ when
                using DMA mode.
                The hal_dspi_tx_cplt_callback() user callbacks
                will be executed respectively at the end of the transmit or Receive process.
                The hal_dspi_error_callback() user callback will be executed when a communication error is detected

        (#) APIs provided for these 2 transfer modes (Blocking mode or Non blocking mode using either Interrupt or DMA)
            exist for 1 Line (simplex) and 2 Lines (full duplex) modes.

## Function Documentation

## ◆ hal_dspi_abort()

hal_status_t hal_dspi_abort | ( | dspi_handle_t * | p_dspi | ) |

Abort the current transmission.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_abort_it()

hal_status_t hal_dspi_abort_it | ( | dspi_handle_t * | p_dspi | ) |

Abort the current transmission (non-blocking function)

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_command()

hal_status_t hal_dspi_command | ( | dspi_handle_t * | p_dspi,
|  | dspi_command_t * | p_cmd,
|  | uint32_t | timeout
| ) |  |

Transmit only instruction in blocking mode.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_cmd | Pointer to a dspi_command_t structure that contains the instruction and address for data transfer.
  [in] | timeout | Timeout duration

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_command_dma()

hal_status_t hal_dspi_command_dma | ( | dspi_handle_t * | p_dspi,
|  | dspi_command_t * | p_cmd
| ) |  |

Transmit instruction in non-blocking mode with DMA.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_cmd | Pointer to a dspi_command_t structure that contains the instruction and address for data transfer.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_command_it()

hal_status_t hal_dspi_command_it | ( | dspi_handle_t * | p_dspi,
|  | dspi_command_t * | p_cmd
| ) |  |

Transmit instruction in non-blocking mode with Interrupt.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_cmd | Pointer to a dspi_command_t structure that contains the instruction and address for data transfer.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_command_transmit()

hal_status_t hal_dspi_command_transmit | ( | dspi_handle_t * | p_dspi,
|  | dspi_command_t * | p_cmd,
|  | uint8_t * | p_data,
|  | uint32_t | timeout
| ) |  |

Transmit an amount of data with the specified instruction in blocking mode.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_cmd | Pointer to a dspi_command_t structure that contains the instruction and address for data transfer.
  [in] | p_data | Pointer to data buffer
  [in] | timeout | Timeout duration

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_command_transmit_dma()

hal_status_t hal_dspi_command_transmit_dma | ( | dspi_handle_t * | p_dspi,
|  | dspi_command_t * | p_cmd,
|  | uint8_t * | p_data
| ) |  |

Transmit an amount of data with the specified instruction in non-blocking mode with DMA .

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_cmd | Pointer to a dspi_command_t structure that contains the instruction and address for data transfer.
  [in] | p_data | Pointer to data buffer

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_command_transmit_dma_sg_llp()

hal_status_t hal_dspi_command_transmit_dma_sg_llp | ( | dspi_handle_t * | p_dspi,
|  | dspi_command_t * | p_cmd,
|  | uint8_t * | p_data,
|  | dma_sg_llp_config_t * | sg_llp_config
| ) |  |

Transmit an amount of data with the specified instruction in non-blocking mode with DMA SG or LLP.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_cmd | Pointer to a dspi_command_t structure that contains the instruction and address for data transfer.
  [in] | p_data | Pointer to data buffer
  [in] | sg_llp_config | The config of source and destination's SG and LLP.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_command_transmit_it()

hal_status_t hal_dspi_command_transmit_it | ( | dspi_handle_t * | p_dspi,
|  | dspi_command_t * | p_cmd,
|  | uint8_t * | p_data
| ) |  |

Transmit an amount of data with the specified instruction in non-blocking mode with Interrupt.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_cmd | Pointer to a dspi_command_t structure that contains the instruction and address for data transfer.
  [in] | p_data | Pointer to data buffer

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_transmit()

hal_status_t hal_dspi_transmit | ( | dspi_handle_t * | p_qspi,
|  | uint8_t * | p_data,
|  | uint32_t | length,
|  | uint32_t | timeout
| ) |  |

Transmit an amount of data in blocking mode.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_qspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_data | Pointer to data buffer
  [in] | length | Amount of data to be sent in bytes
  [in] | timeout | Timeout duration

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_transmit_dma()

hal_status_t hal_dspi_transmit_dma | ( | dspi_handle_t * | p_dspi,
|  | uint8_t * | p_data,
|  | uint32_t | length
| ) |  |

Transmit an amount of data in non-blocking mode with DMA.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_data | Pointer to data buffer
  [in] | length | Amount of data to be sent in bytes, ranging between 0 and 4095.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_transmit_dma_sg_llp()

hal_status_t hal_dspi_transmit_dma_sg_llp | ( | dspi_handle_t * | p_dspi,
|  | uint8_t * | p_data,
|  | uint32_t | length,
|  | dma_sg_llp_config_t * | sg_llp_config
| ) |  |

Transmit an amount of data in non-blocking mode with DMA SG or LLP.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_data | Pointer to data buffer
  [in] | length | Amount of data to be sent in bytes, ranging between 0 and 4095.
  [in] | sg_llp_config | The config of source and destination's SG and LLP.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_dspi_transmit_it()

hal_status_t hal_dspi_transmit_it | ( | dspi_handle_t * | p_dspi,
|  | uint8_t * | p_data,
|  | uint32_t | length
| ) |  |

Transmit an amount of data in non-blocking mode with Interrupt.

Note
  This function is used only in Indirect Write Mode.

Parameters

  [in] | p_dspi | Pointer to a DSPI handle which contains the configuration information for the specified DSPI module.
  [in] | p_data | Pointer to data buffer
  [in] | length | Amount of data to be sent in bytes

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.