Public Attributes | List of all members
ble_gap_evt_subrate_chg_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Subrate change indication event for BLE_GAPC_EVT_SUBRATE_CHANGE_IND. More...

`#include <ble_gapc.h>`

## Public Attributes
uint16_t | subrate_factor
uint16_t | con_latency
uint16_t | continuation_number
uint16_t | supervision_timeout

## Detailed Description

Subrate change indication event for BLE_GAPC_EVT_SUBRATE_CHANGE_IND.

Definition at line 1004 of file ble_gapc.h.

## Member Data Documentation

## ◆ con_latency

uint16_t ble_gap_evt_subrate_chg_ind_t::con_latency

Connection latency value.

Definition at line 1007 of file ble_gapc.h.

## ◆ continuation_number

uint16_t ble_gap_evt_subrate_chg_ind_t::continuation_number

Connection continuation number value.

Definition at line 1008 of file ble_gapc.h.

## ◆ subrate_factor

uint16_t ble_gap_evt_subrate_chg_ind_t::subrate_factor

subrate factor value.

Definition at line 1006 of file ble_gapc.h.

## ◆ supervision_timeout

uint16_t ble_gap_evt_subrate_chg_ind_t::supervision_timeout

Connection supervision timeout value.

Definition at line 1009 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h