Macros
Instruction phase for concurrent xip mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants

## Macros
#define | QSPI_CONCURRENT_XIP_INST_ENABLE LL_QSPI_CONCURRENT_XIP_INST_ENABLE
#define | QSPI_CONCURRENT_XIP_INST_DISABLE LL_QSPI_CONCURRENT_XIP_INST_DISABLE

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_INST_DISABLE

#define QSPI_CONCURRENT_XIP_INST_DISABLE LL_QSPI_CONCURRENT_XIP_INST_DISABLE

Disable Instruction phase.

Definition at line 655 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_INST_ENABLE

#define QSPI_CONCURRENT_XIP_INST_ENABLE LL_QSPI_CONCURRENT_XIP_INST_ENABLE

Enable Instruction phase.

Definition at line 654 of file gr55xx_hal_qspi.h.