Here is a list of all file members with links to the files they belong to:

### - p -

- p_device_resume_func : gr533x_hal_pwr_mgmt.h
- p_device_suspend_func : gr533x_hal_pwr_mgmt.h
- PACK_INT : ble_iso.h
- PACK_SEQ : ble_iso.h
- PACKAGE_NONE : gr533x_sys_sdk.h
- PACKAGE_QFN32 : gr533x_sys_sdk.h
- PACKAGE_QFN48 : gr533x_sys_sdk.h
- package_type_t : gr533x_sys_sdk.h
- PARAM_ID : nvds_tag.h
- PARAM_ID_ACTCLK_DRIFT : nvds_tag.h
- PARAM_ID_ACTIVITY_MOVE_CONFIG : nvds_tag.h
- PARAM_ID_BD_ADDRESS : nvds_tag.h
- PARAM_ID_CH_ASS_EN : nvds_tag.h
- PARAM_ID_DEVICE_NAME : nvds_tag.h
- PARAM_ID_DFT_SLAVE_MD : nvds_tag.h
- PARAM_ID_DIAG_BLE_HW : nvds_tag.h
- PARAM_ID_DIAG_DM_HW : nvds_tag.h
- PARAM_ID_DIAG_PLF : nvds_tag.h
- PARAM_ID_DIAG_SW : nvds_tag.h
- PARAM_ID_GDX_ADV_INT : nvds_tag.h
- PARAM_ID_LE_CODED_PHY_500 : nvds_tag.h
- PARAM_ID_LE_DBG_FIXED_P256_KEY : nvds_tag.h
- PARAM_ID_LE_PRIVATE_KEY_P256 : nvds_tag.h
- PARAM_ID_LPCLK_DRIFT : nvds_tag.h
- PARAM_ID_RF_BTIPT_GAIN_SETTING : nvds_tag.h
- PARAM_ID_RF_BTIPT_VERSION : nvds_tag.h
- PARAM_ID_RF_BTIPT_XO_SETTING : nvds_tag.h
- PARAM_ID_RF_XO_OFFSET : nvds_tag.h
- PARAM_ID_RSSI_HIGH_THR : nvds_tag.h
- PARAM_ID_RSSI_INTERF_THR : nvds_tag.h
- PARAM_ID_RSSI_LOW_THR : nvds_tag.h
- PARAM_ID_SCAN_EXT_ADV : nvds_tag.h
- PARAM_ID_SCHED_SCAN_DUR : nvds_tag.h
- PARAM_ID_TRACER_CONFIG : nvds_tag.h
- pass_alert_status_set() : pass.h
- PASS_ALERT_STATUS_VAL_LEN : pass.h
- PASS_ALL_STATE_ACTIVE : pass.h
- pass_c_alert_status_notify_set() : pass_c.h
- pass_c_alert_status_read() : pass_c.h
- PASS_C_ALL_STATE_ACTIVE : pass_c.h
- PASS_C_CONNECTION_MAX : pass_c.h
- pass_c_ctrl_point_set() : pass_c.h
- PASS_C_CTRL_PT_CANCEL_SLIENT_MODE : pass_c.h
- PASS_C_CTRL_PT_MUTE_ONCE : pass_c.h
- PASS_C_CTRL_PT_SILENT_MODE : pass_c.h
- pass_c_disc_srvc_start() : pass_c.h
- PASS_C_DISPLAY_ALERT_ACTIVE : pass_c.h
- PASS_C_EVT_ALERT_STATUS_NTF_SET_SUCCESS : pass_c.h
- PASS_C_EVT_ALERT_STATUS_RECEIVE : pass_c.h
- PASS_C_EVT_CTRL_POINT_SET_SUCCESS : pass_c.h
- PASS_C_EVT_DISCOVERY_COMPLETE : pass_c.h
- PASS_C_EVT_DISCOVERY_FAIL : pass_c.h
- pass_c_evt_handler_t : pass_c.h
- PASS_C_EVT_INVALID : pass_c.h
- PASS_C_EVT_RINGER_SET_NTF_SET_SUCCESS : pass_c.h
- PASS_C_EVT_RINGER_SET_RECEIVE : pass_c.h
- pass_c_evt_type_t : pass_c.h
- PASS_C_EVT_WRITE_OP_ERR : pass_c.h
- PASS_C_NO_STATE_ACTIVE : pass_c.h
- PASS_C_RINGER_ACTIVE : pass_c.h
- pass_c_ringer_ctrl_pt_t : pass_c.h
- PASS_C_RINGER_CTRL_PT_VAL_LEN : pass_c.h
- PASS_C_RINGER_SET_NORMAL : pass_c.h
- pass_c_ringer_set_notify_set() : pass_c.h
- pass_c_ringer_set_read() : pass_c.h
- PASS_C_RINGER_SET_SILENT : pass_c.h
- PASS_C_VIBRATE_ACTIVE : pass_c.h
- PASS_CHAR_FULL : pass.h
- PASS_CHAR_MANDATORY : pass.h
- PASS_CHAR_RING_CTRL_PT_SUP : pass.h
- pass_client_init() : pass_c.h
- PASS_CONNECTION_MAX : pass.h
- PASS_CTRL_PT_CANCEL_SLIENT_MODE : pass.h
- PASS_CTRL_PT_MUTE_ONCE : pass.h
- PASS_CTRL_PT_SILENT_MODE : pass.h
- PASS_DISPLAY_ALERT_ACTIVE : pass.h
- PASS_EVT_ALERT_STATUS_NTF_DISABLE : pass.h
- PASS_EVT_ALERT_STATUS_NTF_ENABLE : pass.h
- pass_evt_handler_t : pass.h
- PASS_EVT_INVALID : pass.h
- PASS_EVT_MUTE_ONCE_SET : pass.h
- PASS_EVT_RINGER_SET_NTF_DISABLE : pass.h
- PASS_EVT_RINGER_SET_NTF_ENABLE : pass.h
- PASS_EVT_SILENT_MODE_CANCEL : pass.h
- PASS_EVT_SILENT_MODE_SET : pass.h
- pass_evt_type_t : pass.h
- PASS_NO_STATE_ACTIVE : pass.h
- PASS_RINGER_ACTIVE : pass.h
- pass_ringer_ctrl_pt_t : pass.h
- PASS_RINGER_CTRL_PT_VAL_LEN : pass.h
- PASS_RINGER_SET_NORMAL : pass.h
- PASS_RINGER_SET_SILENT : pass.h
- PASS_RINGER_SET_VAL_LEN : pass.h
- pass_ringer_setting_get() : pass.h
- pass_ringer_setting_set() : pass.h
- pass_service_init() : pass.h
- PASS_VIBRATE_ACTIVE : pass.h
- PCS_CONNECTION_MAX : pcs.h
- PCS_EVT_DISCONNECTED : pcs.h
- pcs_evt_handler_t : pcs.h
- PCS_EVT_INVALID : pcs.h
- PCS_EVT_PARAM_SET : pcs.h
- PCS_EVT_SETTING_DISABLE : pcs.h
- PCS_EVT_SETTING_ENABLE : pcs.h
- PCS_EVT_TX_DATA_SENT : pcs.h
- PCS_EVT_TX_DISABLE : pcs.h
- PCS_EVT_TX_ENABLE : pcs.h
- pcs_evt_type_t : pcs.h
- PCS_MAX_DATA_LEN : pcs.h
- pcs_service_init() : pcs.h
- PCS_SERVICE_UUID : pcs.h
- PCS_SET_ADV_DATA_10B : pcs.h
- PCS_SET_ADV_DATA_17B : pcs.h
- PCS_SET_ADV_DATA_24B : pcs.h
- PCS_SET_ADV_DATA_31B : pcs.h
- PCS_SET_ADV_DATA_3B : pcs.h
- PCS_SET_PARAM_FAIL : pcs.h
- PCS_SET_PARAM_SUCCESS : pcs.h
- pcs_setting_reply() : pcs.h
- PCS_SETTING_TYPE_ADV_DATA : pcs.h
- PCS_SETTING_TYPE_ADV_INTERVAL : pcs.h
- PCS_SETTING_TYPE_CONN_PARAM : pcs.h
- PCS_SETTING_TYPE_PHY : pcs.h
- pcs_setting_type_t : pcs.h
- PCS_SETTING_TYPE_TX_POWER : pcs.h
- pcs_tx_data_send() : pcs.h
- PERIPH_DEVICE_NUM_AES : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_CLK_CALIB : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_DMA0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C1 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PWM0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PWM1 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_RNG : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SNSADC : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SPIM : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SPIS : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART1 : gr533x_hal_pwr_mgmt.h
- periph_device_number_t : gr533x_hal_pwr_mgmt.h
- periph_func_t : gr533x_pwr.h
- periph_state_t : gr533x_hal_pwr_mgmt.h
- platform_clock_init() : platform_sdk.h
- platform_init() : platform_sdk.h
- platform_rc_calibration() : platform_sdk.h
- platform_sdk_init() : platform_sdk.h
- PMR_BB_FRAME_ONGOING : gr533x_pwr.h
- PMR_BLE_ACTIVE_MODE : gr533x_pwr.h
- PMR_BT_ACTIVE_MODE : gr533x_pwr.h
- PMR_CRYPT_ONGOING : gr533x_pwr.h
- PMR_CSB_NOT_LPO_ALLOWED : gr533x_pwr.h
- PMR_DEEP_SLEEP : gr533x_pwr.h
- PMR_HOP_CALC_ONGOING : gr533x_pwr.h
- PMR_MGMT_ACTIVE_MODE : gr533x_pwr.h
- PMR_MGMT_FAIL : gr533x_pwr.h
- PMR_MGMT_IDLE_MODE : gr533x_pwr.h
- PMR_MGMT_SLEEP_MODE : gr533x_pwr.h
- PMR_MGMT_SUCCESS : gr533x_pwr.h
- PMR_MWS_WLAN_EVENT_GENERATOR_ACTIVE : gr533x_pwr.h
- PMR_PLF_DEEP_SLEEP_DISABLED : gr533x_pwr.h
- PMR_TL_RX_ONGOING : gr533x_pwr.h
- PMR_TL_TX_ONGOING : gr533x_pwr.h
- PMR_WAKE_UP_ONGOING : gr533x_pwr.h
- pmu_calibration_handler() : platform_sdk.h
- POL_SET : gr533x_ll_gpio.h
- PRF_CHAR_PRES_FMT_SIZE : ble_prf_types.h
- prf_cli_conf_t : ble_prf_types.h
- PRF_CLI_START_IND : ble_prf_types.h
- PRF_CLI_START_NTF : ble_prf_types.h
- PRF_CLI_STOP_NTFIND : ble_prf_types.h
- prf_error_handler_t : ble_prf_types.h
- prf_find_handle_by_idx() : ble_prf_utils.h
- prf_find_idx_by_handle() : ble_prf_utils.h
- prf_init_func_t : ble_prf.h
- PRF_INVALID_HANDLE : ble_prf_types.h
- prf_is_cccd_value_valid() : ble_prf_utils.h
- prf_is_indication_enabled() : ble_prf_utils.h
- prf_is_notification_enabled() : ble_prf_utils.h
- prf_on_connect_func_t : ble_prf.h
- prf_on_disconnect_func_t : ble_prf.h
- prf_pack_char_pres_fmt() : ble_prf_utils.h
- prf_pack_date_time() : ble_prf_utils.h
- prf_unpack_char_pres_fmt() : ble_prf_utils.h
- prf_unpack_date_time() : ble_prf_utils.h
- PROTOCOL_MODE : ble_lcp.h
- PUBLIC : ble_iso.h
- PWM_ACTIONEVENT_CLEAR : gr533x_hal_pwm.h
- PWM_ACTIONEVENT_NONE : gr533x_hal_pwm.h
- PWM_ACTIONEVENT_SET : gr533x_hal_pwm.h
- PWM_ACTIONEVENT_TOGGLE : gr533x_hal_pwm.h
- PWM_ALIGNED_CENTER : gr533x_hal_pwm.h
- PWM_ALIGNED_EDGE : gr533x_hal_pwm.h
- PWM_BREATH_MODE : gr533x_hal_pwm.h
- PWM_CODING_CHANNEL_A : gr533x_hal_pwm.h
- PWM_CODING_CHANNEL_ALL : gr533x_hal_pwm.h
- PWM_CODING_MODE : gr533x_hal_pwm.h
- PWM_DRIVEPOLARITY_NEGATIVE : gr533x_hal_pwm.h
- PWM_DRIVEPOLARITY_POSITIVE : gr533x_hal_pwm.h
- PWM_FLICKER_MODE : gr533x_hal_pwm.h
- PWM_PWR_ID : app_pwr_mgmt.h
- PWM_STOP_LVL_HIGH : gr533x_hal_pwm.h
- PWM_STOP_LVL_LOW : gr533x_hal_pwm.h
- PWM_WAITING_TIME_LVL_HIGH : gr533x_hal_pwm.h
- PWM_WAITING_TIME_LVL_LOW : gr533x_hal_pwm.h
- pwr_before_sleep_func_t : gr533x_pwr.h
- pwr_dev_check_func_t : gr533x_pwr.h
- pwr_enter_sleep_check() : app_pwr_mgmt.h
- pwr_handler_t : gr533x_hal_sleep_timer.h
- PWR_ID_MAX : app_pwr_mgmt.h
- pwr_id_t : app_pwr_mgmt.h
- PWR_MEM_POWER_FULL : gr533x_hal_pwr.h
- PWR_MEM_POWER_OFF : gr533x_hal_pwr.h
- PWR_MEM_POWER_RETENTION : gr533x_hal_pwr.h
- pwr_mgmt_baseband_state_get() : gr533x_pwr.h
- PWR_MGMT_BB_CHECK_FAIL : gr533x_pwr.h
- pwr_mgmt_ble_wakeup() : gr533x_pwr.h
- pwr_mgmt_check_ble_event() : gr533x_pwr.h
- pwr_mgmt_dev_init() : gr533x_pwr.h
- pwr_mgmt_dev_resume() : gr533x_pwr.h
- pwr_mgmt_dev_state_t : gr533x_pwr.h
- pwr_mgmt_dev_suspend() : gr533x_pwr.h
- pwr_mgmt_get_wakeup_flag() : gr533x_pwr.h
- pwr_mgmt_init() : gr533x_pwr.h
- pwr_mgmt_load_context() : gr533x_pwr.h
- pwr_mgmt_mem_ctl_set() : gr533x_pwr.h
- PWR_MGMT_MODE_CHECK_FAIL : gr533x_pwr.h
- pwr_mgmt_mode_get() : gr533x_pwr.h
- pwr_mgmt_mode_set() : gr533x_pwr.h
- pwr_mgmt_mode_t : gr533x_pwr.h
- pwr_mgmt_register_trace_func() : gr533x_pwr.h
- pwr_mgmt_save_context() : gr533x_pwr.h
- pwr_mgmt_schedule() : gr533x_pwr.h
- pwr_mgmt_set_callback() : gr533x_pwr.h
- pwr_mgmt_set_wakeup_flag() : gr533x_pwr.h
- pwr_mgmt_shutdown() : gr533x_pwr.h
- pwr_mgmt_sleep() : gr533x_pwr.h
- pwr_mgmt_ultra_sleep() : gr533x_pwr.h
- pwr_mgmt_warm_boot() : platform_sdk.h
- pwr_mgmt_wfe_sleep() : gr533x_pwr.h
- pwr_register_sleep_cb() : app_pwr_mgmt.h
- pwr_slp_elapsed_handler_t : gr533x_hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_NORMAL : gr533x_hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_RELOAD : gr533x_hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_SINGLE : gr533x_hal_sleep_timer.h
- pwr_table : gr533x_pwr.h
- PWR_TIMER_TYPE_AON_WDT : gr533x_hal_pwr.h
- PWR_TIMER_TYPE_AON_WDT_TIMER : gr533x_hal_pwr.h
- PWR_TIMER_TYPE_CAL_ALARM : gr533x_hal_pwr.h
- PWR_TIMER_TYPE_CAL_TIMER : gr533x_hal_pwr.h
- PWR_TIMER_TYPE_SLP_TIMER : gr533x_hal_pwr.h
- pwr_unregister_sleep_cb() : app_pwr_mgmt.h
- pwr_wake_up_ind() : app_pwr_mgmt.h
- PWR_WKUP_COND_ALL : gr533x_hal_pwr.h
- PWR_WKUP_COND_AON_WDT : gr533x_hal_pwr.h
- PWR_WKUP_COND_AUSB : gr533x_hal_pwr.h
- PWR_WKUP_COND_BLE : gr533x_hal_pwr.h
- PWR_WKUP_COND_CLDR : gr533x_hal_pwr.h
- PWR_WKUP_COND_CLDR_TICK : gr533x_hal_pwr.h
- PWR_WKUP_COND_DUSB : gr533x_hal_pwr.h
- PWR_WKUP_COND_EXT : gr533x_hal_pwr.h
- PWR_WKUP_COND_MSIO_COMP : gr533x_hal_pwr.h
- PWR_WKUP_COND_TIMER : gr533x_hal_pwr.h