Macros
Defines
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control

## Macros
#define | BLE_GAP_CHNL_MAP_LEN 0x05
#define | BLE_GAP_FEATS_LEN 0x08
#define | BLE_GAP_ADDR_LEN 0x06
#define | BLE_GAP_INVALID_CONN_INDEX 0xFF
#define | BLE_GAP_MIN_CTE_LEN 0x02
| CTE length (in number of 8us periods) More...
#define | BLE_GAP_MAX_CTE_LEN 0x14
#define | BLE_GAP_MIN_CTE_CNT 0x01
| CTE count. More...
#define | BLE_GAP_MAX_CTE_CNT 0x10
#define | BLE_GAP_MIN_IQ_SAMPLE_NUM 0x09
#define | BLE_GAP_MAX_IQ_SAMPLE_NUM 0x52
#define | BLE_GAP_MAX_GDX_RANGING_CH 20

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_GAP_ADDR_LEN

#define BLE_GAP_ADDR_LEN 0x06

The length of address.

Definition at line 70 of file ble_gapc.h.

## ◆ BLE_GAP_CHNL_MAP_LEN

#define BLE_GAP_CHNL_MAP_LEN 0x05

The length of channel map.

Definition at line 68 of file ble_gapc.h.

## ◆ BLE_GAP_FEATS_LEN

#define BLE_GAP_FEATS_LEN 0x08

The length of features.

Definition at line 69 of file ble_gapc.h.

## ◆ BLE_GAP_INVALID_CONN_INDEX

#define BLE_GAP_INVALID_CONN_INDEX 0xFF

Invalid connection index.

Definition at line 71 of file ble_gapc.h.

## ◆ BLE_GAP_MAX_CTE_CNT

#define BLE_GAP_MAX_CTE_CNT 0x10

The maximum CTE count.

Definition at line 79 of file ble_gapc.h.

## ◆ BLE_GAP_MAX_CTE_LEN

#define BLE_GAP_MAX_CTE_LEN 0x14

The maximum CTE length.

Definition at line 75 of file ble_gapc.h.

## ◆ BLE_GAP_MAX_GDX_RANGING_CH

#define BLE_GAP_MAX_GDX_RANGING_CH 20

The maximum GDX Ranging Channel.

Definition at line 84 of file ble_gapc.h.

## ◆ BLE_GAP_MAX_IQ_SAMPLE_NUM

#define BLE_GAP_MAX_IQ_SAMPLE_NUM 0x52

The maximum IQ sample number.

Definition at line 82 of file ble_gapc.h.

## ◆ BLE_GAP_MIN_CTE_CNT

#define BLE_GAP_MIN_CTE_CNT 0x01

CTE count.

The minimum CTE count.

Definition at line 78 of file ble_gapc.h.

## ◆ BLE_GAP_MIN_CTE_LEN

#define BLE_GAP_MIN_CTE_LEN 0x02

CTE length (in number of 8us periods)

The minimum CTE length.

Definition at line 74 of file ble_gapc.h.

## ◆ BLE_GAP_MIN_IQ_SAMPLE_NUM

#define BLE_GAP_MIN_IQ_SAMPLE_NUM 0x09

The minimum IQ sample number.

Definition at line 81 of file ble_gapc.h.