### - i -

- I2C_ADDRESSINGMODE_10BIT : gr533x_hal_i2c.h
- I2C_ADDRESSINGMODE_7BIT : gr533x_hal_i2c.h
- I2C_DEFAULT_CONFIG : gr533x_hal_i2c.h
- I2C_FIRST_AND_LAST_FRAME : gr533x_hal_i2c.h
- I2C_FIRST_AND_NEXT_FRAME : gr533x_hal_i2c.h
- I2C_FIRST_FRAME : gr533x_hal_i2c.h
- I2C_GENERALCALL_DISABLE : gr533x_hal_i2c.h
- I2C_GENERALCALL_ENABLE : gr533x_hal_i2c.h
- I2C_LAST_FRAME : gr533x_hal_i2c.h
- I2C_MEM_ADD_LSB : gr533x_hal_i2c.h
- I2C_MEM_ADD_MSB : gr533x_hal_i2c.h
- I2C_MEMADD_SIZE_16BIT : gr533x_hal_i2c.h
- I2C_MEMADD_SIZE_8BIT : gr533x_hal_i2c.h
- I2C_NEXT_FRAME : gr533x_hal_i2c.h
- I2C_SPEED_1000K : gr533x_hal_i2c.h
- I2C_SPEED_100K : gr533x_hal_i2c.h
- I2C_SPEED_400K : gr533x_hal_i2c.h
- IAS_C_CONNECTION_MAX : ias_c.h
- INDI_PAYLOAD_HEADER_LEN : bcs.h
- IS_ADC_CLOCK : gr533x_hal_adc.h
- IS_ADC_INPUT : gr533x_hal_adc.h
- IS_ADC_INPUT_MODE : gr533x_hal_adc.h
- IS_ADC_REF : gr533x_hal_adc.h
- IS_ADC_REF_VALUE : gr533x_hal_adc.h
- IS_AON_GPIO_MODE : gr533x_hal_aon_gpio.h
- IS_AON_GPIO_PIN : gr533x_hal_aon_gpio.h
- IS_AON_GPIO_PIN_ACTION : gr533x_hal_aon_gpio.h
- IS_AON_GPIO_PULL : gr533x_hal_aon_gpio.h
- IS_CALENDAR_ALARM_TYPE : gr533x_hal_calendar.h
- IS_CALENDAR_DATE : gr533x_hal_calendar.h
- IS_CALENDAR_LEAP_YEAR : gr533x_hal_calendar.h
- IS_CALENDAR_WEEKDAY : gr533x_hal_calendar.h
- IS_COMP_HYST_NEG : gr533x_hal_comp.h
- IS_COMP_HYST_POS : gr533x_hal_comp.h
- IS_COMP_INPUT : gr533x_hal_comp.h
- IS_COMP_REF : gr533x_hal_comp.h
- IS_COMP_RES_DEGENERATION_NEG : gr533x_hal_comp.h
- IS_COMP_RES_DEGENERATION_POS : gr533x_hal_comp.h
- IS_DMA_ALL_INSTANCE : gr533x_hal_dma.h
- IS_DMA_ALL_P_INSTANCE : gr533x_hal_dma.h
- IS_DMA_ALL_REQUEST : gr533x_hal_dma.h
- IS_DMA_BUFFER_SIZE : gr533x_hal_dma.h
- IS_DMA_DESTINATION_DATA_SIZE : gr533x_hal_dma.h
- IS_DMA_DESTINATION_INC_STATE : gr533x_hal_dma.h
- IS_DMA_DIRECTION : gr533x_hal_dma.h
- IS_DMA_PRIORITY : gr533x_hal_dma.h
- IS_DMA_SOURCE_DATA_SIZE : gr533x_hal_dma.h
- IS_DMA_SOURCE_INC_STATE : gr533x_hal_dma.h
- IS_DUAL_TIMER_COUNTERMODE : gr533x_hal_dual_tim.h
- IS_DUAL_TIMER_IO_ACT_MODE : gr533x_hal_dual_tim.h
- IS_DUAL_TIMER_IO_INIT_STATE : gr533x_hal_dual_tim.h
- IS_DUAL_TIMER_PRESCALER : gr533x_hal_dual_tim.h
- IS_GPIO_MODE : gr533x_hal_gpio.h
- IS_GPIO_PIN : gr533x_hal_gpio.h
- IS_GPIO_PIN_ACTION : gr533x_hal_gpio.h
- IS_GPIO_PULL : gr533x_hal_gpio.h
- IS_I2C_ADDRESSING_MODE : gr533x_hal_i2c.h
- IS_I2C_GENERAL_CALL : gr533x_hal_i2c.h
- IS_I2C_MEMADD_SIZE : gr533x_hal_i2c.h
- IS_I2C_OWN_ADDRESS : gr533x_hal_i2c.h
- IS_I2C_SLV_ADDRESS : gr533x_hal_i2c.h
- IS_I2C_SPEED : gr533x_hal_i2c.h
- IS_I2C_TRANSFER_OPTIONS_REQUEST : gr533x_hal_i2c.h
- IS_MSIO_DIRECTION : gr533x_hal_msio.h
- IS_MSIO_MODE : gr533x_hal_msio.h
- IS_MSIO_PIN : gr533x_hal_msio.h
- IS_MSIO_PIN_ACTION : gr533x_hal_msio.h
- IS_MSIO_PULL : gr533x_hal_msio.h
- IS_NVIC_DEVICE_IRQ : gr533x_hal_cortex.h
- IS_NVIC_PREEMPTION_PRIORITY : gr533x_hal_cortex.h
- IS_NVIC_PRIORITY_GROUP : gr533x_hal_cortex.h
- IS_NVIC_SUB_PRIORITY : gr533x_hal_cortex.h
- IS_PWM_ALIGNMENT_MODE : gr533x_hal_pwm.h
- IS_PWM_DRIVEPOLARITY : gr533x_hal_pwm.h
- IS_PWM_MODE : gr533x_hal_pwm.h
- IS_PWM_STOP_LVL : gr533x_hal_pwm.h
- IS_PWM_WAITING_TIME_LVL : gr533x_hal_pwm.h
- IS_PWR_MEM_BLOCK : gr533x_hal_pwr.h
- IS_PWR_MEM_POWER_STAT : gr533x_hal_pwr.h
- IS_PWR_PWR_TIMER_TYPE : gr533x_hal_pwr.h
- IS_PWR_WAKEUP_CONDITION : gr533x_hal_pwr.h
- IS_SPI_BAUDRATE_PRESCALER : gr533x_hal_spi.h
- IS_SPI_CPHA : gr533x_hal_spi.h
- IS_SPI_CPOL : gr533x_hal_spi.h
- IS_SPI_DATASIZE : gr533x_hal_spi.h
- IS_SPI_DIRECTION : gr533x_hal_spi.h
- IS_SPI_FIFO_THRESHOLD : gr533x_hal_spi.h
- IS_SPI_RX_SAMPLE_DLY : gr533x_hal_spi.h
- IS_SPI_SLAVE : gr533x_hal_spi.h
- IS_SPI_TIMODE : gr533x_hal_spi.h
- IS_SYSTICK_CLK_SOURCE : gr533x_hal_cortex.h
- IS_TRANSFER_REQUEST : gr533x_hal_i2c.h
- IS_UART_BAUDRATE : gr533x_hal_uart.h
- IS_UART_DATABITS : gr533x_hal_uart.h
- IS_UART_HARDWARE_FLOW_CONTROL : gr533x_hal_uart.h
- IS_UART_PARITY : gr533x_hal_uart.h
- IS_UART_STOPBITS : gr533x_hal_uart.h
- IS_WDT_RESET_MODE : gr533x_hal_wdt.h
- IS_XQSPI_ADDRESS_SIZE : gr533x_hal_xqspi.h
- IS_XQSPI_BAUD_RATE : gr533x_hal_xqspi.h
- IS_XQSPI_CACHE_FLUSH : gr533x_hal_xqspi.h
- IS_XQSPI_CACHE_MAPPING : gr533x_hal_xqspi.h
- IS_XQSPI_CACHE_MODE : gr533x_hal_xqspi.h
- IS_XQSPI_CLOCK_MODE : gr533x_hal_xqspi.h
- IS_XQSPI_DATA_MODE : gr533x_hal_xqspi.h
- IS_XQSPI_FIFO_THRESHOLD : gr533x_hal_xqspi.h
- IS_XQSPI_INSTADDR_MODE : gr533x_hal_xqspi.h
- IS_XQSPI_INSTRUCTION_SIZE : gr533x_hal_xqspi.h
- IS_XQSPI_READ_CMD : gr533x_hal_xqspi.h
- IS_XQSPI_WORK_MODE : gr533x_hal_xqspi.h
- ISO_ADDR_LEN : ble_iso.h
- ISO_SYNC0_PULSE : ble_iso.h
- ISO_SYNC1_PULSE : ble_iso.h