Macros
SPI Interrupt Definition
Peripheral Driver » HAL Driver » SPI » CS Signal Description » Defines » SPI Exported Constants

## Macros
#define | SPI_IT_MST LL_SPI_IS_MST
#define | SPI_IT_RXF LL_SPI_IS_RXF
#define | SPI_IT_RXO LL_SPI_IS_RXO
#define | SPI_IT_RXU LL_SPI_IS_RXU
#define | SPI_IT_TXO LL_SPI_IS_TXO
#define | SPI_IT_TXE LL_SPI_IS_TXE

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_IT_MST

#define SPI_IT_MST LL_SPI_IS_MST

Multi-Master Contention Interrupt flag

Definition at line 392 of file gr533x_hal_spi.h.

## ◆ SPI_IT_RXF

#define SPI_IT_RXF LL_SPI_IS_RXF

Receive FIFO Full Interrupt flag

Definition at line 393 of file gr533x_hal_spi.h.

## ◆ SPI_IT_RXO

#define SPI_IT_RXO LL_SPI_IS_RXO

Receive FIFO Overflow Interrupt flag

Definition at line 394 of file gr533x_hal_spi.h.

## ◆ SPI_IT_RXU

#define SPI_IT_RXU LL_SPI_IS_RXU

Receive FIFO Underflow Interrupt flag

Definition at line 395 of file gr533x_hal_spi.h.

## ◆ SPI_IT_TXE

#define SPI_IT_TXE LL_SPI_IS_TXE

Transmit FIFO Empty Interrupt flag

Definition at line 397 of file gr533x_hal_spi.h.

## ◆ SPI_IT_TXO

#define SPI_IT_TXO LL_SPI_IS_TXO

Transmit FIFO Overflow Interrupt flag

Definition at line 396 of file gr533x_hal_spi.h.