Macros
Defines
BLE Services » HRS RSCS Relay Control Point Service (HRRCPS)

## Macros
#define | HRRCPS_CONNECTION_MAX 10
#define | HRRCPS_CTRL_PT_VAL_LEN 2
#define | HRRCPS_CTRL_PT_RSP_VAL_LEN 4
#define | HRRCPS_SERVICE_UUID

## Detailed Description

## Macro Definition Documentation

## ◆ HRRCPS_CONNECTION_MAX

#define HRRCPS_CONNECTION_MAX 10

Maximum number of HRS RSCS Relay Control Point Service connections.

Definition at line 70 of file hrrcps.h.

## ◆ HRRCPS_CTRL_PT_RSP_VAL_LEN

#define HRRCPS_CTRL_PT_RSP_VAL_LEN 4

Length of the value of Control Point Response characteristic.

Definition at line 72 of file hrrcps.h.

## ◆ HRRCPS_CTRL_PT_VAL_LEN

#define HRRCPS_CTRL_PT_VAL_LEN 2

Length of the value of Control Point characteristic.

Definition at line 71 of file hrrcps.h.

## ◆ HRRCPS_SERVICE_UUID

#define HRRCPS_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x06, 0xED, 0xA6

The UUID of HRS RSCS Relay Control Point Service for setting advertising data.

Definition at line 74 of file hrrcps.h.