Public Attributes | List of all members
ieee_float32_t Struct Reference
BLE Services » Health Thermometer Service (HTS) » Structures

SFLOAT format (IEEE-11073 32-bit FLOAT, defined as a 32-bit vlue with 24-bit mantissa and 8-bit exponent. More...

`#include <hts.h>`

## Public Attributes
int8_t | exponent
int32_t | mantissa

## Detailed Description

SFLOAT format (IEEE-11073 32-bit FLOAT, defined as a 32-bit vlue with 24-bit mantissa and 8-bit exponent.

Definition at line 187 of file hts.h.

## Member Data Documentation

## ◆ exponent

int8_t ieee_float32_t::exponent

Base 10 exponent, only 8 bits

Definition at line 189 of file hts.h.

## ◆ mantissa

int32_t ieee_float32_t::mantissa

Mantissa, only 24 bits

Definition at line 190 of file hts.h.

The documentation for this struct was generated from the following file:

- hts.h