### - t -

- temp : __attribute__
- temp_convert_value : hts_meas_val_t
- temp_meas_type : hts_meas_val_t
- temp_original_value : hts_meas_val_t
- temp_ref : __attribute__
- temp_type : hts_init_t , hts_meas_val_t
- temperature_units : hts_init_t
- test_role : thscps_evt_t
- tester_and_health : gls_meas_ctx_t
- ths_mode : thscps_test_conn_info_t
- ths_rx_handle : ths_c_handles_t
- ths_setting_cccd_handle : ths_c_handles_t
- ths_setting_handle : ths_c_handles_t
- ths_srvc_end_handle : ths_c_handles_t
- ths_srvc_start_handle : ths_c_handles_t
- ths_toggle_handle : ths_c_handles_t
- ths_tx_cccd_handle : ths_c_handles_t
- ths_tx_handle : ths_c_handles_t
- ti_mode : _spi_init
- tick : _rtc_handle_t
- tim_env : app_tim_params_t
- tim_state : tim_env_t
- time : gls_racp_filter_t
- time_offset : gls_meas_val_t , iso_read_iso_tx_sync_cmpl_evt_t
- time_stamp : bcs_meas_val_t , bps_meas_t , hts_meas_val_t , iso_hci_data_t , wss_meas_val_t
- time_stamp_present : bcs_meas_flag_t , bps_meas_t , hts_init_t , wss_init_t
- time_stap : iso_read_iso_tx_sync_cmpl_evt_t
- time_zone : cts_c_loc_time_info_t , cts_loc_time_info_t
- timeout : _spi_handle , ble_gap_scan_param_t , iso_disc_ann_t
- timer_msp_deinit : _hal_timer_base_callback
- timer_msp_init : _hal_timer_base_callback
- timer_period_elapsed_callback : _hal_timer_base_callback
- tk : ble_sec_cfm_enc_data_t
- tk_type : ble_sec_enc_req_data_t
- total_distance : rscs_c_meas_val_t , rscs_meas_val_t
- total_distance_present : rscs_c_meas_val_t , rscs_meas_val_t
- total_length : ags_stream_env_t
- total_trxn_length : ags_header_first_ext_t , ags_header_first_t
- tps_srvc_end_handle : tps_c_handles_t
- tps_srvc_start_handle : tps_c_handles_t
- tps_tx_power_level_handle : tps_c_handles_t
- tran_latency : iso_create_big_t
- tran_latency_m2s : iso_cis_est_evt_t
- tran_latency_s2m : iso_cis_est_evt_t
- trans_latency_m2s : iso_set_cig_param_t
- trans_latency_s2m : iso_set_cig_param_t
- transfer_direction : _ll_spim_init_t
- transport_mode : ths_init_t
- trigger : _ll_gpio_init
- trigger_offset : iso_set_data_path_trigger_t
- trx_mode : gdx_lcp_config_t
- trx_timer_period_us : gdx_lcp_config_t
- trx_timer_trigger_trx_time_us : gdx_lcp_config_t
- trxn_id : ags_header_base_t , ags_stream_env_t
- trxn_type : ags_header_base_t
- twext : ble_slp_config_t
- twosc : ble_slp_config_t
- twrm : ble_slp_config_t
- tx : app_uart_pin_cfg_t
- tx_abort_flag : uart_env_t
- tx_buf : app_uart_tx_buf_t
- tx_buf_size : app_uart_tx_buf_t
- tx_dma_channel : app_i2c_dma_cfg_t , app_spi_dma_cfg_t , app_uart_dma_cfg_t
- tx_dma_instance : app_i2c_dma_cfg_t , app_spi_dma_cfg_t , app_uart_dma_cfg_t
- tx_done : spi_env_t
- tx_done_cb : gdx_lcp_config_t
- tx_hold_time : _i2c_init
- tx_path_comp : ble_gap_dev_rf_path_comp_ind_t
- tx_phy : ble_gap_evt_phy_update_t , ble_gap_le_phy_ind_t , thscps_test_conn_info_t
- tx_power : __attribute__ , rf_trim_info_t , thscps_adv_param_t , thscps_test_conn_info_t
- tx_power_level : tps_c_evt_t
- tx_pwr : ble_gap_evt_adv_report_t , ble_gap_evt_remote_tx_pwr_read_ind_t , ble_gap_evt_tx_pwr_change_report_t , ble_gap_ext_adv_report_ind_t , ble_gap_remote_tx_pwr_read_ind_t , ble_gap_tx_pwr_change_report_t
- tx_pwr_change_report : ble_gapc_evt_t
- tx_ring_buffer : uart_env_t
- tx_send_buf : uart_env_t
- tx_state : _uart_handle
- tx_xfer_count : _spi_handle , _uart_handle , _xqspi_handle_t
- tx_xfer_size : _spi_handle , _uart_handle , _xqspi_handle_t
- txpwr_dbm : gdx_lcp_config_t
- type : app_adc_evt_t , app_adc_pin_t , app_bod_evt_t , app_comp_pin_t , app_gpiote_param_t , app_i2c_evt_t , app_i2c_pin_t , app_io_evt_t , app_pwm_pin_t , app_rng_evt_t , app_rtc_evt_t , app_spi_evt_t , app_spi_pin_t , app_uart_evt_t , app_uart_pin_t , ble_gap_evt_rslv_addr_report_t , ble_gap_ext_adv_param_t , ble_gap_ext_init_param_t , ble_gap_ext_scan_param_t , ble_gap_init_param_t , ble_gap_per_sync_param_t , ble_gattc_evt_ntf_ind_t , ble_gattc_ntf_ind_t , ble_gatts_evt_ntf_ind_t , ble_gatts_noti_ind_t , ble_gatts_ntf_ind_t , gls_meas_val_t