Public Attributes | List of all members
iso_per_adv_sync_tran_rcv_evt_t Struct Reference
BLE » Core Isochronous Channels | BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

The parameter for receiving periodic advertising Synchronization transport event. More...

`#include <ble_iso.h>`

## Public Attributes
uint8_t | status
uint16_t | conn_hdl
uint16_t | service_data
uint8_t | adv_sid
uint16_t | sync_hdl

## Detailed Description

The parameter for receiving periodic advertising Synchronization transport event.

Definition at line 565 of file ble_iso.h.

## Member Data Documentation

## ◆ adv_sid

uint8_t iso_per_adv_sync_tran_rcv_evt_t::adv_sid

Value of the Advertising SID used to advertise the periodic advertising.

Definition at line 570 of file ble_iso.h.

## ◆ conn_hdl

uint16_t iso_per_adv_sync_tran_rcv_evt_t::conn_hdl

Connection_Handle, (Range: 0x0000 to 0x0EFF).

Definition at line 568 of file ble_iso.h.

## ◆ service_data

uint16_t iso_per_adv_sync_tran_rcv_evt_t::service_data

A value provided by the peer device.

Definition at line 569 of file ble_iso.h.

## ◆ status

uint8_t iso_per_adv_sync_tran_rcv_evt_t::status

0x00: Synchronization to the periodic advertising succeeded, 0x01 to 0xFF: Synchronization to the periodic advertising failed

Definition at line 567 of file ble_iso.h.

## ◆ sync_hdl

uint16_t iso_per_adv_sync_tran_rcv_evt_t::sync_hdl

Sync_Handle identifying the periodic advertising, (Range: 0x0000 to 0x0EFF).

Definition at line 571 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h