Public Attributes | List of all members
_ll_pwm_none_coding_channel_init_t Struct Reference
Peripheral Driver » LL Driver » PWM » Structures » PWM Exported init structures

LL PWM Output Channel init Structure definition. More...

`#include <gr533x_ll_pwm.h>`

## Public Attributes
uint8_t | duty
uint8_t | drive_polarity
uint32_t | flickerstop_lvl

## Detailed Description

LL PWM Output Channel init Structure definition.

Definition at line 91 of file gr533x_ll_pwm.h.

## Member Data Documentation

## ◆ drive_polarity

uint8_t _ll_pwm_none_coding_channel_init_t::drive_polarity

Specifies the drive polarity in PWM output mode. This parameter can be a value of PWM drive polarity.

This feature can be modified afterwards using unitary function ll_pwm_enable_positive_drive_channel_x() and ll_pwm_disable_positive_drive_channel_x() where X can be (A, B, C).

Definition at line 96 of file gr533x_ll_pwm.h.

## ◆ duty

uint8_t _ll_pwm_none_coding_channel_init_t::duty

Specifies the duty in PWM output mode. This parameter must be a number ranges between Min_Data=0 and Max_Data=100.

Definition at line 93 of file gr533x_ll_pwm.h.

## ◆ flickerstop_lvl

uint32_t _ll_pwm_none_coding_channel_init_t::flickerstop_lvl

Specifies the IO level when channel flicker stop. This parameter can be a value of PWM stop io level.

Definition at line 102 of file gr533x_ll_pwm.h.

The documentation for this struct was generated from the following file:

- gr533x_ll_pwm.h