Public Attributes | List of all members
iso_read_iso_tx_sync_cmpl_evt_t Struct Reference
BLE » Core Isochronous Channels | BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

The parameter for read iso tx sync complete event. More...

`#include <ble_iso.h>`

## Public Attributes
uint8_t | status
uint16_t | con_hdl
uint16_t | pkt_seq_num
uint32_t | time_stap
uint32_t | time_offset

## Detailed Description

The parameter for read iso tx sync complete event.

Definition at line 577 of file ble_iso.h.

## Member Data Documentation

## ◆ con_hdl

uint16_t iso_read_iso_tx_sync_cmpl_evt_t::con_hdl

Connection handle of the bis or cis, (Range: 0x0000 to 0x0EFF).

Definition at line 580 of file ble_iso.h.

## ◆ pkt_seq_num

uint16_t iso_read_iso_tx_sync_cmpl_evt_t::pkt_seq_num

The packet sequence number of the ISO_SDU.

Definition at line 581 of file ble_iso.h.

## ◆ status

uint8_t iso_read_iso_tx_sync_cmpl_evt_t::status

0x00: succeeded. 0x01-0xFF: failed

Definition at line 579 of file ble_iso.h.

## ◆ time_offset

uint32_t iso_read_iso_tx_sync_cmpl_evt_t::time_offset

The time offset associated with the ISO_SDU identified by the seq_num, (Range: 0x000000 to 0xFFFFFF)

Definition at line 583 of file ble_iso.h.

## ◆ time_stap

uint32_t iso_read_iso_tx_sync_cmpl_evt_t::time_stap

The timestamp of an SDU identified by the seq_num, (Range: 0x00000000 to 0xFFFFFFFF)

Definition at line 582 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h