Public Attributes | List of all members
ble_gap_antenna_inf_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

antenna information. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | supp_switching_sampl_rates
uint8_t | antennae_num
uint8_t | max_switching_pattern_len
uint8_t | max_cte_len

## Detailed Description

antenna information.

Definition at line 371 of file ble_gapc.h.

## Member Data Documentation

## ◆ antennae_num

uint8_t ble_gap_antenna_inf_t::antennae_num

Number of antennae, range 0x01 to 0x4B.

Definition at line 374 of file ble_gapc.h.

## ◆ max_cte_len

uint8_t ble_gap_antenna_inf_t::max_cte_len

Max CTE length, range 0x02 to 0x14.

Definition at line 376 of file ble_gapc.h.

## ◆ max_switching_pattern_len

uint8_t ble_gap_antenna_inf_t::max_switching_pattern_len

Max length of switching pattern (number of antenna IDs in the pattern), range 0x02 to 0x4B.

Definition at line 375 of file ble_gapc.h.

## ◆ supp_switching_sampl_rates

uint8_t ble_gap_antenna_inf_t::supp_switching_sampl_rates

Supported switching sampling rates bit field (

See also
  enum gap_switch_sampling_rate).

Definition at line 373 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h