Public Attributes | List of all members
cts_updata_ref_time_info_t Struct Reference
BLE Services » Current Time Service (CTS) » Structures

CTS Reference Time Updata Information. More...

`#include <cts.h>`

## Public Attributes
uint8_t | before_updata_sec
uint8_t | current_time_min
uint8_t | current_time_sec
uint8_t | expected_time_1min_adapt
cts_ref_time_source_t | stage_update_source
uint8_t | updata_time_flag

## Detailed Description

CTS Reference Time Updata Information.

Definition at line 195 of file cts.h.

## Member Data Documentation

## ◆ before_updata_sec

uint8_t cts_updata_ref_time_info_t::before_updata_sec

The second before the update.

Definition at line 197 of file cts.h.

## ◆ current_time_min

uint8_t cts_updata_ref_time_info_t::current_time_min

Minutes of the current time.

Definition at line 198 of file cts.h.

## ◆ current_time_sec

uint8_t cts_updata_ref_time_info_t::current_time_sec

The second of the current time.

Definition at line 199 of file cts.h.

## ◆ expected_time_1min_adapt

uint8_t cts_updata_ref_time_info_t::expected_time_1min_adapt

Minutes of the expected update time.

Definition at line 200 of file cts.h.

## ◆ stage_update_source

cts_ref_time_source_t cts_updata_ref_time_info_t::stage_update_source

Minutes of the expected update time.

Definition at line 201 of file cts.h.

## ◆ updata_time_flag

uint8_t cts_updata_ref_time_info_t::updata_time_flag

1 minute time flag bit.

Definition at line 202 of file cts.h.

The documentation for this struct was generated from the following file:

- cts.h