Functions
Functions
BLE Services » Device Information Service Client (DIS_C)

## Functions
sdk_err_t | dis_client_init (dis_c_evt_handler_t evt_handler)
| Register DIS Client event handler. More...
sdk_err_t | dis_c_disc_srvc_start (uint8_t conn_idx)
| Discovery Device Information Service on peer. More...
sdk_err_t | dis_c_char_value_read (uint8_t conn_idx, dis_c_char_type_t char_read_type)
| Read Device Information Service characteristic value. More...

## Detailed Description

## Function Documentation

## ◆ dis_c_char_value_read()

sdk_err_t dis_c_char_value_read | ( | uint8_t | conn_idx,
|  | dis_c_char_type_t | char_read_type
| ) |  |

Read Device Information Service characteristic value.

Parameters

  [in] | conn_idx | Index of connection.
  [in] | char_read_type | Type of characteristic read.

Returns
  Operation result.

## ◆ dis_c_disc_srvc_start()

sdk_err_t dis_c_disc_srvc_start | ( | uint8_t | conn_idx | ) |

Discovery Device Information Service on peer.

Parameters

  [in] | conn_idx | Index of connection.

Returns
  Operation result.

## ◆ dis_client_init()

sdk_err_t dis_client_init | ( | dis_c_evt_handler_t | evt_handler | ) |

Register DIS Client event handler.

Parameters

  [in] | evt_handler | Device Information Service Client event handler.

Returns
  Result of initialization.