Enumerations
HAL EFUSE state
Peripheral Driver » HAL Driver » EFUSE » Enumerations

## Enumerations
enum | hal_efuse_state_t { HAL_EFUSE_STATE_RESET = 0x00, HAL_EFUSE_STATE_READY = 0x01, HAL_EFUSE_STATE_BUSY = 0x02, HAL_EFUSE_STATE_ERROR = 0x04 }
| HAL eFuse State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_efuse_state_t

enum hal_efuse_state_t

HAL eFuse State Enumerations definition.

Enumerator
HAL_EFUSE_STATE_RESET | Peripheral not yet initialized or disabled
HAL_EFUSE_STATE_READY | Peripheral Initialized and ready for use
HAL_EFUSE_STATE_BUSY | An internal process is ongoing
HAL_EFUSE_STATE_ERROR | Reception process is error

Definition at line 75 of file gr533x_hal_efuse.h.