Modules | Macros
Defines
BLE Services » Heart Rate Service (HRS)

## Modules
| Characteristics Mask
| Bit masks for the initialization of hrs_init_t::char_mask.

## Macros
#define | HRS_CONNECTION_MAX 10
#define | HRS_MEAS_MAX_LEN 20
#define | HRS_MAX_BUFFERED_RR_INTERVALS 9

## Detailed Description

## Macro Definition Documentation

## ◆ HRS_CONNECTION_MAX

#define HRS_CONNECTION_MAX 10

Maximum number of Heart Rate Service connections.

Definition at line 81 of file hrs.h.

## ◆ HRS_MAX_BUFFERED_RR_INTERVALS

#define HRS_MAX_BUFFERED_RR_INTERVALS 9

Size of RR Interval buffer inside service.

Definition at line 83 of file hrs.h.

## ◆ HRS_MEAS_MAX_LEN

#define HRS_MEAS_MAX_LEN 20

Maximum length of heart rate measurement characteristic.

Definition at line 82 of file hrs.h.