Public Attributes | List of all members
iso_start_bd_ann_t Struct Reference
BLE » Core Isochronous Channels | BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

The parameter for starting broadcast announcement. More...

`#include <ble_iso.h>`

## Public Attributes
uint8_t | adv_idx
uint8_t | sid
uint16_t | interval
uint16_t | data_len
uint8_t * | data

## Detailed Description

The parameter for starting broadcast announcement.

Definition at line 205 of file ble_iso.h.

## Member Data Documentation

## ◆ adv_idx

uint8_t iso_start_bd_ann_t::adv_idx

Adv index, (Range: 0 to 4).

Definition at line 207 of file ble_iso.h.

## ◆ data

uint8_t* iso_start_bd_ann_t::data

Broadcast audio announcement data.

Definition at line 211 of file ble_iso.h.

## ◆ data_len

uint16_t iso_start_bd_ann_t::data_len

Broadcast audio announcement data length.

Definition at line 210 of file ble_iso.h.

## ◆ interval

uint16_t iso_start_bd_ann_t::interval

Adv interval, (Range: 0x0006 to 0xFFFF), Time = N * 1.25 ms,Time Range: 7.5ms to 81.91875 s.

Definition at line 209 of file ble_iso.h.

## ◆ sid

uint8_t iso_start_bd_ann_t::sid

Adv set ID, (Range: 0x00 to 0xFF).

Definition at line 208 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h