Public Attributes | List of all members
_dma_lock_config Struct Reference
Peripheral Driver » HAL Driver » DMA » Structures

DMA LOCK Structure definition. More...

`#include <gr533x_hal_dma.h>`

## Public Attributes
uint32_t | channel_lock_en
uint32_t | channel_lock_level
uint32_t | bus_lock_en
uint32_t | bus_lock_level

## Detailed Description

DMA LOCK Structure definition.

Definition at line 131 of file gr533x_hal_dma.h.

## Member Data Documentation

## ◆ bus_lock_en

uint32_t _dma_lock_config::bus_lock_en

Specifies the dma bus lock enable. This parameter can be a value of DMA Channel Lock Enable

Definition at line 139 of file gr533x_hal_dma.h.

## ◆ bus_lock_level

uint32_t _dma_lock_config::bus_lock_level

Specifies the dma bus lock level. This parameter can be a value of DMA Bus Lock Level

Definition at line 142 of file gr533x_hal_dma.h.

## ◆ channel_lock_en

uint32_t _dma_lock_config::channel_lock_en

Specifies the dma channel lock enable. This parameter can be a value of DMA Channel Lock Enable

Definition at line 133 of file gr533x_hal_dma.h.

## ◆ channel_lock_level

uint32_t _dma_lock_config::channel_lock_level

Specifies the dma channel lock level. This parameter can be a value of DMA Channel Lock Level

Definition at line 136 of file gr533x_hal_dma.h.

The documentation for this struct was generated from the following file:

- gr533x_hal_dma.h