Macros
Defines
BLE Services » Throughput Control Point Client (THSCPS)

## Macros
#define | THSCPS_CONNECTION_MAX 10
#define | THSCPS_CTRL_PT_VAL_LEN 20
#define | THSCPS_TEST_SETTING_VAL_LEN 20
#define | THSCPS_TEST_INFO_VAL_LEN 20
#define | THSCPS_CONN_INFO_VAL_LEN 20
#define | THSCPS_SERVICE_UUID
#define | THSCPS_ACTION_ON 0x01
#define | THSCPS_ACTION_OFF 0x00
#define | THSCPS_CTRL_PT_RSP_CODE 0xff

## Detailed Description

## Macro Definition Documentation

## ◆ THSCPS_ACTION_OFF

#define THSCPS_ACTION_OFF 0x00

Stop the action.

Definition at line 76 of file thscps.h.

## ◆ THSCPS_ACTION_ON

#define THSCPS_ACTION_ON 0x01

Start the action.

Definition at line 75 of file thscps.h.

## ◆ THSCPS_CONN_INFO_VAL_LEN

#define THSCPS_CONN_INFO_VAL_LEN 20

Length of the value of Connection Information characteristic.

Definition at line 72 of file thscps.h.

## ◆ THSCPS_CONNECTION_MAX

#define THSCPS_CONNECTION_MAX 10

Maximum number of THSCPS connections.

Definition at line 68 of file thscps.h.

## ◆ THSCPS_CTRL_PT_RSP_CODE

#define THSCPS_CTRL_PT_RSP_CODE 0xff

Response code.

Definition at line 77 of file thscps.h.

## ◆ THSCPS_CTRL_PT_VAL_LEN

#define THSCPS_CTRL_PT_VAL_LEN 20

Length of the value of Control Point characteristic.

Definition at line 69 of file thscps.h.

## ◆ THSCPS_SERVICE_UUID

#define THSCPS_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x07, 0xED, 0xA6

The UUID of THS Control Point Control Point Service for setting advertising data.

Definition at line 74 of file thscps.h.

## ◆ THSCPS_TEST_INFO_VAL_LEN

#define THSCPS_TEST_INFO_VAL_LEN 20

Length of the value of Test Information characteristic.

Definition at line 71 of file thscps.h.

## ◆ THSCPS_TEST_SETTING_VAL_LEN

#define THSCPS_TEST_SETTING_VAL_LEN 20

Length of the value of Test Setting characteristic.

Definition at line 70 of file thscps.h.