Public Attributes | List of all members
ble_gap_per_sync_trans_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Default periodic advertising synchronization transfer parameters. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | mode
uint16_t | skip
uint16_t | sync_to
uint8_t | cte_type

## Detailed Description

Default periodic advertising synchronization transfer parameters.

Definition at line 642 of file ble_gapc.h.

## Member Data Documentation

## ◆ cte_type

uint8_t ble_gap_per_sync_trans_param_t::cte_type

Type of Constant Tone Extension device should sync on (

See also
  enum gap_sync_cte_type).

Definition at line 648 of file ble_gapc.h.

## ◆ mode

uint8_t ble_gap_per_sync_trans_param_t::mode

See also
  gap_per_adv_sync_info_rec_mode.

Definition at line 644 of file ble_gapc.h.

## ◆ skip

uint16_t ble_gap_per_sync_trans_param_t::skip

Number of periodic advertising that can be skipped after a successful receive. Maximum authorized value is 499.

Definition at line 645 of file ble_gapc.h.

## ◆ sync_to

uint16_t ble_gap_per_sync_trans_param_t::sync_to

Synchronization timeout for the periodic advertising (in unit of 10 ms between 100 ms and 163.84s).

Definition at line 647 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h