Macros
DUAL_TIM prescaler
Peripheral Driver » LL Driver » DUAL_TIMER » Defines » DUAL_TIM Exported Constants

## Macros
#define | LL_DUAL_TIMER_PRESCALER_DIV0 0x00000000U
#define | LL_DUAL_TIMER_PRESCALER_DIV16 (1UL << DUAL_TIMER_CTRL_PRE_Pos)
#define | LL_DUAL_TIMER_PRESCALER_DIV256 (2UL << DUAL_TIMER_CTRL_PRE_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DUAL_TIMER_PRESCALER_DIV0

#define LL_DUAL_TIMER_PRESCALER_DIV0 0x00000000U

0 stage of prescale, clock is divided by 1.

Definition at line 125 of file gr533x_ll_dual_tim.h.

## ◆ LL_DUAL_TIMER_PRESCALER_DIV16

#define LL_DUAL_TIMER_PRESCALER_DIV16 (1UL << DUAL_TIMER_CTRL_PRE_Pos)

4 stages of prescale, clock is divided by 16.

Definition at line 126 of file gr533x_ll_dual_tim.h.

## ◆ LL_DUAL_TIMER_PRESCALER_DIV256

#define LL_DUAL_TIMER_PRESCALER_DIV256 (2UL << DUAL_TIMER_CTRL_PRE_Pos)

8 stages of prescale, clock is divided by 256.

Definition at line 127 of file gr533x_ll_dual_tim.h.