Macros
Block1 Clock During WFI
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_WFI_AON_MCUSUB_HCLK MCU_SUB_WFI_AON_MCUSUB_HCLK
#define | LL_CGC_WFI_XF_XQSPI_HCLK MCU_SUB_WFI_XF_XQSPI_HCLK
#define | LL_CGC_WFI_SRAM_HCLK MCU_SUB_WFI_SRAM_HCLK
#define | LL_CGC_WFI_ALL_HCLK1 ((uint32_t)0x00000007U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_WFI_ALL_HCLK1

#define LL_CGC_WFI_ALL_HCLK1 ((uint32_t)0x00000007U)

All clock group 1

Definition at line 96 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_WFI_AON_MCUSUB_HCLK

#define LL_CGC_WFI_AON_MCUSUB_HCLK MCU_SUB_WFI_AON_MCUSUB_HCLK

Hclk for Always-on register

Definition at line 92 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_WFI_SRAM_HCLK

#define LL_CGC_WFI_SRAM_HCLK MCU_SUB_WFI_SRAM_HCLK

Hclk for SRAMs

Definition at line 94 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_WFI_XF_XQSPI_HCLK

#define LL_CGC_WFI_XF_XQSPI_HCLK MCU_SUB_WFI_XF_XQSPI_HCLK

Hclk for cache top

Definition at line 93 of file gr533x_ll_cgc.h.