Modules | Macros
XQSPI Cache direct map enable
Peripheral Driver » LL Driver » Defines » XQSPI Exported Constants

## Modules
| XQSPI Cache flush enable
| QSPI Present Bypass
| QSPI Flash write bits
| InitStrcut default configuartion

## Macros
#define | LL_XQSPI_CACHE_DIRECT_MAP_DIS 0
#define | LL_XQSPI_CACHE_DIRECT_MAP_EN 1

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_CACHE_DIRECT_MAP_DIS

#define LL_XQSPI_CACHE_DIRECT_MAP_DIS 0

Cache work on 4-Way Set Associative

Definition at line 320 of file gr533x_ll_xqspi.h.

## ◆ LL_XQSPI_CACHE_DIRECT_MAP_EN

#define LL_XQSPI_CACHE_DIRECT_MAP_EN 1

Cache work on Direct Map

Definition at line 321 of file gr533x_ll_xqspi.h.