### - s -

- sadc : __attribute__
- sample_location : gls_meas_val_t
- sampling_enable : ble_gap_set_conn_cte_rcv_param_t
- sca : iso_req_peer_sca_cmpl_evt_t , iso_set_cig_param_t
- scan_dup_filt : ble_gap_scan_param_t
- scan_intv : ble_gap_scan_wd_op_param_t
- scan_mode : ble_gap_scan_param_t
- scan_param_1m : ble_gap_ext_init_param_t , ble_gap_ext_scan_param_t
- scan_param_coded : ble_gap_ext_init_param_t , ble_gap_ext_scan_param_t
- scan_req : ble_gapm_evt_t
- scan_req_ind_en : ble_gap_adv_param_t
- scan_stop : ble_gapm_evt_t
- scan_type : ble_gap_scan_param_t
- scan_wd : ble_gap_scan_wd_op_param_t
- scl : app_i2c_pin_cfg_t
- sda : app_i2c_pin_cfg_t
- sdu : iso_hci_data_t
- sdu_int_m2s : iso_set_cig_param_t
- sdu_int_s2m : iso_set_cig_param_t
- sdu_interval : iso_big_info_report_evt_t , iso_create_big_t
- sdu_len : iso_hci_data_t
- sdu_recv : ble_l2cap_evt_t
- sdu_send : ble_l2cap_evt_t
- sdu_size_m2s : iso_cis_param_t
- sdu_size_s2m : iso_cis_param_t
- sec : _calendar_time , prf_date_time_t
- sec_evt : ble_evt_t
- sec_lvl : ble_gap_lepsm_register_t
- second_cfg : ble_gap_ext_adv_param_t
- seed : _ll_rng_init
- seed_mode : _rng_init
- segm_num : uds_regi_user_data_stream_t
- segm_offset : uds_regi_user_data_stream_t
- sensor_loc : hrs_c_evt_t , hrs_init_t
- sensor_location : cscs_init_t , rscs_init_t
- sensor_status_annunciation : gls_meas_val_t
- seq_num : gls_racp_filter_t , iso_hci_data_t
- sequ_num : ags_header_base_t
- sequence_number : gls_meas_val_t
- serial_num_str : dis_init_t
- serv_data : ble_gap_sync_established_ind_t
- serv_type : ble_gattc_browse_srvc_t , ble_gattc_evt_browse_srvc_t
- service_data : iso_per_adv_sync_tran_rcv_evt_t , iso_per_adv_sync_tran_t , iso_set_per_adv_set_info_tran_t
- services : ble_gattc_evt_srvc_disc_t , ble_gattc_srvc_disc_t
- setting_info : thscps_evt_t
- setting_type : ths_evt_t
- shdl : ble_gatts_create_db_t
- sid : iso_start_bd_ann_t , iso_sync_ann_t
- signature_algorithm : dfu_boot_info_t
- signed_write : ble_gattc_write_no_resp_t
- silent : ancs_ntf_flags_t
- single_tx : ble_gap_set_pref_slave_evt_dur_param_t
- size : app_i2c_evt_t , app_spi_evt_t , app_uart_evt_t
- skip : ble_gap_per_sync_param_t , ble_gap_per_sync_trans_param_t , iso_set_default_per_adv_sync_tran_param_t , iso_set_per_adv_sync_tran_param_t
- slave_addr : app_i2c_evt_t
- slave_latency : ble_gap_conn_param_t , ble_gap_conn_update_param_t , ble_gap_evt_conn_param_update_req_t , ble_gap_evt_conn_param_updated_t , ble_gap_evt_connected_t , ble_gap_init_param_t , gap_slv_pref_t
- slave_select : _ll_spim_init_t , _spi_init
- sleep_algo_dur : ble_slp_config_t
- sleep_enable : ble_slp_config_t
- slope_ext_1p0 : __attribute__ , adc_trim_info_t
- slope_int_0p8 : __attribute__ , adc_trim_info_t
- slope_int_1p2 : __attribute__ , adc_trim_info_t
- slope_int_1p6 : __attribute__ , adc_trim_info_t
- slope_int_2p0 : adc_trim_info_t
- slot_dur : ble_gap_conn_iq_report_t , ble_gap_connless_iq_report_t , ble_gap_connless_iq_sample_param_t , ble_gap_evt_conn_iq_report_t , ble_gap_evt_connless_iq_report_t
- slot_durations : ble_gap_set_conn_cte_rcv_param_t
- slv_dev_addr : i2c_env_t
- soft_cs_magic : _spi_handle
- soft_lean_mass : bcs_meas_val_t
- soft_lean_mass_present : bcs_meas_flag_t
- source : cts_c_ref_time_info_t , cts_ref_time_info_t
- speed : _aon_gpio_init , _gpio_init , _i2c_init , _ll_gpio_init , _ll_i2c_init , _msio_init
- spi_abort_cplt_callback : _hal_spi_callback
- spi_dma_state : spi_env_t
- spi_env : app_spi_params_t
- spi_error_callback : _hal_spi_callback
- spi_msp_deinit : _hal_spi_callback
- spi_msp_init : _hal_spi_callback
- spi_rx_cplt_callback : _hal_spi_callback
- spi_soft_cs_assert : _hal_spi_callback
- spi_soft_cs_deassert : _hal_spi_callback
- spi_state : spi_env_t
- spi_tx_cplt_callback : _hal_spi_callback
- spi_tx_rx_cplt_callback : _hal_spi_callback
- src_data_alignment : _dma_init
- src_increment : _dma_init
- src_request : _dma_init
- srvc_browse : ble_gattc_evt_t
- srvc_perm : ble_gatts_create_db_t
- stage_update_source : cts_updata_ref_time_info_t
- start_act_it : _dual_timer_io_ctrl_cfg
- start_act_mode : _dual_timer_io_ctrl_cfg
- start_flag : i2c_env_t , spi_env_t
- start_flush_flag : uart_env_t
- start_hdl : ble_gattc_browse_inc_srvc_t , ble_gattc_browse_srvc_t , ble_gattc_disc_char_t , ble_gattc_evt_browse_srvc_t , ble_gattc_include_t , ble_gattc_read_by_uuid_t , ble_gattc_service_t , ble_gatts_evt_inited_ind_t , gattc_prf_reg_peer_evt_t
- start_tx_flag : uart_env_t
- start_value : _rtc_init_t
- state : _adc_handle , _alarm_handle_t , _comp_handle , _dma_handle , _dual_timer_handle , _efuse_handle , _i2c_handle , _rng_handle , _rtc_handle_t , _spi_handle , _tick_handle_t , _timer_handle , _xqspi_handle_t , pwm_handle_t
- status : ble_gap_ranging_cmp_ind_t , ble_gap_ranging_ind_t , ble_gap_ranging_sample_report_ind_t , ble_gatts_prep_write_cfm_t , ble_gatts_read_cfm_t , ble_gatts_write_cfm_t , gls_racp_rsp_t , iso_big_create_sync_est_evt_t , iso_cis_est_evt_t , iso_create_big_cmpl_evt_t , iso_per_adv_sync_tran_rcv_evt_t , iso_read_iso_tx_sync_cmpl_evt_t , iso_req_peer_sca_cmpl_evt_t , iso_set_cig_param_cmpl_evt_t , prf_att_info_t , thscps_rsp_val_t
- stb_io_ldo_1P8 : __attribute__
- stb_io_ldo_3p0 : __attribute__
- step_calorie : wechat_pedo_meas_t
- step_count : wechat_pedo_meas_t , wechat_pedo_target_t
- step_count_target : wechat_init_t
- step_dist : wechat_pedo_meas_t
- stop_act_it : _dual_timer_io_ctrl_cfg
- stop_act_mode : _dual_timer_io_ctrl_cfg
- stop_bits : _ll_uart_init_t , _uart_init
- str_info : ans_c_new_alert_t , ans_new_alert_t
- stream_id : ags_header_base_t , ags_stream_env_t
- strength : _aon_gpio_init , _gpio_init , _ll_gpio_init , _msio_init
- string_data : ble_dis_c_read_rsp_t
- subrate_chg_ind : ble_gapc_evt_t
- subrate_factor : ble_gap_evt_subrate_chg_ind_t , ble_gap_subrate_chg_ind_t
- subrate_max : ble_gap_dft_subrate_param_t , ble_gap_subrate_req_t
- subrate_min : ble_gap_dft_subrate_param_t , ble_gap_subrate_req_t
- sugg_dflt_data_len : ble_gap_dev_info_t
- suggted_max_tx_octets : ble_gap_sugg_dflt_data_len_t
- suggted_max_tx_time : ble_gap_sugg_dflt_data_len_t
- sup_new_alert_cat : ans_init_t
- sup_new_alert_cat_ids : ans_c_evt_t
- sup_timeout : ble_gap_conn_param_t , ble_gap_conn_update_cmp_t , ble_gap_conn_update_param_t , ble_gap_evt_conn_param_update_req_t , ble_gap_evt_conn_param_updated_t , ble_gap_evt_connected_t , ble_gap_init_param_t
- sup_to : gap_conn_cmp_t
- sup_unread_alert_cat_ids : ans_c_evt_t
- sup_unread_alert_sta : ans_init_t
- superv_timeout : ble_gap_dft_subrate_param_t , ble_gap_subrate_req_t
- supervision_timeout : ble_gap_evt_subrate_chg_ind_t , ble_gap_subrate_chg_ind_t
- supervision_to : ble_gap_ext_conn_param_t
- supp_switching_sampl_rates : ble_gap_antenna_inf_t
- suppted_max_rx_octets : ble_gap_max_data_len_t
- suppted_max_rx_time : ble_gap_max_data_len_t
- suppted_max_tx_octets : ble_gap_max_data_len_t
- suppted_max_tx_time : ble_gap_max_data_len_t
- sw_rev_str : dis_init_t
- sync_cnt : dss_evt_t
- sync_dev_num : dss_evt_t
- sync_established : ble_gapm_evt_t
- sync_hdl : ble_gap_evt_sync_established_t , ble_gap_sync_established_ind_t , iso_per_adv_sync_tran_rcv_evt_t , iso_per_adv_sync_tran_t , iso_set_per_adv_rcv_enable_t
- sync_timeout : iso_set_default_per_adv_sync_tran_param_t , iso_set_per_adv_sync_tran_param_t , iso_sync_ann_t
- sync_to : ble_gap_per_sync_param_t , ble_gap_per_sync_trans_param_t
- sys_id : ble_dis_c_read_rsp_t
- sys_ldo_1p05 : __attribute__ , pmu_trim_info_t
- sys_ldo_1p15 : __attribute__ , pmu_trim_info_t
- system_clk : dfu_boot_info_t
- SystemCoreLowClock : _aon_wdt_handle
- systick_callback : _hal_callback
- systolic : bps_meas_t