Macros
Defines
BLE » Core Isochronous Channels

## Macros
#define | ISO_ADDR_LEN 6
#define | ENC_CODE_LEN 16
#define | ISO_SYNC0_PULSE (0x1 << 0)
#define | ISO_SYNC1_PULSE (0x1 << 1)

## Detailed Description

## Macro Definition Documentation

## ◆ ENC_CODE_LEN

#define ENC_CODE_LEN 16

Length for encryption code.

Definition at line 61 of file ble_iso.h.

## ◆ ISO_ADDR_LEN

#define ISO_ADDR_LEN 6

Length for address.

Definition at line 60 of file ble_iso.h.

## ◆ ISO_SYNC0_PULSE

#define ISO_SYNC0_PULSE (0x1 << 0)

ISO sync0 pulse.

Definition at line 63 of file ble_iso.h.

## ◆ ISO_SYNC1_PULSE

#define ISO_SYNC1_PULSE (0x1 << 1)

ISO sync1 pulse.

Definition at line 64 of file ble_iso.h.