Functions
Configuration
Peripheral Driver » LL Driver » I2C » Functions

## Functions
__STATIC_INLINE void | ll_i2c_enable (i2c_regs_t *I2Cx)
| Enable I2C peripheral (ENABLE = 1). More...
__STATIC_INLINE void | ll_i2c_disable (i2c_regs_t *I2Cx)
| Disable I2C peripheral (ENABLE = 0). More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled (i2c_regs_t *I2Cx)
| Check if the I2C peripheral is enabled or disabled. More...
__STATIC_INLINE void | ll_i2c_enable_master_mode (i2c_regs_t *I2Cx)
| Enable I2C master mode. More...
__STATIC_INLINE void | ll_i2c_disable_master_mode (i2c_regs_t *I2Cx)
| Disable I2C master mode and enable slave mode. More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled_master_mode (i2c_regs_t *I2Cx)
| Check if I2C master mode is enabled or disabled. More...
__STATIC_INLINE void | ll_i2c_enable_general_call (i2c_regs_t *I2Cx)
| Enable General Call(slave mode). More...
__STATIC_INLINE void | ll_i2c_disable_general_call (i2c_regs_t *I2Cx)
| Disable General Call(slave mode). More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled_general_call (i2c_regs_t *I2Cx)
| Check if General Call is enabled or disabled(slave mode). More...
__STATIC_INLINE void | ll_i2c_enable_master_restart (i2c_regs_t *I2Cx)
| Enable Master Restart. More...
__STATIC_INLINE void | ll_i2c_disable_master_restart (i2c_regs_t *I2Cx)
| Disable Master Restart. More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled_master_restart (i2c_regs_t *I2Cx)
| Check if Master Restart is enabled or disabled. More...
__STATIC_INLINE void | ll_i2c_enable_stop_det_if_addressed (i2c_regs_t *I2Cx)
| Enable Slave issues STOP_DET interrupt only if addressed function. More...
__STATIC_INLINE void | ll_i2c_disable_stop_det_if_addressed (i2c_regs_t *I2Cx)
| Disable Slave issues STOP_DET interrupt only if addressed function. More...
__STATIC_INLINE void | ll_i2c_hold_bus_if_rx_full (i2c_regs_t *I2Cx)
| Hold bus when the RX FIFO if full function. More...
__STATIC_INLINE void | ll_i2c_overflow_if_rx_full (i2c_regs_t *I2Cx)
| overflow when the RX FIFO if full function. More...
__STATIC_INLINE void | ll_i2c_enable_bus_clear_feature (i2c_regs_t *I2Cx)
| enable bus clear feature function. More...
__STATIC_INLINE void | ll_i2c_disable_bus_clear_feature (i2c_regs_t *I2Cx)
| disable bus clear feature function. More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled_bus_clear_feature (i2c_regs_t *I2Cx)
| check bus clear feature is enabled function. More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled_stop_det_if_addressed (i2c_regs_t *I2Cx)
| Check if Slave issues STOP_DET interrupt only if addressed function is enabled or disabled. More...
__STATIC_INLINE void | ll_i2c_set_master_addressing_mode (i2c_regs_t *I2Cx, uint32_t addressing_mode)
| Configure the Master to transfers in 7-bit or 10-bit addressing mode. More...
__STATIC_INLINE uint32_t | ll_i2c_get_master_addressing_mode (i2c_regs_t *I2Cx)
| Get the Master addressing mode. More...
__STATIC_INLINE void | ll_i2c_set_own_address (i2c_regs_t *I2Cx, uint32_t own_address, uint32_t own_addr_size)
| Set the Own Address. More...
__STATIC_INLINE void | ll_i2c_set_clock_high_period_ss (i2c_regs_t *I2Cx, uint32_t count)
| Set the SCL clock high-period count for standard speed. More...
__STATIC_INLINE uint32_t | ll_i2c_get_clock_high_period_ss (i2c_regs_t *I2Cx)
| Get the SCL clock high-period count for standard speed. More...
__STATIC_INLINE void | ll_i2c_set_clock_low_period_ss (i2c_regs_t *I2Cx, uint32_t count)
| Set the SCL clock low-period count for standard speed. More...
__STATIC_INLINE uint32_t | ll_i2c_get_clock_low_period_ss (i2c_regs_t *I2Cx)
| Get the SCL clock low-period count for standard speed. More...
__STATIC_INLINE void | ll_i2c_set_clock_high_period_fs (i2c_regs_t *I2Cx, uint32_t count)
| Set the SCL clock high-period count for fast speed. More...
__STATIC_INLINE uint32_t | ll_i2c_get_clock_high_period_fs (i2c_regs_t *I2Cx)
| Get the SCL clock high-period count for fast speed. More...
__STATIC_INLINE void | ll_i2c_set_clock_low_period_fs (i2c_regs_t *I2Cx, uint32_t count)
| Set the SCL clock low-period count for fast speed. More...
__STATIC_INLINE uint32_t | ll_i2c_get_clock_low_period_fs (i2c_regs_t *I2Cx)
| Get the SCL clock low-period count for fast speed. More...
__STATIC_INLINE void | ll_i2c_set_clock_high_period_hs (i2c_regs_t *I2Cx, uint32_t count)
| Get the SCL clock high-period count for high speed. More...
__STATIC_INLINE uint32_t | ll_i2c_get_clock_high_period_hs (i2c_regs_t *I2Cx)
| Get the SCL clock high-period count for high speed. More...
__STATIC_INLINE void | ll_i2c_set_clock_low_period_hs (i2c_regs_t *I2Cx, uint32_t count)
| Get the SCL clock low-period count for high speed. More...
__STATIC_INLINE uint32_t | ll_i2c_get_clock_low_period_hs (i2c_regs_t *I2Cx)
| Get the SCL clock low-period count for high speed. More...
__STATIC_INLINE void | ll_i2c_set_spike_len_fs (i2c_regs_t *I2Cx, uint32_t length)
| Set the spike len in fast speed mode. More...
__STATIC_INLINE uint32_t | ll_i2c_get_spike_len_fs (i2c_regs_t *I2Cx)
| Get the spike len in fast speed mode. More...
__STATIC_INLINE void | ll_i2c_set_spike_len_hs (i2c_regs_t *I2Cx, uint32_t length)
| Set the spike len in high speed mode. More...
__STATIC_INLINE uint32_t | ll_i2c_get_spike_len_hs (i2c_regs_t *I2Cx)
| Get the spike len in high speed mode. More...
__STATIC_INLINE void | ll_i2c_set_speed_mode (i2c_regs_t *I2Cx, uint32_t speed_mode)
| Set I2C Speed mode. More...
__STATIC_INLINE uint32_t | ll_i2c_get_speed_mode (i2c_regs_t *I2Cx)
| Get I2C Speed mode. More...
__STATIC_INLINE void | ll_i2c_set_high_speed_master_code (i2c_regs_t *I2Cx, uint32_t code)
| Set I2C High Speed Master Code Address. More...
__STATIC_INLINE uint32_t | ll_i2c_get_high_speed_master_code (i2c_regs_t *I2Cx)
| Get I2C Speed mode. More...
__STATIC_INLINE void | ll_i2c_set_data_tx_hold_time (i2c_regs_t *I2Cx, uint32_t time)
| Set the required transmit SDA hold time in units of ic_clk period. More...
__STATIC_INLINE uint32_t | ll_i2c_get_data_tx_hold_time (i2c_regs_t *I2Cx)
| Get the required transmit SDA hold time in units of ic_clk period. More...
__STATIC_INLINE void | ll_i2c_set_data_rx_hold_time (i2c_regs_t *I2Cx, uint32_t time)
| Set the required receive SDA hold time in units of ic_clk period. More...
__STATIC_INLINE uint32_t | ll_i2c_get_data_rx_hold_time (i2c_regs_t *I2Cx)
| Get the required receive SDA hold time in units of ic_clk period. More...
__STATIC_INLINE void | ll_i2c_set_data_setup_time (i2c_regs_t *I2Cx, uint32_t time)
| Set the SDA setup time when operating as a slave transmitter. More...
__STATIC_INLINE uint32_t | ll_i2c_get_data_setup_time (i2c_regs_t *I2Cx)
| Get the SDA setup time when operating as a slave transmitter. More...
__STATIC_INLINE void | ll_i2c_set_tx_fifo_threshold (i2c_regs_t *I2Cx, uint32_t threshold)
| Set threshold of entries (or below) that trigger the TX_EMPTY interrupt. More...
__STATIC_INLINE uint32_t | ll_i2c_get_tx_fifo_threshold (i2c_regs_t *I2Cx)
| Get threshold of TX FIFO that triggers an THRE interrupt. More...
__STATIC_INLINE void | ll_i2c_set_rx_fifo_threshold (i2c_regs_t *I2Cx, uint32_t threshold)
| Set threshold of RX FIFO that triggers an RDA interrupt. More...
__STATIC_INLINE uint32_t | ll_i2c_get_rx_fifo_threshold (i2c_regs_t *I2Cx)
| Get threshold of RX FIFO that triggers an RDA interrupt. More...
__STATIC_INLINE uint32_t | ll_i2c_get_tx_fifo_level (i2c_regs_t *I2Cx)
| Get FIFO Transmission Level. More...
__STATIC_INLINE uint32_t | ll_i2c_get_rx_fifo_level (i2c_regs_t *I2Cx)
| Get FIFO reception Level. More...
__STATIC_INLINE void | ll_i2c_enable_sda_stuck_recovery (i2c_regs_t *I2Cx)
| Master initates the SDA stuck at low recovery mechanism. More...
__STATIC_INLINE void | ll_i2c_disable_sda_stuck_recovery (i2c_regs_t *I2Cx)
| Master disabled the SDA stuck at low recovery mechanism. More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled_sda_stuck_recovery (i2c_regs_t *I2Cx)
| the SDA stuck at low recovery mechanism is enabled or disabled. More...
__STATIC_INLINE void | ll_i2c_enable_transfer_abort (i2c_regs_t *I2Cx)
| Enable DMA reception requests. More...
__STATIC_INLINE uint32_t | ll_i2c_is_enabled_transfer_abort (i2c_regs_t *I2Cx)
| Check if DMA reception requests are enabled or disabled. More...
__STATIC_INLINE uint32_t | ll_i2c_get_abort_source (i2c_regs_t *I2Cx)
| Get the transmit abort source. More...
__STATIC_INLINE uint32_t | ll_i2c_get_tx_flush_count (i2c_regs_t *I2Cx)
| Get the number of Tx FIFO Data Commands which are flushed due to TX_ABRT interrupt. More...

## Detailed Description

## Function Documentation

## ◆ ll_i2c_disable()

__STATIC_INLINE void ll_i2c_disable | ( | i2c_regs_t * | I2Cx | ) |

Disable I2C peripheral (ENABLE = 0).

Note
  When ENABLE = 0, the TX FIFO and RX FIFO get flushed. Status bits in the IC_INTR_STAT register are still active until DW_apb_i2c goes into IDLE state. If the module is transmitting, it stops as well as deletes the contents of the transmit buffer after the current transfer is complete. If the module is receiving, the DW_apb_i2c stops the current transfer at the end of the current byte and does not acknowledge the transfer..

Register|BitsName ---------------|--------------- EN | ACTIVITY

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 404 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_disable_bus_clear_feature()

__STATIC_INLINE void ll_i2c_disable_bus_clear_feature | ( | i2c_regs_t * | I2Cx | ) |

disable bus clear feature function.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | BUS_CLR_FEATURE

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 665 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_disable_general_call()

__STATIC_INLINE void ll_i2c_disable_general_call | ( | i2c_regs_t * | I2Cx | ) |

Disable General Call(slave mode).

Note
  When disabled, the Address 0x00 is NACKed.

Register|BitsName ---------------|--------------- ACK_GEN_CALL | ACK_GEN_CALL

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 497 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_disable_master_mode()

__STATIC_INLINE void ll_i2c_disable_master_mode | ( | i2c_regs_t * | I2Cx | ) |

Disable I2C master mode and enable slave mode.

Register|BitsName ---------------|--------------- CTRL | MASTER_ENABLE CTRL | SLAVE_DISABLE

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 449 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_disable_master_restart()

__STATIC_INLINE void ll_i2c_disable_master_restart | ( | i2c_regs_t * | I2Cx | ) |

Disable Master Restart.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | RESTART_EN

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 550 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_disable_sda_stuck_recovery()

__STATIC_INLINE void ll_i2c_disable_sda_stuck_recovery | ( | i2c_regs_t * | I2Cx | ) |

Master disabled the SDA stuck at low recovery mechanism.

Register|BitsName ---------------|--------------- EN | SDA_STUCK_RECOVERY

Parameters

  I2Cx | I2C instance

Definition at line 1436 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_disable_stop_det_if_addressed()

__STATIC_INLINE void ll_i2c_disable_stop_det_if_addressed | ( | i2c_regs_t * | I2Cx | ) |

Disable Slave issues STOP_DET interrupt only if addressed function.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | STOP_DET_INT

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 601 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable()

__STATIC_INLINE void ll_i2c_enable | ( | i2c_regs_t * | I2Cx | ) |

Enable I2C peripheral (ENABLE = 1).

Register|BitsName ---------------|--------------- EN | ACTIVITY

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 384 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable_bus_clear_feature()

__STATIC_INLINE void ll_i2c_enable_bus_clear_feature | ( | i2c_regs_t * | I2Cx | ) |

enable bus clear feature function.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | BUS_CLR_FEATURE

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 649 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable_general_call()

__STATIC_INLINE void ll_i2c_enable_general_call | ( | i2c_regs_t * | I2Cx | ) |

Enable General Call(slave mode).

Note
  When enabled, the Address 0x00 is ACKed.

Register|BitsName ---------------|--------------- ACK_GEN_CALL | ACK_GEN_CALL

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 481 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable_master_mode()

__STATIC_INLINE void ll_i2c_enable_master_mode | ( | i2c_regs_t * | I2Cx | ) |

Enable I2C master mode.

Register|BitsName ---------------|--------------- CTRL | MASTER_ENABLE CTRL | SLAVE_DISABLE

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 434 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable_master_restart()

__STATIC_INLINE void ll_i2c_enable_master_restart | ( | i2c_regs_t * | I2Cx | ) |

Enable Master Restart.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0). This bit determines whether RESTART conditions may be sent when acting as a master. Some older slaves do not support handling RESTART conditions. When RESTART is disabled, the master is prohibited from performing the following functions:
  - Performing any high-speed mode operation.
  - Performing direction changes in combined format mode.
  - Performing a read operation with a 10-bit address.

Register|BitsName ---------------|--------------- CTRL | RESTART_EN

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 534 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable_sda_stuck_recovery()

__STATIC_INLINE void ll_i2c_enable_sda_stuck_recovery | ( | i2c_regs_t * | I2Cx | ) |

Master initates the SDA stuck at low recovery mechanism.

Register|BitsName ---------------|--------------- EN | SDA_STUCK_RECOVERY

Parameters

  I2Cx | I2C instance

Definition at line 1422 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable_stop_det_if_addressed()

__STATIC_INLINE void ll_i2c_enable_stop_det_if_addressed | ( | i2c_regs_t * | I2Cx | ) |

Enable Slave issues STOP_DET interrupt only if addressed function.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0). During a general call address, the slave does not issue the STOP_DET interrupt if STOP_DET_IF_ADDRESSED = 1'b1, even if the slave responds to the general call address by generating ACK. The STOP_DET interrupt is generated only when the transmitted address matches the slave address (SAR).

Register|BitsName ---------------|--------------- CTRL | STOP_DET_INT

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 585 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_enable_transfer_abort()

__STATIC_INLINE void ll_i2c_enable_transfer_abort | ( | i2c_regs_t * | I2Cx | ) |

Enable DMA reception requests.

Register|BitsName ---------------|--------------- EN | ABORT

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 1466 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_abort_source()

__STATIC_INLINE uint32_t ll_i2c_get_abort_source | ( | i2c_regs_t * | I2Cx | ) |

Get the transmit abort source.

Note
  This can be used to retrieve source of TX_ABRT interrupt.

Register|BitsName ---------------|--------------- TX_ABORT_SRC | ABRT_USER_ABRT TX_ABORT_SRC | ABRT_SLVRD_INTX TX_ABORT_SRC | ABRT_SLV_ARBLOST TX_ABORT_SRC | ABRT_SLVFLUSH_TXFIFO TX_ABORT_SRC | ABRT_ARB_LOST TX_ABORT_SRC | ABRT_MST_DIS TX_ABORT_SRC | ABRT_10B_RD_NORSTRT TX_ABORT_SRC | ABRT_SBYTE_NORSTRT TX_ABORT_SRC | ABRT_HS_NORSTRT TX_ABORT_SRC | ABRT_SBYTE_ACKDET TX_ABORT_SRC | ABRT_HS_ACKDET TX_ABORT_SRC | ABRT_GCALL_READ TX_ABORT_SRC | ABRT_GCALL_NOACK TX_ABORT_SRC | ABRT_TXDATA_NOACK TX_ABORT_SRC | ABRT_10ADDR2_NOACK TX_ABORT_SRC | ABRT_10ADDR1_NOACK TX_ABORT_SRC | ABRT_7B_ADDR_NOACK

Parameters

  I2Cx | I2C instance

Return values

  Returned | value can be a combination of the following values: LL_I2C_ABRT_USER_ABRT LL_I2C_ABRT_SLVRD_INTX LL_I2C_ABRT_SLV_ARBLOST LL_I2C_ABRT_SLVFLUSH_TXFIFO LL_I2C_ABRT_ARB_LOST LL_I2C_ABRT_MST_DIS LL_I2C_ABRT_10B_RD_NORSTRT LL_I2C_ABRT_SBYTE_NORSTRT LL_I2C_ABRT_HS_NORSTRT LL_I2C_ABRT_SBYTE_ACKDET LL_I2C_ABRT_HS_ACKDET LL_I2C_ABRT_GCALL_READ LL_I2C_ABRT_GCALL_NOACK LL_I2C_ABRT_TXDATA_NOACK LL_I2C_ABRT_10ADDR2_NOACK LL_I2C_ABRT_10ADDR1_NOACK LL_I2C_ABRT_7B_ADDR_NOACK

Note
  - LL_I2C_ABRT_TX_FLUSH_CNT can be used as a mask to get the number of Tx FIFO Data Commands which are flushed due to TX_ABRT interrupt.

Definition at line 1534 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_clock_high_period_fs()

__STATIC_INLINE uint32_t ll_i2c_get_clock_high_period_fs | ( | i2c_regs_t * | I2Cx | ) |

Get the SCL clock high-period count for fast speed.

Register|BitsName ---------------|--------------- FS_CLK_HCOUNT | COUNT

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x6 and 0xFFFF.

Definition at line 852 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_clock_high_period_hs()

__STATIC_INLINE uint32_t ll_i2c_get_clock_high_period_hs | ( | i2c_regs_t * | I2Cx | ) |

Get the SCL clock high-period count for high speed.

Register|BitsName ---------------|--------------- HS_CLK_HCOUNT | COUNT

Parameters

  I2Cx | I2C instance.

Return values

  range | between 0x6 and 0xFFFF, should be larger than IC_HS_SPKLEN + 7.

Definition at line 916 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_clock_high_period_ss()

__STATIC_INLINE uint32_t ll_i2c_get_clock_high_period_ss | ( | i2c_regs_t * | I2Cx | ) |

Get the SCL clock high-period count for standard speed.

Register|BitsName ---------------|--------------- SS_CLK_HCOUNT | COUNT

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x6 and 0xFFF5.

Definition at line 788 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_clock_low_period_fs()

__STATIC_INLINE uint32_t ll_i2c_get_clock_low_period_fs | ( | i2c_regs_t * | I2Cx | ) |

Get the SCL clock low-period count for fast speed.

Register|BitsName ---------------|--------------- FS_CLK_LCOUNT | COUNT

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x8 and 0xFFFF.

Definition at line 884 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_clock_low_period_hs()

__STATIC_INLINE uint32_t ll_i2c_get_clock_low_period_hs | ( | i2c_regs_t * | I2Cx | ) |

Get the SCL clock low-period count for high speed.

Register|BitsName ---------------|--------------- HS_CLK_LCOUNT | COUNT

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x8 and 0xFFFF

Definition at line 948 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_clock_low_period_ss()

__STATIC_INLINE uint32_t ll_i2c_get_clock_low_period_ss | ( | i2c_regs_t * | I2Cx | ) |

Get the SCL clock low-period count for standard speed.

Register|BitsName ---------------|--------------- SS_CLK_LCOUNT | COUNT

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x8 and 0xFFFF.

Definition at line 820 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_data_rx_hold_time()

__STATIC_INLINE uint32_t ll_i2c_get_data_rx_hold_time | ( | i2c_regs_t * | I2Cx | ) |

Get the required receive SDA hold time in units of ic_clk period.

Register|BitsName ---------------|--------------- SDA_HOLD | RX_HOLD

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 1 and (N_SCL_LOW - 2) in master mode or 7 and (N_SCL_LOW - 2) in slave mode

Definition at line 1148 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_data_setup_time()

__STATIC_INLINE uint32_t ll_i2c_get_data_setup_time | ( | i2c_regs_t * | I2Cx | ) |

Get the SDA setup time when operating as a slave transmitter.

Register|BitsName ---------------|--------------- SDA_SETUP | SETUP

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x02 and 0xFF.

Definition at line 1182 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_data_tx_hold_time()

__STATIC_INLINE uint32_t ll_i2c_get_data_tx_hold_time | ( | i2c_regs_t * | I2Cx | ) |

Get the required transmit SDA hold time in units of ic_clk period.

Register|BitsName ---------------|--------------- SDA_HOLD | TX_HOLD

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 1 and (N_SCL_LOW - 2) in master mode or 7 and (N_SCL_LOW - 2) in slave mode

Definition at line 1115 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_high_speed_master_code()

__STATIC_INLINE uint32_t ll_i2c_get_high_speed_master_code | ( | i2c_regs_t * | I2Cx | ) |

Get I2C Speed mode.

Register|BitsName ---------------|--------------- M_HS_ADDR | HS_MAR

Parameters

  I2Cx | I2C instance.

Return values

  Returned | value range between 0x00 and 0x07.

Definition at line 1082 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_master_addressing_mode()

__STATIC_INLINE uint32_t ll_i2c_get_master_addressing_mode | ( | i2c_regs_t * | I2Cx | ) |

Get the Master addressing mode.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | ADDR_BIT_M

Parameters

  I2Cx | I2C instance.

Return values

  Returned | value can be one of the following values: LL_I2C_ADDRESSING_MODE_7BIT LL_I2C_ADDRESSING_MODE_10BIT

Definition at line 733 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_rx_fifo_level()

__STATIC_INLINE uint32_t ll_i2c_get_rx_fifo_level | ( | i2c_regs_t * | I2Cx | ) |

Get FIFO reception Level.

Register|BitsName ---------------|--------------- RX_FIFO_THD | LEVEL

Parameters

  I2Cx | I2C instance

Return values

  Value | range between 0x0 and 0x1F.

Definition at line 1408 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_rx_fifo_threshold()

__STATIC_INLINE uint32_t ll_i2c_get_rx_fifo_threshold | ( | i2c_regs_t * | I2Cx | ) |

Get threshold of RX FIFO that triggers an RDA interrupt.

Register|BitsName ---------------|--------------- RX_FIFO_THD | THD

Parameters

  I2Cx | I2C instance

Return values

  Returned | value can be one of the following values: LL_I2C_RX_FIFO_TH_CHAR_1 LL_I2C_RX_FIFO_TH_CHAR_2 LL_I2C_RX_FIFO_TH_CHAR_3 LL_I2C_RX_FIFO_TH_CHAR_4 LL_I2C_RX_FIFO_TH_CHAR_5 LL_I2C_RX_FIFO_TH_CHAR_6 LL_I2C_RX_FIFO_TH_CHAR_7 LL_I2C_RX_FIFO_TH_CHAR_8 LL_I2C_RX_FIFO_TH_CHAR_9 LL_I2C_RX_FIFO_TH_CHAR_10 LL_I2C_RX_FIFO_TH_CHAR_11 LL_I2C_RX_FIFO_TH_CHAR_12 LL_I2C_RX_FIFO_TH_CHAR_13 LL_I2C_RX_FIFO_TH_CHAR_14 LL_I2C_RX_FIFO_TH_CHAR_15 LL_I2C_RX_FIFO_TH_CHAR_16 LL_I2C_RX_FIFO_TH_CHAR_17 LL_I2C_RX_FIFO_TH_CHAR_18 LL_I2C_RX_FIFO_TH_CHAR_19 LL_I2C_RX_FIFO_TH_CHAR_20 LL_I2C_RX_FIFO_TH_CHAR_21 LL_I2C_RX_FIFO_TH_CHAR_22 LL_I2C_RX_FIFO_TH_CHAR_23 LL_I2C_RX_FIFO_TH_CHAR_24 LL_I2C_RX_FIFO_TH_CHAR_25 LL_I2C_RX_FIFO_TH_CHAR_26 LL_I2C_RX_FIFO_TH_CHAR_27 LL_I2C_RX_FIFO_TH_CHAR_28 LL_I2C_RX_FIFO_TH_CHAR_29 LL_I2C_RX_FIFO_TH_CHAR_30 LL_I2C_RX_FIFO_TH_CHAR_31 LL_I2C_RX_FIFO_TH_CHAR_32 LL_I2C_RX_FIFO_TH_FULL

Definition at line 1378 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_speed_mode()

__STATIC_INLINE uint32_t ll_i2c_get_speed_mode | ( | i2c_regs_t * | I2Cx | ) |

Get I2C Speed mode.

Register|BitsName ---------------|--------------- CTRL | SPEED

Parameters

  I2Cx | I2C instance.

Return values

  Value | can be one of the following values: LL_I2C_SPEED_MODE_STANDARD LL_I2C_SPEED_MODE_FAST LL_I2C_SPEED_MODE_HIGH

Definition at line 1050 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_spike_len_fs()

__STATIC_INLINE uint32_t ll_i2c_get_spike_len_fs | ( | i2c_regs_t * | I2Cx | ) |

Get the spike len in fast speed mode.

Register|BitsName ---------------|--------------- FS_SPKLEN | FS_SPKLEN

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x2 and 0xFF.

Definition at line 980 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_spike_len_hs()

__STATIC_INLINE uint32_t ll_i2c_get_spike_len_hs | ( | i2c_regs_t * | I2Cx | ) |

Get the spike len in high speed mode.

Register|BitsName ---------------|--------------- HS_SPKLEN | HS_SPKLEN

Parameters

  I2Cx | I2C instance.

Return values

  Value | range between 0x2 and 0xFF.

Definition at line 1012 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_tx_fifo_level()

__STATIC_INLINE uint32_t ll_i2c_get_tx_fifo_level | ( | i2c_regs_t * | I2Cx | ) |

Get FIFO Transmission Level.

Register|BitsName ---------------|--------------- RX_FIFO_THD | LEVEL

Parameters

  I2Cx | I2C instance

Return values

  Value | range between 0x0 and 0x1F.

Definition at line 1393 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_tx_fifo_threshold()

__STATIC_INLINE uint32_t ll_i2c_get_tx_fifo_threshold | ( | i2c_regs_t * | I2Cx | ) |

Get threshold of TX FIFO that triggers an THRE interrupt.

Register|BitsName ---------------|--------------- TX_FIFO_THD | THD

Parameters

  I2Cx | I2C instance

Return values

  Returned | value can be one of the following values: LL_I2C_TX_FIFO_TH_EMPTY LL_I2C_TX_FIFO_TH_CHAR_1 LL_I2C_TX_FIFO_TH_CHAR_2 LL_I2C_TX_FIFO_TH_CHAR_3 LL_I2C_TX_FIFO_TH_CHAR_4 LL_I2C_TX_FIFO_TH_CHAR_5 LL_I2C_TX_FIFO_TH_CHAR_6 LL_I2C_TX_FIFO_TH_CHAR_7 LL_I2C_TX_FIFO_TH_CHAR_8 LL_I2C_TX_FIFO_TH_CHAR_9 LL_I2C_TX_FIFO_TH_CHAR_10 LL_I2C_TX_FIFO_TH_CHAR_11 LL_I2C_TX_FIFO_TH_CHAR_12 LL_I2C_TX_FIFO_TH_CHAR_13 LL_I2C_TX_FIFO_TH_CHAR_14 LL_I2C_TX_FIFO_TH_CHAR_15 LL_I2C_TX_FIFO_TH_CHAR_16 LL_I2C_TX_FIFO_TH_CHAR_17 LL_I2C_TX_FIFO_TH_CHAR_18 LL_I2C_TX_FIFO_TH_CHAR_19 LL_I2C_TX_FIFO_TH_CHAR_20 LL_I2C_TX_FIFO_TH_CHAR_21 LL_I2C_TX_FIFO_TH_CHAR_22 LL_I2C_TX_FIFO_TH_CHAR_23 LL_I2C_TX_FIFO_TH_CHAR_24 LL_I2C_TX_FIFO_TH_CHAR_25 LL_I2C_TX_FIFO_TH_CHAR_26 LL_I2C_TX_FIFO_TH_CHAR_27 LL_I2C_TX_FIFO_TH_CHAR_28 LL_I2C_TX_FIFO_TH_CHAR_29 LL_I2C_TX_FIFO_TH_CHAR_30 LL_I2C_TX_FIFO_TH_CHAR_31 LL_I2C_TX_FIFO_TH_CHAR_32

Definition at line 1280 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_get_tx_flush_count()

__STATIC_INLINE uint32_t ll_i2c_get_tx_flush_count | ( | i2c_regs_t * | I2Cx | ) |

Get the number of Tx FIFO Data Commands which are flushed due to TX_ABRT interrupt.

Register|BitsName ---------------|--------------- TX_ABORT_SRC | TX_FLUSH_CNT

Parameters

  I2Cx | I2C instance

Return values

  Tx | flush count.

Definition at line 1549 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_hold_bus_if_rx_full()

__STATIC_INLINE void ll_i2c_hold_bus_if_rx_full | ( | i2c_regs_t * | I2Cx | ) |

Hold bus when the RX FIFO if full function.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | RXFIFO_FULL_HLD

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 617 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled()

__STATIC_INLINE uint32_t ll_i2c_is_enabled | ( | i2c_regs_t * | I2Cx | ) |

Check if the I2C peripheral is enabled or disabled.

Register|BitsName ---------------|--------------- STAT | STAT_EN

Parameters

  I2Cx | I2C instance.

Return values

  State | of bit (1 or 0).

Definition at line 419 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled_bus_clear_feature()

__STATIC_INLINE uint32_t ll_i2c_is_enabled_bus_clear_feature | ( | i2c_regs_t * | I2Cx | ) |

check bus clear feature is enabled function.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | BUS_CLR_FEATURE

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 681 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled_general_call()

__STATIC_INLINE uint32_t ll_i2c_is_enabled_general_call | ( | i2c_regs_t * | I2Cx | ) |

Check if General Call is enabled or disabled(slave mode).

Register|BitsName ---------------|--------------- ACK_GEN_CALL | ACK_GEN_CALL

Parameters

  I2Cx | I2C instance.

Return values

  State | of bit (1 or 0).

Definition at line 512 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled_master_mode()

__STATIC_INLINE uint32_t ll_i2c_is_enabled_master_mode | ( | i2c_regs_t * | I2Cx | ) |

Check if I2C master mode is enabled or disabled.

Register|BitsName ---------------|--------------- CTRL | MASTER_ENABLE CTRL | SLAVE_DISABLE

Parameters

  I2Cx | I2C instance.

Return values

  State | of bit (1 or 0).

Definition at line 465 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled_master_restart()

__STATIC_INLINE uint32_t ll_i2c_is_enabled_master_restart | ( | i2c_regs_t * | I2Cx | ) |

Check if Master Restart is enabled or disabled.

Register|BitsName ---------------|--------------- CTRL | RESTART_EN

Parameters

  I2Cx | I2C instance.

Return values

  State | of bit (1 or 0).

Definition at line 565 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled_sda_stuck_recovery()

__STATIC_INLINE uint32_t ll_i2c_is_enabled_sda_stuck_recovery | ( | i2c_regs_t * | I2Cx | ) |

the SDA stuck at low recovery mechanism is enabled or disabled.

Register|BitsName ---------------|--------------- EN | SDA_STUCK_RECOVERY

Parameters

  I2Cx | I2C instance

Return values

  State | of bit (1 or 0).

Definition at line 1451 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled_stop_det_if_addressed()

__STATIC_INLINE uint32_t ll_i2c_is_enabled_stop_det_if_addressed | ( | i2c_regs_t * | I2Cx | ) |

Check if Slave issues STOP_DET interrupt only if addressed function is enabled or disabled.

Register|BitsName ---------------|--------------- CTRL | STOP_DET_INT

Parameters

  I2Cx | I2C instance.

Return values

  State | of bit (1 or 0).

Definition at line 696 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_is_enabled_transfer_abort()

__STATIC_INLINE uint32_t ll_i2c_is_enabled_transfer_abort | ( | i2c_regs_t * | I2Cx | ) |

Check if DMA reception requests are enabled or disabled.

Register|BitsName ---------------|--------------- EN | ABORT

Parameters

  I2Cx | I2C instance.

Return values

  State | of bit (1 or 0).

Definition at line 1481 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_overflow_if_rx_full()

__STATIC_INLINE void ll_i2c_overflow_if_rx_full | ( | i2c_regs_t * | I2Cx | ) |

overflow when the RX FIFO if full function.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | RXFIFO_FULL_HLD

Parameters

  I2Cx | I2C instance.

Return values

  None. |

Definition at line 633 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_clock_high_period_fs()

__STATIC_INLINE void ll_i2c_set_clock_high_period_fs | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | count
| ) |  |

Set the SCL clock high-period count for fast speed.

Note
  The register IC_FS_SCL_HCNT can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- FS_CLK_HCOUNT | COUNT

Parameters

  I2Cx | I2C instance.
  count | range between 0x6 and 0xFFFF.

Return values

  None. |

Definition at line 837 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_clock_high_period_hs()

__STATIC_INLINE void ll_i2c_set_clock_high_period_hs | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | count
| ) |  |

Get the SCL clock high-period count for high speed.

Note
  The register IC_HS_SCL_HCNT can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- HS_CLK_HCOUNT | COUNT

Parameters

  I2Cx | I2C instance.
  count | range between 0x6 and 0xFFFF, should be larger than IC_HS_SPKLEN + 5.

Return values

  None. |

Definition at line 901 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_clock_high_period_ss()

__STATIC_INLINE void ll_i2c_set_clock_high_period_ss | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | count
| ) |  |

Set the SCL clock high-period count for standard speed.

Note
  The register IC_SS_SCL_HCNT can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- SS_CLK_HCOUNT | SS_SCL_HCNT

Parameters

  I2Cx | I2C instance.
  count | This parameter must be a value range between 6 ~ 0xFFF5.

Return values

  None. |

Definition at line 773 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_clock_low_period_fs()

__STATIC_INLINE void ll_i2c_set_clock_low_period_fs | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | count
| ) |  |

Set the SCL clock low-period count for fast speed.

Note
  The register IC_FS_SCL_LCNT can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- FS_CLK_LCOUNT | COUNT

Parameters

  I2Cx | I2C instance.
  count | range between 0x8 and 0xFFFF

Return values

  None. |

Definition at line 869 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_clock_low_period_hs()

__STATIC_INLINE void ll_i2c_set_clock_low_period_hs | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | count
| ) |  |

Get the SCL clock low-period count for high speed.

Note
  The register IC_HS_SCL_LCNT can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- HS_CLK_LCOUNT | COUNT

Parameters

  I2Cx | I2C instance.
  count | range between 0x8 and 0xFFFF

Return values

  None. |

Definition at line 933 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_clock_low_period_ss()

__STATIC_INLINE void ll_i2c_set_clock_low_period_ss | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | count
| ) |  |

Set the SCL clock low-period count for standard speed.

Note
  The register IC_SS_SCL_LCNT can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- SS_CLK_LCOUNT | COUNT

Parameters

  I2Cx | I2C instance.
  count | This parameter must be a value range between 0x8 and 0xFFFF.

Return values

  None. |

Definition at line 805 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_data_rx_hold_time()

__STATIC_INLINE void ll_i2c_set_data_rx_hold_time | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | time
| ) |  |

Set the required receive SDA hold time in units of ic_clk period.

Note
  The register IC_SDA_HOLD can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- SDA_HOLD | RX_HOLD

Parameters

  I2Cx | I2C instance.
  time | SDA Tx hold time in units of ic_clk period. Time should range between 1 and (N_SCL_LOW - 2) in master mode or 7 and (N_SCL_LOW - 2) in slave mode.

Return values

  Value | between Min_Data=0x0 and Max_Data=0xF

Definition at line 1133 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_data_setup_time()

__STATIC_INLINE void ll_i2c_set_data_setup_time | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | time
| ) |  |

Set the SDA setup time when operating as a slave transmitter.

Note
  The register IC_SDA_SETUP can only be programmed when the I2C is disabled (ENABLE = 0). The length of setup time is calculated using [(IC_SDA_SETUP - 1) * (ic_clk_period)], so if the user requires 10 ic_clk periods of setup time, they should program a value of 11.

Register|BitsName ---------------|--------------- SDA_SETUP | SETUP

Parameters

  I2Cx | I2C instance.
  time | SDA data setup time in units of ic_clk period, range between 2 ~ 0xFF.

Return values

  None. |

Definition at line 1167 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_data_tx_hold_time()

__STATIC_INLINE void ll_i2c_set_data_tx_hold_time | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | time
| ) |  |

Set the required transmit SDA hold time in units of ic_clk period.

Note
  The register IC_SDA_HOLD can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- SDA_HOLD | TX_HOLD

Parameters

  I2Cx | I2C instance.
  time | SDA Tx hold time in units of ic_clk period. Time should range between 1 and (N_SCL_LOW - 2) in master mode or 7 and (N_SCL_LOW - 2) in slave mode.

Return values

  None. |

Definition at line 1100 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_high_speed_master_code()

__STATIC_INLINE void ll_i2c_set_high_speed_master_code | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | code
| ) |  |

Set I2C High Speed Master Code Address.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- M_HS_ADDR | HS_MAR

Parameters

  I2Cx | I2C instance.
  code | HS mode master code, range between 0x00 and 0x07.

Return values

  None. |

Definition at line 1067 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_master_addressing_mode()

__STATIC_INLINE void ll_i2c_set_master_addressing_mode | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | addressing_mode
| ) |  |

Configure the Master to transfers in 7-bit or 10-bit addressing mode.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | ADDR_BIT_M

Parameters

  I2Cx | I2C instance.
  addressing_mode | This parameter can be one of the following values: LL_I2C_ADDRESSING_MODE_7BIT LL_I2C_ADDRESSING_MODE_10BIT

Return values

  None. |

Definition at line 715 of file gr533x_ll_i2c.h.

Referenced by ll_i2c_handle_transfer().

## ◆ ll_i2c_set_own_address()

__STATIC_INLINE void ll_i2c_set_own_address | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | own_address,
|  | uint32_t | own_addr_size
| ) |  |

Set the Own Address.

Note
  The register IC_CON and IC_SAR can only be programmed when the I2C is disabled (IC_ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | ADDR_BIT_S S_ADDR | SAR

Parameters

  I2Cx | I2C instance.
  own_address | This parameter must be a value range between 0 ~ 0x3FF(10-bit mode) or 0 ~ 0x7F(7-bit mode). Reserved address 0x00 to 0x07, or 0x78 to 0x7f should not be configured.
  own_addr_size | This parameter can be one of the following values: LL_I2C_OWNADDRESS_7BIT LL_I2C_OWNADDRESS_10BIT

Return values

  None. |

Definition at line 755 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_rx_fifo_threshold()

__STATIC_INLINE void ll_i2c_set_rx_fifo_threshold | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | threshold
| ) |  |

Set threshold of RX FIFO that triggers an RDA interrupt.

Note
  TX FIFO threshold only can be configured after FIFO was enabled.

Register|BitsName ---------------|--------------- RX_FIFO_THD | THD

Parameters

  I2Cx | I2C instance
  threshold | This parameter can be one of the following values: LL_I2C_RX_FIFO_TH_CHAR_1 LL_I2C_RX_FIFO_TH_CHAR_2 LL_I2C_RX_FIFO_TH_CHAR_3 LL_I2C_RX_FIFO_TH_CHAR_4 LL_I2C_RX_FIFO_TH_CHAR_5 LL_I2C_RX_FIFO_TH_CHAR_6 LL_I2C_RX_FIFO_TH_CHAR_7 LL_I2C_RX_FIFO_TH_CHAR_8 LL_I2C_RX_FIFO_TH_CHAR_9 LL_I2C_RX_FIFO_TH_CHAR_10 LL_I2C_RX_FIFO_TH_CHAR_11 LL_I2C_RX_FIFO_TH_CHAR_12 LL_I2C_RX_FIFO_TH_CHAR_13 LL_I2C_RX_FIFO_TH_CHAR_14 LL_I2C_RX_FIFO_TH_CHAR_15 LL_I2C_RX_FIFO_TH_CHAR_16 LL_I2C_RX_FIFO_TH_CHAR_17 LL_I2C_RX_FIFO_TH_CHAR_18 LL_I2C_RX_FIFO_TH_CHAR_19 LL_I2C_RX_FIFO_TH_CHAR_20 LL_I2C_RX_FIFO_TH_CHAR_21 LL_I2C_RX_FIFO_TH_CHAR_22 LL_I2C_RX_FIFO_TH_CHAR_23 LL_I2C_RX_FIFO_TH_CHAR_24 LL_I2C_RX_FIFO_TH_CHAR_25 LL_I2C_RX_FIFO_TH_CHAR_26 LL_I2C_RX_FIFO_TH_CHAR_27 LL_I2C_RX_FIFO_TH_CHAR_28 LL_I2C_RX_FIFO_TH_CHAR_29 LL_I2C_RX_FIFO_TH_CHAR_30 LL_I2C_RX_FIFO_TH_CHAR_31 LL_I2C_RX_FIFO_TH_CHAR_32 LL_I2C_RX_FIFO_TH_FULL

Return values

  None. |

Definition at line 1330 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_speed_mode()

__STATIC_INLINE void ll_i2c_set_speed_mode | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | speed_mode
| ) |  |

Set I2C Speed mode.

Note
  The register IC_CON can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- CTRL | SPEED

Parameters

  I2Cx | I2C instance.
  speed_mode | This parameter can be one of the following values: LL_I2C_SPEED_MODE_STANDARD LL_I2C_SPEED_MODE_FAST LL_I2C_SPEED_MODE_HIGH

Return values

  None. |

Definition at line 1032 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_spike_len_fs()

__STATIC_INLINE void ll_i2c_set_spike_len_fs | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | length
| ) |  |

Set the spike len in fast speed mode.

Note
  The register FS_SPKLEN can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- FS_SPKLEN | FS_SPKLEN

Parameters

  I2Cx | I2C instance.
  length | Spike len.

Return values

  None. |

Definition at line 965 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_spike_len_hs()

__STATIC_INLINE void ll_i2c_set_spike_len_hs | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | length
| ) |  |

Set the spike len in high speed mode.

Note
  The register FS_SPKLEN can only be programmed when the I2C is disabled (ENABLE = 0).

Register|BitsName ---------------|--------------- HS_SPKLEN | HS_SPKLEN

Parameters

  I2Cx | I2C instance.
  length | Spike len.

Return values

  None. |

Definition at line 997 of file gr533x_ll_i2c.h.

## ◆ ll_i2c_set_tx_fifo_threshold()

__STATIC_INLINE void ll_i2c_set_tx_fifo_threshold | ( | i2c_regs_t * | I2Cx,
|  | uint32_t | threshold
| ) |  |

Set threshold of entries (or below) that trigger the TX_EMPTY interrupt.

Note
  TX FIFO threshold only can be configured after FIFO was enabled.

Register|BitsName ---------------|--------------- TX_FIFO_THD | THD

Parameters

  I2Cx | I2C instance
  threshold | This parameter can be one of the following values: LL_I2C_TX_FIFO_TH_EMPTY LL_I2C_TX_FIFO_TH_CHAR_1 LL_I2C_TX_FIFO_TH_CHAR_2 LL_I2C_TX_FIFO_TH_CHAR_3 LL_I2C_TX_FIFO_TH_CHAR_4 LL_I2C_TX_FIFO_TH_CHAR_5 LL_I2C_TX_FIFO_TH_CHAR_6 LL_I2C_TX_FIFO_TH_CHAR_7 LL_I2C_TX_FIFO_TH_CHAR_8 LL_I2C_TX_FIFO_TH_CHAR_9 LL_I2C_TX_FIFO_TH_CHAR_10 LL_I2C_TX_FIFO_TH_CHAR_11 LL_I2C_TX_FIFO_TH_CHAR_12 LL_I2C_TX_FIFO_TH_CHAR_13 LL_I2C_TX_FIFO_TH_CHAR_14 LL_I2C_TX_FIFO_TH_CHAR_15 LL_I2C_TX_FIFO_TH_CHAR_16 LL_I2C_TX_FIFO_TH_CHAR_17 LL_I2C_TX_FIFO_TH_CHAR_18 LL_I2C_TX_FIFO_TH_CHAR_19 LL_I2C_TX_FIFO_TH_CHAR_20 LL_I2C_TX_FIFO_TH_CHAR_21 LL_I2C_TX_FIFO_TH_CHAR_22 LL_I2C_TX_FIFO_TH_CHAR_23 LL_I2C_TX_FIFO_TH_CHAR_24 LL_I2C_TX_FIFO_TH_CHAR_25 LL_I2C_TX_FIFO_TH_CHAR_26 LL_I2C_TX_FIFO_TH_CHAR_27 LL_I2C_TX_FIFO_TH_CHAR_28 LL_I2C_TX_FIFO_TH_CHAR_29 LL_I2C_TX_FIFO_TH_CHAR_30 LL_I2C_TX_FIFO_TH_CHAR_31 LL_I2C_TX_FIFO_TH_CHAR_32

Return values

  None. |

Definition at line 1232 of file gr533x_ll_i2c.h.