Here is a list of all class members with links to the classes they belong to:

### - l -

- l2cap_evt : ble_evt_t
- last_crank_event_time : cscs_meas_val_t
- last_wheel_event_time : cscs_meas_val_t
- latency : ble_gap_conn_update_cmp_t
- le_psm : ble_gap_lepsm_register_t , ble_l2cap_evt_conn_ind_t , ble_l2cap_evt_conn_req_t , ble_l2cap_lecb_conn_req_t , lecb_conn_ind_t , lecb_conn_req_ind_t
- leading_address : app_spi_screen_config_t
- len : ble_gattc_multiple_att_t , hids_evt_t , hids_report_map_t , link_node
- length : _xqspi_command_t , ags_evt_t , ams_c_attr_info_t , ams_c_cmd_list_t , ams_c_cplt_attr_data_t , ans_c_new_alert_t , ans_new_alert_t , bcs_evt_t , ble_gap_dev_name_ind_t , ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t , ble_gap_max_adv_data_len_ind_t , ble_gattc_evt_ntf_ind_t , ble_gattc_ntf_ind_t , ble_gattc_read_value_t , ble_gattc_write_attr_value_t , ble_gattc_write_no_resp_t , ble_gatts_evt_write_t , ble_gatts_noti_ind_t , ble_gatts_prep_write_cfm_t , ble_gatts_read_cfm_t , ble_l2cap_evt_sdu_recv_t , ble_l2cap_lecb_sdu_t , cscs_evt_t , cts_evt_t , dis_c_string_t , dis_string_t , gatts_write_req_cb_t , gls_evt_t , gus_c_evt_t , gus_evt_t , hts_evt_t , lms_evt_t , lns_log_data_t , mlmr_c_evt_t , mlmr_evt_t , noti_multiple_t , otas_c_evt_t , otas_evt_t , pcs_evt_t , prf_att_info_t , rscs_evt_t , samples_evt_t , ths_c_evt_t , ths_evt_t , thscps_setting_t , uds_evt_t , uds_regi_user_data_stream_t , wechat_data_t , wss_evt_t
- length_ext : ags_header_base_t
- level : ble_sec_param_t
- lfsr_mode : _ll_rng_init , _rng_init
- list_len : dis_reg_cert_data_list_t
- list_length : dis_c_reg_cert_data_list_t
- ll_capture_channel0 : _ll_timer_init_t
- ll_capture_channel1 : _ll_timer_init_t
- ll_capture_channel2 : _ll_timer_init_t
- ll_capture_channel3 : _ll_timer_init_t
- ll_capture_pin : _ll_timer_capture_channel_init
- ll_channel_a : _ll_pwm_coding_mode_init_t
- ll_channel_b : _ll_pwm_coding_mode_init_t
- ll_channel_c : _ll_pwm_coding_mode_init_t
- ll_coding_channel_select : _ll_pwm_coding_mode_init_t
- ll_comp0 : _ll_pwm_coding_channel_init_t
- ll_comp1 : _ll_pwm_coding_channel_init_t
- ll_data_width_valid : _ll_pwm_coding_mode_init_t
- ll_drive_polarity : _ll_pwm_coding_channel_init_t
- ll_edge_capture : _ll_timer_capture_channel_init
- ll_mode : _ll_pwm_init_t
- ll_period : _ll_pwm_coding_mode_init_t
- ll_prd_cycles : _ll_pwm_init_t
- ll_role : ble_gap_evt_connected_t , gap_conn_cmp_t
- ll_waiting_time : _ll_pwm_coding_mode_init_t
- ll_waiting_time_lvl : _ll_pwm_coding_channel_init_t
- llc_ext_llcp_proc_error_cb : ble_ext_llcp_cb_func_t
- llc_ext_llcp_req_handler_cb : ble_ext_llcp_cb_func_t
- llc_ext_llcp_req_proc_done_cb : ble_ext_llcp_cb_func_t
- lls_alert_level_handle : lls_c_handles_t
- lls_srvc_end_handle : lls_c_handles_t
- lls_srvc_start_handle : lls_c_handles_t
- lmp_subver : ble_gap_dev_version_ind_t
- lmp_subvers : ble_gap_peer_version_ind_t
- lmp_ver : ble_gap_dev_version_ind_t
- lmp_vers : ble_gap_peer_version_ind_t
- load_addr : dfu_boot_info_t
- loc_time_info : cts_adj_info_t , cts_c_evt_t , cts_evt_t , cts_init_t
- local_cid : ble_l2cap_evt_add_credits_cplt_t , ble_l2cap_evt_add_credits_ind_t , ble_l2cap_evt_conn_ind_t , ble_l2cap_evt_disconnect_t , ble_l2cap_lecb_add_credits_t , ble_l2cap_lecb_cfm_conn_t , ble_l2cap_lecb_conn_req_t , lecb_add_credits_ind_t , lecb_conn_ind_t , lecb_disconn_ind_t
- local_credits : ble_l2cap_evt_conn_ind_t , ble_l2cap_lecb_cfm_conn_t , ble_l2cap_lecb_conn_req_t , lecb_conn_ind_t
- local_irk : ble_gap_ral_dev_info_t
- local_tx_pwr_read : ble_gapc_evt_t
- lock : _adc_handle , _aon_wdt_handle , _bod_handle , _calendar_handle , _comp_handle , _dma_handle , _dual_timer_handle , _efuse_handle , _i2c_handle , _rng_handle , _rtc_handle_t , _spi_handle , _timer_handle , _uart_handle , _wdt_handle , _xqspi_handle_t , pwm_handle_t
- low_hyst : ble_gap_set_path_loss_report_param_t
- low_thr : ble_gap_set_path_loss_report_param_t