Public Attributes | List of all members
ias_c_handles_t Struct Reference
BLE Services » Immediate Alert Service Client (IAS_C) » Structures

Handles on the connected peer device needed to interact with it. More...

`#include <ias_c.h>`

## Public Attributes
uint16_t | ias_srvc_start_handle
uint16_t | ias_srvc_end_handle
uint16_t | ias_alert_level_handle

## Detailed Description

Handles on the connected peer device needed to interact with it.

Definition at line 100 of file ias_c.h.

## Member Data Documentation

## ◆ ias_alert_level_handle

uint16_t ias_c_handles_t::ias_alert_level_handle

IAS Alert Level characteristic Value handle which has been got from peer.

Definition at line 104 of file ias_c.h.

## ◆ ias_srvc_end_handle

uint16_t ias_c_handles_t::ias_srvc_end_handle

IAS Service end handle.

Definition at line 103 of file ias_c.h.

## ◆ ias_srvc_start_handle

uint16_t ias_c_handles_t::ias_srvc_start_handle

IAS Service start handle.

Definition at line 102 of file ias_c.h.

The documentation for this struct was generated from the following file:

- ias_c.h