Public Attributes | List of all members
ble_gap_evt_path_loss_threshold_report_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Path loss threshold reporting info event for BLE_GAPC_EVT_PATH_LOSS_THRESHOLD_REPORT. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | curr_path_loss
uint8_t | zone_entered

## Detailed Description

Path loss threshold reporting info event for BLE_GAPC_EVT_PATH_LOSS_THRESHOLD_REPORT.

Definition at line 956 of file ble_gapc.h.

## Member Data Documentation

## ◆ curr_path_loss

uint8_t ble_gap_evt_path_loss_threshold_report_t::curr_path_loss

Current path loss (dB).

Definition at line 958 of file ble_gapc.h.

## ◆ zone_entered

uint8_t ble_gap_evt_path_loss_threshold_report_t::zone_entered

Zone entered, see ble_gap_path_loss_zone_t.

Definition at line 959 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h