Macros
Get Flags Defines
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

Flags definitions which can be used with LL_SPI_ReadReg function. More...

## Macros
#define | LL_SPI_SR_DCOL SPI_STAT_DATA_COLN_ERR
#define | LL_SPI_SR_TXE SPI_STAT_TX_ERR
#define | LL_SPI_SR_RFF SPI_STAT_RX_FIFO_FULL
#define | LL_SPI_SR_RFNE SPI_STAT_RX_FIFO_NE
#define | LL_SPI_SR_TFE SPI_STAT_TX_FIFO_EMPTY
#define | LL_SPI_SR_TFNF SPI_STAT_TX_FIFO_NF
#define | LL_SPI_SR_BUSY SPI_STAT_SSI_BUSY

## Detailed Description

Flags definitions which can be used with LL_SPI_ReadReg function.

## Macro Definition Documentation

## ◆ LL_SPI_SR_BUSY

#define LL_SPI_SR_BUSY SPI_STAT_SSI_BUSY

Busy flag

Definition at line 160 of file gr533x_ll_spi.h.

## ◆ LL_SPI_SR_DCOL

#define LL_SPI_SR_DCOL SPI_STAT_DATA_COLN_ERR

Data collision error flag

Definition at line 154 of file gr533x_ll_spi.h.

## ◆ LL_SPI_SR_RFF

#define LL_SPI_SR_RFF SPI_STAT_RX_FIFO_FULL

Rx FIFO full flag

Definition at line 156 of file gr533x_ll_spi.h.

## ◆ LL_SPI_SR_RFNE

#define LL_SPI_SR_RFNE SPI_STAT_RX_FIFO_NE

Rx FIFO not empty flag

Definition at line 157 of file gr533x_ll_spi.h.

## ◆ LL_SPI_SR_TFE

#define LL_SPI_SR_TFE SPI_STAT_TX_FIFO_EMPTY

Tx FIFO empty flag

Definition at line 158 of file gr533x_ll_spi.h.

## ◆ LL_SPI_SR_TFNF

#define LL_SPI_SR_TFNF SPI_STAT_TX_FIFO_NF

Tx FIFO not full flag

Definition at line 159 of file gr533x_ll_spi.h.

## ◆ LL_SPI_SR_TXE

#define LL_SPI_SR_TXE SPI_STAT_TX_ERR

Transmission error flag

Definition at line 155 of file gr533x_ll_spi.h.