Functions
Initialization and de-initialization functions
Peripheral Driver » HAL Driver » CGC » Functions

Initialization and Configuration functions. More...

## Functions
void | hal_cgc_init (cgc_init_t *p_cgc_init)
| Initialize the CGC registers according to the specified parameters in the cgc_init_t. More...
void | hal_cgc_deinit (void)
| De-initialize the CGC registers to their default reset values. More...

## Detailed Description

Initialization and Configuration functions.

## Function Documentation

## ◆ hal_cgc_deinit()

void hal_cgc_deinit | ( | void |  | ) |

De-initialize the CGC registers to their default reset values.

## ◆ hal_cgc_init()

void hal_cgc_init | ( | cgc_init_t * | p_cgc_init | ) |

Initialize the CGC registers according to the specified parameters in the cgc_init_t.

Parameters

  [in] | p_cgc_init | Pointer to a cgc_init_t structure that contains the configuration information for the specified CGC registers.