Functions
Initialization and de-initialization functions
Peripheral Driver » HAL Driver » AON_GPIO » Functions

Initialization and Configuration functions. More...

## Functions
void | hal_aon_gpio_init (aon_gpio_init_t *p_aon_gpio_init)
| Initialize the AON_GPIOx peripheral according to the specified parameters in the aon_gpio_init_t. More...
void | hal_aon_gpio_deinit (uint32_t aon_gpio_pin)
| De-initialize the AON_GPIOx peripheral registers to their default reset values. More...

## Detailed Description

Initialization and Configuration functions.

## Function Documentation

## ◆ hal_aon_gpio_deinit()

void hal_aon_gpio_deinit | ( | uint32_t | aon_gpio_pin | ) |

De-initialize the AON_GPIOx peripheral registers to their default reset values.

Parameters

  [in] | aon_gpio_pin | Specifies the port bit to be written. This parameter can be a combination of the following values: AON_GPIO_PIN_0 AON_GPIO_PIN_1 AON_GPIO_PIN_2 AON_GPIO_PIN_3 AON_GPIO_PIN_4 AON_GPIO_PIN_5 AON_GPIO_PIN_ALL

## ◆ hal_aon_gpio_init()

void hal_aon_gpio_init | ( | aon_gpio_init_t * | p_aon_gpio_init | ) |

Initialize the AON_GPIOx peripheral according to the specified parameters in the aon_gpio_init_t.

Parameters

  [in] | p_aon_gpio_init | Pointer to an aon_gpio_init_t structure that contains the configuration information for the specified AON_GPIO peripheral port.