Modules | Macros
Defines
BLE Services » Running Speed and Cadence Service Client (RSCS_C)

## Modules
| Measurement Flag Bits
| Running Speed and Cadence Measurement Flags.
| Feature Bits
| Running Speed and Cadence Service feature bits.

## Macros
#define | RSCS_C_CONNECTION_MAX 10
#define | RSCS_C_PT_RSP_LEN_MAX (3 + RSCS_C_SENSOR_LOC_SUP_NB)
#define | RSCS_C_ERROR_PROC_IN_PROGRESS 0x80
#define | RSCS_C_ERROR_CCCD_INVALID 0x81

## Detailed Description

## Macro Definition Documentation

## ◆ RSCS_C_CONNECTION_MAX

#define RSCS_C_CONNECTION_MAX 10

Maximum number of HRS Client connections.

Definition at line 72 of file rscs_c.h.

## ◆ RSCS_C_ERROR_CCCD_INVALID

#define RSCS_C_ERROR_CCCD_INVALID 0x81

Error code: The Client Characteristic Configuration descriptor is not configured.

Definition at line 75 of file rscs_c.h.

## ◆ RSCS_C_ERROR_PROC_IN_PROGRESS

#define RSCS_C_ERROR_PROC_IN_PROGRESS 0x80

Error code: A previously triggered SC Control Point operation is still in progress.

Definition at line 74 of file rscs_c.h.

## ◆ RSCS_C_PT_RSP_LEN_MAX

#define RSCS_C_PT_RSP_LEN_MAX (3 + RSCS_C_SENSOR_LOC_SUP_NB)

Maximum length of SC Control Point response value.

Definition at line 73 of file rscs_c.h.