Public Attributes | List of all members
iso_start_gen_ann_t Struct Reference
BLE » Core Isochronous Channels | BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

The parameter for starting genneral announcement. More...

`#include <ble_iso.h>`

## Public Attributes
uint8_t | adv_idx
uint32_t | interval
uint16_t | data_len
uint8_t * | data

## Detailed Description

The parameter for starting genneral announcement.

Definition at line 217 of file ble_iso.h.

## Member Data Documentation

## ◆ adv_idx

uint8_t iso_start_gen_ann_t::adv_idx

Adv index.

Definition at line 219 of file ble_iso.h.

## ◆ data

uint8_t* iso_start_gen_ann_t::data

General audio announcement data.

Definition at line 222 of file ble_iso.h.

## ◆ data_len

uint16_t iso_start_gen_ann_t::data_len

General audio announcement data length.

Definition at line 221 of file ble_iso.h.

## ◆ interval

uint32_t iso_start_gen_ann_t::interval

Adv interval, (Range: 0x000020 to 0xFFFFFF), Time = N * 0.625.

Definition at line 220 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h