Public Attributes | List of all members
rscs_init_t Struct Reference
BLE Services » Running Speed and Cadence Service (RSCS) » Structures

Running Speed and Cadence Service init stucture. This contains all option and data needed for initialization of the service. More...

`#include <rscs.h>`

## Public Attributes
rscs_evt_handler_t | evt_handler
uint16_t | char_mask
rscs_sensor_loc_t | sensor_location
uint16_t | feature

## Detailed Description

Running Speed and Cadence Service init stucture. This contains all option and data needed for initialization of the service.

Definition at line 211 of file rscs.h.

## Member Data Documentation

## ◆ char_mask

uint16_t rscs_init_t::char_mask

Initial mask of supported characteristics, and configured with Characteristics Mask.

Definition at line 214 of file rscs.h.

## ◆ evt_handler

rscs_evt_handler_t rscs_init_t::evt_handler

Running Speed and Cadence Service event handler.

Definition at line 213 of file rscs.h.

## ◆ feature

uint16_t rscs_init_t::feature

Initial value for features.

Definition at line 216 of file rscs.h.

## ◆ sensor_location

rscs_sensor_loc_t rscs_init_t::sensor_location

Initial sensor location.

Definition at line 215 of file rscs.h.

The documentation for this struct was generated from the following file:

- rscs.h