Public Attributes | List of all members
_ll_rng_init Struct Reference
Peripheral Driver » LL Driver » RNG » Structures » RNG Exported Init structures

LL RNG Init Structure definition. More...

`#include <gr533x_ll_rng.h>`

## Public Attributes
uint32_t | seed
uint32_t | lfsr_mode
uint32_t | out_mode
uint32_t | post_mode
uint32_t | interrupt

## Detailed Description

LL RNG Init Structure definition.

Definition at line 76 of file gr533x_ll_rng.h.

## Member Data Documentation

## ◆ interrupt

uint32_t _ll_rng_init::interrupt

Specifies interrupt configuration for the RNG. This parameter can be a value of RNG hardware interrupt enable.

Definition at line 90 of file gr533x_ll_rng.h.

## ◆ lfsr_mode

uint32_t _ll_rng_init::lfsr_mode

Specifies the configuration mode for the LFSR. This parameter can be a value of LFSR configuration mode

Definition at line 81 of file gr533x_ll_rng.h.

## ◆ out_mode

uint32_t _ll_rng_init::out_mode

Specifies the Output mode for the RNG. This parameter can be a value of RNG Output mode

Definition at line 84 of file gr533x_ll_rng.h.

## ◆ post_mode

uint32_t _ll_rng_init::post_mode

Specifies post-process configuration for the RNG. This parameter can be a value of Post-process mode

Definition at line 87 of file gr533x_ll_rng.h.

## ◆ seed

uint32_t _ll_rng_init::seed

Specifies the seed source for the LFSR. This parameter can be a value of LFSR seed source

Definition at line 78 of file gr533x_ll_rng.h.

The documentation for this struct was generated from the following file:

- gr533x_ll_rng.h