Macros
Feature Bits
BLE Services » Running Speed and Cadence Service Client (RSCS_C) » Defines

Running Speed and Cadence Service feature bits. More...

## Macros
#define | RSCS_C_FEAT_INSTANT_STRIDE_LEN_BIT (0x01 << 0)
#define | RSCS_C_FEAT_TOTAL_DISTANCE_BIT (0x01 << 1)
#define | RSCS_C_FEAT_RUNNING_OR_WALKING_STATUS_BIT (0x01 << 2)
#define | RSCS_C_FEAT_CALIBRATION_PROCEDURE_BIT (0x01 << 3)
#define | RSCS_C_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 4)

## Detailed Description

Running Speed and Cadence Service feature bits.

## Macro Definition Documentation

## ◆ RSCS_C_FEAT_CALIBRATION_PROCEDURE_BIT

#define RSCS_C_FEAT_CALIBRATION_PROCEDURE_BIT (0x01 << 3)

Bit for Calibration Procedure Supported.

Definition at line 95 of file rscs_c.h.

## ◆ RSCS_C_FEAT_INSTANT_STRIDE_LEN_BIT

#define RSCS_C_FEAT_INSTANT_STRIDE_LEN_BIT (0x01 << 0)

Bit for Instantaneous Stride Length Measurement Supported.

Definition at line 92 of file rscs_c.h.

## ◆ RSCS_C_FEAT_MULTIPLE_SENSORS_BIT

#define RSCS_C_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 4)

Bit for Multiple Sensor Locations Supported.

Definition at line 96 of file rscs_c.h.

## ◆ RSCS_C_FEAT_RUNNING_OR_WALKING_STATUS_BIT

#define RSCS_C_FEAT_RUNNING_OR_WALKING_STATUS_BIT (0x01 << 2)

Bit for Running or Walking Status Supported.

Definition at line 94 of file rscs_c.h.

## ◆ RSCS_C_FEAT_TOTAL_DISTANCE_BIT

#define RSCS_C_FEAT_TOTAL_DISTANCE_BIT (0x01 << 1)

Bit for Total Distance Measurement Supported.

Definition at line 93 of file rscs_c.h.