Enumerations
HAL DUAL TIM state
Peripheral Driver » HAL Driver » DUAL TIMER » Enumerations

## Enumerations
enum | hal_dual_timer_state_t { HAL_DUAL_TIMER_STATE_RESET = 0x00, HAL_DUAL_TIMER_STATE_READY = 0x01, HAL_DUAL_TIMER_STATE_BUSY = 0x02, HAL_DUAL_TIMER_STATE_ERROR = 0x04 }
| HAL DUAL TIMER State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_dual_timer_state_t

enum hal_dual_timer_state_t

HAL DUAL TIMER State Enumerations definition.

Enumerator
HAL_DUAL_TIMER_STATE_RESET | Peripheral not yet initialized or disabled
HAL_DUAL_TIMER_STATE_READY | Peripheral Initialized and ready for use
HAL_DUAL_TIMER_STATE_BUSY | An internal process is ongoing
HAL_DUAL_TIMER_STATE_ERROR | Reception process is ongoing

Definition at line 75 of file gr533x_hal_dual_tim.h.