Modules
Throughput Service (THS)
BLE Services

Definitions and prototypes for the THS interface. More...

## Modules
| Defines
| Enumerations
| Structures
| Typedefs
| Functions

## Detailed Description

Definitions and prototypes for the THS interface.

The Throughput Service is a customized GATT-based service with Settings, Toggle, Tx and Rx characteristics. The developer uses the service to test throughput. The data is sent to the peer as Handle Value Notification, and the data received from the peer is transmitted with GATT Write Command.

The peer writes Toggle characteristic to command the application starting/stopping throughput. The application calls ths_data_send() to send data to the peer. The application handles THS_EVT_DATA_RECEIVED in ths_init_t::evt_handler() to get the data received from the peer. The application uses ths_settings_notify() to request the change of the parameters related with throughput, including CI, MTU, PDU and PHY.