Enumerations
Enumerations
BLE Services » Phone Alert Status Service Client (PASS_C)

## Enumerations
enum | pass_c_ringer_ctrl_pt_t { PASS_C_CTRL_PT_SILENT_MODE = 0x01, PASS_C_CTRL_PT_MUTE_ONCE, PASS_C_CTRL_PT_CANCEL_SLIENT_MODE }
| Phone Alert Status Service Client Ringer Control Point. More...
enum | pass_c_evt_type_t { PASS_C_EVT_INVALID, PASS_C_EVT_DISCOVERY_COMPLETE, PASS_C_EVT_DISCOVERY_FAIL, PASS_C_EVT_ALERT_STATUS_NTF_SET_SUCCESS, PASS_C_EVT_RINGER_SET_NTF_SET_SUCCESS, PASS_C_EVT_ALERT_STATUS_RECEIVE, PASS_C_EVT_RINGER_SET_RECEIVE, PASS_C_EVT_CTRL_POINT_SET_SUCCESS, PASS_C_EVT_WRITE_OP_ERR }
| Phone Alert Status Service Client event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ pass_c_evt_type_t

enum pass_c_evt_type_t

Phone Alert Status Service Client event type.

Enumerator
PASS_C_EVT_INVALID |
PASS_C_EVT_DISCOVERY_COMPLETE | PASS Client has found PASS service and its characteristics.
PASS_C_EVT_DISCOVERY_FAIL | PASS Client found PASS service failed because of invalid operation or no found at the peer.
PASS_C_EVT_ALERT_STATUS_NTF_SET_SUCCESS | PASS Client has set Notification of Alert Status characteristic.
PASS_C_EVT_RINGER_SET_NTF_SET_SUCCESS | PASS Client has set Notification of Ringer Setting characteristic.
PASS_C_EVT_ALERT_STATUS_RECEIVE | PASS Client has received Alert Status value (Read or Notification from peer).
PASS_C_EVT_RINGER_SET_RECEIVE | PASS Client has received Ringer Setting Value (Read or Notification from peer).
PASS_C_EVT_CTRL_POINT_SET_SUCCESS | PASS Client has writen Control Point completely.
PASS_C_EVT_WRITE_OP_ERR | Error occured when PASS Client writen to peer.

Definition at line 110 of file pass_c.h.

## ◆ pass_c_ringer_ctrl_pt_t

enum pass_c_ringer_ctrl_pt_t

Phone Alert Status Service Client Ringer Control Point.

Enumerator
PASS_C_CTRL_PT_SILENT_MODE | Silent Mode.
PASS_C_CTRL_PT_MUTE_ONCE | Mute Once.
PASS_C_CTRL_PT_CANCEL_SLIENT_MODE | Cancel Silent Mode.

Definition at line 102 of file pass_c.h.