Modules | Enumerations
Enumerations
Peripheral Driver » HAL Driver » PWM

## Modules
| HAL PWM active channel

## Enumerations
enum | hal_pwm_mode_t { PWM_FLICKER_MODE = 0x00, PWM_BREATH_MODE, PWM_CODING_MODE }
| HAL_PWM_MODE Enumerations definition. More...
enum | hal_pwm_state_t { HAL_PWM_STATE_RESET = 0x00, HAL_PWM_STATE_READY = 0x01, HAL_PWM_STATE_BUSY = 0x02, HAL_PWM_STATE_ERROR = 0x04 }
| HAL PWM State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_pwm_mode_t

enum hal_pwm_mode_t

HAL_PWM_MODE Enumerations definition.

Enumerator
PWM_FLICKER_MODE | Choose PWM Flicker Mode
PWM_BREATH_MODE | Choose PWM Breath Mode
PWM_CODING_MODE | Choose PWM Coding Mode

Definition at line 71 of file gr533x_hal_pwm.h.

## ◆ hal_pwm_state_t

enum hal_pwm_state_t

HAL PWM State Enumerations definition.

Enumerator
HAL_PWM_STATE_RESET | Peripheral is not initialized or disabled
HAL_PWM_STATE_READY | Peripheral is initialized and ready for use
HAL_PWM_STATE_BUSY | An internal process is ongoing
HAL_PWM_STATE_ERROR | Reception process is ongoing

Definition at line 81 of file gr533x_hal_pwm.h.