Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » PWM » Defines » PWM Exported Constants

## Macros
#define | LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG
| LL PWM None Coding Channel InitStrcut default configuartion. More...
#define | LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG
| LL PWM Coding Channel InitStrcut default configuartion. More...
#define | LL_PWM_NONE_CODING_DEFAULT_CONFIG
| LL PWM None Coding InitStrcut default configuartion. More...
#define | LL_PWM_CODING_DEFAULT_CONFIG
| LL PWM Coding InitStrcut default configuartion. More...
#define | LL_PWM_DEFAULT_CONFIG
| LL PWM InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG

#define LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG

Value:
{ \
.ll_comp0 = 0, \
.ll_comp1 = 640, \
.ll_drive_polarity = LL_PWM_DRIVEPOLARITY_POSITIVE, \
.ll_waiting_time_lvl = LL_PWM_WAITING_TIME_LVL_LOW, \
}

LL PWM Coding Channel InitStrcut default configuartion.

Definition at line 297 of file gr533x_ll_pwm.h.

## ◆ LL_PWM_CODING_DEFAULT_CONFIG

#define LL_PWM_CODING_DEFAULT_CONFIG

Value:
{ \
.ll_period = 640, \
.ll_waiting_time = 640, \
.ll_data_width_valid = 0x1F, \
.ll_coding_channel_select = LL_PWM_CODING_CHANNEL_ALL, \
.ll_channel_a = LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG, \
.ll_channel_b = LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG, \
.ll_channel_c = LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG, \
}

LL PWM Coding InitStrcut default configuartion.

Definition at line 323 of file gr533x_ll_pwm.h.

## ◆ LL_PWM_DEFAULT_CONFIG

#define LL_PWM_DEFAULT_CONFIG

Value:
{ \
.ll_mode = LL_PWM_FLICKER_MODE, \
.ll_prd_cycles = 0x0, \
.none_coding_mode_cfg = LL_PWM_NONE_CODING_DEFAULT_CONFIG, \
.coding_mode_cfg = LL_PWM_CODING_DEFAULT_CONFIG, \
}

LL PWM InitStrcut default configuartion.

Definition at line 337 of file gr533x_ll_pwm.h.

## ◆ LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG

#define LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG

Value:
{ \
.duty = 50, \
.drive_polarity = LL_PWM_DRIVEPOLARITY_POSITIVE, \
.flickerstop_lvl = LL_PWM_STOP_LVL_LOW, \
}

LL PWM None Coding Channel InitStrcut default configuartion.

Definition at line 287 of file gr533x_ll_pwm.h.

## ◆ LL_PWM_NONE_CODING_DEFAULT_CONFIG

#define LL_PWM_NONE_CODING_DEFAULT_CONFIG

Value:
{ \
.align = LL_PWM_EDGE_ALIGNED, \
.prescaler = 10 * LL_PWM_PRESCALER_UNIT, \
.bprescaler = 10 * LL_PWM_BREATH_PRESCALER_UNIT * 10 * LL_PWM_PRESCALER_UNIT, \
.hprescaler = 10 * LL_PWM_HOLD_PRESCALER_UNIT * 10 * LL_PWM_PRESCALER_UNIT, \
.breathstop_lvl = LL_PWM_STOP_LVL_LOW, \
.channel_a = LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG, \
.channel_b = LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG, \
.channel_c = LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG, \
}

LL PWM None Coding InitStrcut default configuartion.

Definition at line 308 of file gr533x_ll_pwm.h.

LL_PWM_PRESCALER_UNIT
#define LL_PWM_PRESCALER_UNIT
Definition: gr533x_ll_pwm.h:275
LL_PWM_DRIVEPOLARITY_POSITIVE
#define LL_PWM_DRIVEPOLARITY_POSITIVE
Definition: gr533x_ll_pwm.h:260
LL_PWM_EDGE_ALIGNED
#define LL_PWM_EDGE_ALIGNED
Definition: gr533x_ll_pwm.h:231
LL_PWM_HOLD_PRESCALER_UNIT
#define LL_PWM_HOLD_PRESCALER_UNIT
Definition: gr533x_ll_pwm.h:277
LL_PWM_WAITING_TIME_LVL_LOW
#define LL_PWM_WAITING_TIME_LVL_LOW
Definition: gr533x_ll_pwm.h:245
LL_PWM_BREATH_PRESCALER_UNIT
#define LL_PWM_BREATH_PRESCALER_UNIT
Definition: gr533x_ll_pwm.h:276
LL_PWM_STOP_LVL_LOW
#define LL_PWM_STOP_LVL_LOW
Definition: gr533x_ll_pwm.h:238
LL_PWM_NONE_CODING_DEFAULT_CONFIG
#define LL_PWM_NONE_CODING_DEFAULT_CONFIG
LL PWM None Coding InitStrcut default configuartion.
Definition: gr533x_ll_pwm.h:308
LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG
#define LL_PWM_CODING_CHANNEL_DEFAULT_CONFIG
LL PWM Coding Channel InitStrcut default configuartion.
Definition: gr533x_ll_pwm.h:297
LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG
#define LL_PWM_NONE_CODING_CHANNEL_DEFAULT_CONFIG
LL PWM None Coding Channel InitStrcut default configuartion.
Definition: gr533x_ll_pwm.h:287
LL_PWM_FLICKER_MODE
@ LL_PWM_FLICKER_MODE
Definition: gr533x_ll_pwm.h:72
LL_PWM_CODING_CHANNEL_ALL
#define LL_PWM_CODING_CHANNEL_ALL
Definition: gr533x_ll_pwm.h:252
LL_PWM_CODING_DEFAULT_CONFIG
#define LL_PWM_CODING_DEFAULT_CONFIG
LL PWM Coding InitStrcut default configuartion.
Definition: gr533x_ll_pwm.h:323