Public Attributes | List of all members
pwm_coding_channel_init_t Struct Reference
Peripheral Driver » HAL Driver » PWM » Structures » PWM Configuration

PWM Coding Channel init Structure definition. More...

`#include <gr533x_hal_pwm.h>`

## Public Attributes
uint32_t | comp0
uint32_t | comp1
uint8_t | drive_polarity
uint8_t | waiting_time_lvl

## Detailed Description

PWM Coding Channel init Structure definition.

Definition at line 147 of file gr533x_hal_pwm.h.

## Member Data Documentation

## ◆ comp0

uint32_t pwm_coding_channel_init_t::comp0

Specifies current channel first compare value This parameter must be a number ranges between Min_Data=0 and Max_Data=period.

Definition at line 149 of file gr533x_hal_pwm.h.

## ◆ comp1

uint32_t pwm_coding_channel_init_t::comp1

Specifies current channel second compare value This parameter must be a number ranges between Min_Data=0 and Max_Data=period.

Definition at line 152 of file gr533x_hal_pwm.h.

## ◆ drive_polarity

uint8_t pwm_coding_channel_init_t::drive_polarity

Specifies the drive polarity in PWM output mode. This parameter can be a value of PWM Drive Polarity.

Definition at line 155 of file gr533x_hal_pwm.h.

## ◆ waiting_time_lvl

uint8_t pwm_coding_channel_init_t::waiting_time_lvl

Specifies the waiting time level in coding mode. This parameter can be a value of PWM waiting time io level.

Definition at line 158 of file gr533x_hal_pwm.h.

The documentation for this struct was generated from the following file:

- gr533x_hal_pwm.h