Macros
State from Software CS Assert
Peripheral Driver » HAL Driver » SPI » CS Signal Description » Defines

## Macros
#define | CS_STA_STATE_POLL_TX 0x01
| State from Software CS Assert. More...
#define | CS_STA_STATE_POLL_RX 0x02
#define | CS_STA_STATE_POLL_TX_RX 0x03
#define | CS_STA_STATE_POLL_EEPREAD 0x04
#define | CS_STA_STATE_IT_TX 0x05
#define | CS_STA_STATE_IT_RX 0x06
#define | CS_STA_STATE_IT_TX_RX 0x07
#define | CS_STA_STATE_IT_EEPREAD 0x08
#define | CS_STA_STATE_DMA_TX 0x09
#define | CS_STA_STATE_DMA_RX 0x0A
#define | CS_STA_STATE_DMA_TX_RX 0x0B
#define | CS_STA_STATE_DMA_EEPREAD 0x0C
#define | CS_STA_STATE_DMA_LLP_TX 0x0D
#define | CS_STA_STATE_DMA_SCATTER_RX 0x0E

## Detailed Description

## Macro Definition Documentation

## ◆ CS_STA_STATE_DMA_EEPREAD

#define CS_STA_STATE_DMA_EEPREAD 0x0C

CS ASSERT when EEPREAD Starts by DMA

Definition at line 158 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_DMA_LLP_TX

#define CS_STA_STATE_DMA_LLP_TX 0x0D

CS ASSERT when Transferring Starts by DMA LLP

Definition at line 159 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_DMA_RX

#define CS_STA_STATE_DMA_RX 0x0A

CS ASSERT when Receiving Starts by DMA

Definition at line 156 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_DMA_SCATTER_RX

#define CS_STA_STATE_DMA_SCATTER_RX 0x0E

CS ASSERT when Receiving Starts by DMA Scatter

Definition at line 160 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_DMA_TX

#define CS_STA_STATE_DMA_TX 0x09

CS ASSERT when Transferring Starts by DMA

Definition at line 155 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_DMA_TX_RX

#define CS_STA_STATE_DMA_TX_RX 0x0B

CS ASSERT when DUPLEX Starts by DMA

Definition at line 157 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_IT_EEPREAD

#define CS_STA_STATE_IT_EEPREAD 0x08

CS ASSERT when EEPREAD Starts by Interrupt

Definition at line 154 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_IT_RX

#define CS_STA_STATE_IT_RX 0x06

CS ASSERT when Receiving Starts by Interrupt

Definition at line 152 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_IT_TX

#define CS_STA_STATE_IT_TX 0x05

CS ASSERT when Transferring Starts by Interrupt

Definition at line 151 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_IT_TX_RX

#define CS_STA_STATE_IT_TX_RX 0x07

CS ASSERT when DUPLEX Starts by Interrupt

Definition at line 153 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_POLL_EEPREAD

#define CS_STA_STATE_POLL_EEPREAD 0x04

CS ASSERT when EEPREAD Starts by Polling

Definition at line 150 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_POLL_RX

#define CS_STA_STATE_POLL_RX 0x02

CS ASSERT when Receiving Starts by Polling

Definition at line 148 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_POLL_TX

#define CS_STA_STATE_POLL_TX 0x01

State from Software CS Assert.

CS ASSERT when Transferring Starts by Polling

Definition at line 147 of file gr533x_hal_spi.h.

## ◆ CS_STA_STATE_POLL_TX_RX

#define CS_STA_STATE_POLL_TX_RX 0x03

CS ASSERT when DUPLEX Starts by Polling

Definition at line 149 of file gr533x_hal_spi.h.